    //! This file provides the system interface functions for Linux matching those
    //! that are provided by libc, whether or not libc is linked. The following
    //! abstractions are made:
    //! * Work around kernel bugs and limitations. For example, see sendmmsg.
    //! * Implement all the syscalls in the same way that libc functions will
    //!   provide `rename` when only the `renameat` syscall exists.
    //! * Does not support POSIX thread cancellation.
    const std = @import("../std.zig");
    const builtin = @import("builtin");
    const assert = std.debug.assert;
    const maxInt = std.math.maxInt;
    const elf = std.elf;
    const vdso = @import("linux/vdso.zig");
    const dl = @import("../dynamic_library.zig");
    const native_arch = builtin.cpu.arch;
    const native_endian = native_arch.endian();
    const is_mips = native_arch.isMIPS();
    const is_ppc = native_arch.isPPC();
    const is_ppc64 = native_arch.isPPC64();
    const is_sparc = native_arch.isSPARC();
    const iovec = std.os.iovec;
    const iovec_const = std.os.iovec_const;

    test {
        if (builtin.os.tag == .linux) {
            _ = @import("linux/test.zig");
        }
    }

    const syscall_bits = switch (native_arch) {
        .thumb => @import("linux/thumb.zig"),
        else => arch_bits,
    };

    const arch_bits = switch (native_arch) {
        .i386 => @import("linux/i386.zig"),
        .x86_64 => @import("linux/x86_64.zig"),
        .aarch64 => @import("linux/arm64.zig"),
        .arm, .thumb => @import("linux/arm-eabi.zig"),
        .riscv64 => @import("linux/riscv64.zig"),
        .sparc64 => @import("linux/sparc64.zig"),
        .mips, .mipsel => @import("linux/mips.zig"),
        .powerpc => @import("linux/powerpc.zig"),
        .powerpc64, .powerpc64le => @import("linux/powerpc64.zig"),
        else => struct {},
    };
    pub const syscall0 = syscall_bits.syscall0;
    pub const syscall1 = syscall_bits.syscall1;
    pub const syscall2 = syscall_bits.syscall2;
    pub const syscall3 = syscall_bits.syscall3;
    pub const syscall4 = syscall_bits.syscall4;
    pub const syscall5 = syscall_bits.syscall5;
    pub const syscall6 = syscall_bits.syscall6;
    pub const syscall7 = syscall_bits.syscall7;
    pub const restore = syscall_bits.restore;
    pub const restore_rt = syscall_bits.restore_rt;
    pub const socketcall = syscall_bits.socketcall;
    pub const syscall_pipe = syscall_bits.syscall_pipe;
    pub const syscall_fork = syscall_bits.syscall_fork;

    pub const ARCH = arch_bits.ARCH;
    pub const Elf_Symndx = arch_bits.Elf_Symndx;
    pub const F = arch_bits.F;
    pub const Flock = arch_bits.Flock;
    pub const HWCAP = arch_bits.HWCAP;
    pub const LOCK = arch_bits.LOCK;
    pub const MMAP2_UNIT = arch_bits.MMAP2_UNIT;
    pub const REG = arch_bits.REG;
    pub const SC = arch_bits.SC;
    pub const Stat = arch_bits.Stat;
    pub const VDSO = arch_bits.VDSO;
    pub const blkcnt_t = arch_bits.blkcnt_t;
    pub const blksize_t = arch_bits.blksize_t;
    pub const clone = arch_bits.clone;
    pub const dev_t = arch_bits.dev_t;
    pub const ino_t = arch_bits.ino_t;
    pub const mcontext_t = arch_bits.mcontext_t;
    pub const mode_t = arch_bits.mode_t;
    pub const msghdr = arch_bits.msghdr;
    pub const msghdr_const = arch_bits.msghdr_const;
    pub const nlink_t = arch_bits.nlink_t;
    pub const off_t = arch_bits.off_t;
    pub const time_t = arch_bits.time_t;
    pub const timeval = arch_bits.timeval;
    pub const timezone = arch_bits.timezone;
    pub const ucontext_t = arch_bits.ucontext_t;
    pub const user_desc = arch_bits.user_desc;

    pub const tls = @import("linux/tls.zig");
    pub const pie = @import("linux/start_pie.zig");
    pub const BPF = @import("linux/bpf.zig");
    pub const IOCTL = @import("linux/ioctl.zig");
    pub const SECCOMP = @import("linux/seccomp.zig");

    pub const syscalls = @import("linux/syscalls.zig");
    pub const SYS = switch (@import("builtin").cpu.arch) {
        .i386 => syscalls.X86,
        .x86_64 => syscalls.X64,
        .aarch64 => syscalls.Arm64,
        .arm, .thumb => syscalls.Arm,
        .riscv64 => syscalls.RiscV64,
        .sparc64 => syscalls.Sparc64,
        .mips, .mipsel => syscalls.Mips,
        .powerpc => syscalls.PowerPC,
        .powerpc64, .powerpc64le => syscalls.PowerPC64,
        else => @compileError("The Zig Standard Library is missing syscall definitions for the target CPU architecture"),
    };

    pub const MAP = struct {
        pub usingnamespace arch_bits.MAP;

        /// Share changes
        pub const SHARED = 0x01;
        /// Changes are private
        pub const PRIVATE = 0x02;
        /// share + validate extension flags
        pub const SHARED_VALIDATE = 0x03;
        /// Mask for type of mapping
        pub const TYPE = 0x0f;
        /// Interpret addr exactly
        pub const FIXED = 0x10;
        /// don't use a file
        pub const ANONYMOUS = if (is_mips) 0x800 else 0x20;
        // MAP_ 0x0100 - 0x4000 flags are per architecture

        /// populate (prefault) pagetables
        pub const POPULATE = if (is_mips) 0x10000 else 0x8000;
        /// do not block on IO
        pub const NONBLOCK = if (is_mips) 0x20000 else 0x10000;
        /// give out an address that is best suited for process/thread stacks
        pub const STACK = if (is_mips) 0x40000 else 0x20000;
        /// create a huge page mapping
        pub const HUGETLB = if (is_mips) 0x80000 else 0x40000;
        /// perform synchronous page faults for the mapping
        pub const SYNC = 0x80000;
        /// MAP_FIXED which doesn't unmap underlying mapping
        pub const FIXED_NOREPLACE = 0x100000;
        /// For anonymous mmap, memory could be uninitialized
        pub const UNINITIALIZED = 0x4000000;
    };

    pub const O = struct {
        pub usingnamespace arch_bits.O;

        pub const RDONLY = 0o0;
        pub const WRONLY = 0o1;
        pub const RDWR = 0o2;
    };

    pub usingnamespace @import("linux/io_uring.zig");

    /// Set by startup code, used by `getauxval`.
    pub var elf_aux_maybe: ?[*]std.elf.Auxv = null;

    /// See `std.elf` for the constants.
    pub fn getauxval(index: usize) usize {
        const auxv = elf_aux_maybe orelse return 0;
        var i: usize = 0;
        while (auxv[i].a_type != std.elf.AT_NULL) : (i += 1) {
            if (auxv[i].a_type == index)
                return auxv[i].a_un.a_val;
        }
        return 0;
    }

    // Some architectures (and some syscalls) require 64bit parameters to be passed

    // in a even-aligned register pair.

    const require_aligned_register_pair =
        builtin.cpu.arch.isPPC() or
        builtin.cpu.arch.isMIPS() or
        builtin.cpu.arch.isARM() or
        builtin.cpu.arch.isThumb();

    // Split a 64bit value into a {LSB,MSB} pair.

    // The LE/BE variants specify the endianness to assume.

    fn splitValueLE64(val: i64) [2]u32 {
        const u = @bitCast(u64, val);
        return [2]u32{
            @truncate(u32, u),
            @truncate(u32, u >> 32),
        };
    }
    fn splitValueBE64(val: i64) [2]u32 {
        const u = @bitCast(u64, val);
        return [2]u32{
            @truncate(u32, u >> 32),
            @truncate(u32, u),
        };
    }
    fn splitValue64(val: i64) [2]u32 {
        const u = @bitCast(u64, val);
        switch (native_endian) {
            .Little => return [2]u32{
                @truncate(u32, u),
                @truncate(u32, u >> 32),
            },
            .Big => return [2]u32{
                @truncate(u32, u >> 32),
                @truncate(u32, u),
            },
        }
    }

    /// Get the errno from a syscall return value, or 0 for no error.
    pub fn getErrno(r: usize) E {
        const signed_r = @bitCast(isize, r);
        const int = if (signed_r > -4096 and signed_r < 0) -signed_r else 0;
        return @intToEnum(E, int);
    }

    pub fn dup(old: i32) usize {
        return syscall1(.dup, @bitCast(usize, @as(isize, old)));
    }

    pub fn dup2(old: i32, new: i32) usize {
        if (@hasField(SYS, "dup2")) {
            return syscall2(.dup2, @bitCast(usize, @as(isize, old)), @bitCast(usize, @as(isize, new)));
        } else {
            if (old == new) {
                if (std.debug.runtime_safety) {
                    const rc = syscall2(.fcntl, @bitCast(usize, @as(isize, old)), F.GETFD);
                    if (@bitCast(isize, rc) < 0) return rc;
                }
                return @intCast(usize, old);
            } else {
                return syscall3(.dup3, @bitCast(usize, @as(isize, old)), @bitCast(usize, @as(isize, new)), 0);
            }
        }
    }

    pub fn dup3(old: i32, new: i32, flags: u32) usize {
        return syscall3(.dup3, @bitCast(usize, @as(isize, old)), @bitCast(usize, @as(isize, new)), flags);
    }

    pub fn chdir(path: [*:0]const u8) usize {
        return syscall1(.chdir, @ptrToInt(path));
    }

    pub fn fchdir(fd: fd_t) usize {
        return syscall1(.fchdir, @bitCast(usize, @as(isize, fd)));
    }

    pub fn chroot(path: [*:0]const u8) usize {
        return syscall1(.chroot, @ptrToInt(path));
    }

    pub fn execve(path: [*:0]const u8, argv: [*:null]const ?[*:0]const u8, envp: [*:null]const ?[*:0]const u8) usize {
        return syscall3(.execve, @ptrToInt(path), @ptrToInt(argv), @ptrToInt(envp));
    }

    pub fn fork() usize {
        if (comptime native_arch.isSPARC()) {
            return syscall_fork();
        } else if (@hasField(SYS, "fork")) {
            return syscall0(.fork);
        } else {
            return syscall2(.clone, SIG.CHLD, 0);
        }
    }

    /// This must be inline, and inline call the syscall function, because if the
    /// child does a return it will clobber the parent's stack.
    /// It is advised to avoid this function and use clone instead, because
    /// the compiler is not aware of how vfork affects control flow and you may
    /// see different results in optimized builds.
    pub inline fn vfork() usize {
        return @call(.{ .modifier = .always_inline }, syscall0, .{.vfork});
    }

    pub fn futimens(fd: i32, times: *const [2]timespec) usize {
        return utimensat(fd, null, times, 0);
    }

    pub fn utimensat(dirfd: i32, path: ?[*:0]const u8, times: *const [2]timespec, flags: u32) usize {
        return syscall4(.utimensat, @bitCast(usize, @as(isize, dirfd)), @ptrToInt(path), @ptrToInt(times), flags);
    }

    pub fn fallocate(fd: i32, mode: i32, offset: i64, length: i64) usize {
        if (usize_bits < 64) {
            const offset_halves = splitValue64(offset);
            const length_halves = splitValue64(length);
            return syscall6(
                .fallocate,
                @bitCast(usize, @as(isize, fd)),
                @bitCast(usize, @as(isize, mode)),
                offset_halves[0],
                offset_halves[1],
                length_halves[0],
                length_halves[1],
            );
        } else {
            return syscall4(
                .fallocate,
                @bitCast(usize, @as(isize, fd)),
                @bitCast(usize, @as(isize, mode)),
                @bitCast(u64, offset),
                @bitCast(u64, length),
            );
        }
    }

    pub fn futex_wait(uaddr: *const i32, futex_op: u32, val: i32, timeout: ?*const timespec) usize {
        return syscall4(.futex, @ptrToInt(uaddr), futex_op, @bitCast(u32, val), @ptrToInt(timeout));
    }

    pub fn futex_wake(uaddr: *const i32, futex_op: u32, val: i32) usize {
        return syscall3(.futex, @ptrToInt(uaddr), futex_op, @bitCast(u32, val));
    }

    pub fn getcwd(buf: [*]u8, size: usize) usize {
        return syscall2(.getcwd, @ptrToInt(buf), size);
    }

    pub fn getdents(fd: i32, dirp: [*]u8, len: usize) usize {
        return syscall3(
            .getdents,
            @bitCast(usize, @as(isize, fd)),
            @ptrToInt(dirp),
            std.math.min(len, maxInt(c_int)),
        );
    }

    pub fn getdents64(fd: i32, dirp: [*]u8, len: usize) usize {
        return syscall3(
            .getdents64,
            @bitCast(usize, @as(isize, fd)),
            @ptrToInt(dirp),
            std.math.min(len, maxInt(c_int)),
        );
    }

    pub fn inotify_init1(flags: u32) usize {
        return syscall1(.inotify_init1, flags);
    }

    pub fn inotify_add_watch(fd: i32, pathname: [*:0]const u8, mask: u32) usize {
        return syscall3(.inotify_add_watch, @bitCast(usize, @as(isize, fd)), @ptrToInt(pathname), mask);
    }

    pub fn inotify_rm_watch(fd: i32, wd: i32) usize {
        return syscall2(.inotify_rm_watch, @bitCast(usize, @as(isize, fd)), @bitCast(usize, @as(isize, wd)));
    }

    pub fn readlink(noalias path: [*:0]const u8, noalias buf_ptr: [*]u8, buf_len: usize) usize {
        if (@hasField(SYS, "readlink")) {
            return syscall3(.readlink, @ptrToInt(path), @ptrToInt(buf_ptr), buf_len);
        } else {
            return syscall4(.readlinkat, @bitCast(usize, @as(isize, AT.FDCWD)), @ptrToInt(path), @ptrToInt(buf_ptr), buf_len);
        }
    }

    pub fn readlinkat(dirfd: i32, noalias path: [*:0]const u8, noalias buf_ptr: [*]u8, buf_len: usize) usize {
        return syscall4(.readlinkat, @bitCast(usize, @as(isize, dirfd)), @ptrToInt(path), @ptrToInt(buf_ptr), buf_len);
    }

    pub fn mkdir(path: [*:0]const u8, mode: u32) usize {
        if (@hasField(SYS, "mkdir")) {
            return syscall2(.mkdir, @ptrToInt(path), mode);
        } else {
            return syscall3(.mkdirat, @bitCast(usize, @as(isize, AT.FDCWD)), @ptrToInt(path), mode);
        }
    }

    pub fn mkdirat(dirfd: i32, path: [*:0]const u8, mode: u32) usize {
        return syscall3(.mkdirat, @bitCast(usize, @as(isize, dirfd)), @ptrToInt(path), mode);
    }

    pub fn mknod(path: [*:0]const u8, mode: u32, dev: u32) usize {
        if (@hasField(SYS, "mknod")) {
            return syscall3(.mknod, @ptrToInt(path), mode, dev);
        } else {
            return mknodat(AT.FDCWD, path, mode, dev);
        }
    }

    pub fn mknodat(dirfd: i32, path: [*:0]const u8, mode: u32, dev: u32) usize {
        return syscall4(.mknodat, @bitCast(usize, @as(isize, dirfd)), @ptrToInt(path), mode, dev);
    }

    pub fn mount(special: [*:0]const u8, dir: [*:0]const u8, fstype: ?[*:0]const u8, flags: u32, data: usize) usize {
        return syscall5(.mount, @ptrToInt(special), @ptrToInt(dir), @ptrToInt(fstype), flags, data);
    }

    pub fn umount(special: [*:0]const u8) usize {
        return syscall2(.umount2, @ptrToInt(special), 0);
    }

    pub fn umount2(special: [*:0]const u8, flags: u32) usize {
        return syscall2(.umount2, @ptrToInt(special), flags);
    }

    pub fn mmap(address: ?[*]u8, length: usize, prot: usize, flags: u32, fd: i32, offset: i64) usize {
        if (@hasField(SYS, "mmap2")) {
            // Make sure the offset is also specified in multiples of page size

            if ((offset & (MMAP2_UNIT - 1)) != 0)
                return @bitCast(usize, -@as(isize, @enumToInt(E.INVAL)));

            return syscall6(
                .mmap2,
                @ptrToInt(address),
                length,
                prot,
                flags,
                @bitCast(usize, @as(isize, fd)),
                @truncate(usize, @bitCast(u64, offset) / MMAP2_UNIT),
            );
        } else {
            return syscall6(
                .mmap,
                @ptrToInt(address),
                length,
                prot,
                flags,
                @bitCast(usize, @as(isize, fd)),
                @bitCast(u64, offset),
            );
        }
    }

    pub fn mprotect(address: [*]const u8, length: usize, protection: usize) usize {
        return syscall3(.mprotect, @ptrToInt(address), length, protection);
    }

    pub const MSF = struct {
        pub const ASYNC = 1;
        pub const INVALIDATE = 2;
        pub const SYNC = 4;
    };

    pub fn msync(address: [*]const u8, length: usize, flags: i32) usize {
        return syscall3(.msync, @ptrToInt(address), length, @bitCast(u32, flags));
    }

    pub fn munmap(address: [*]const u8, length: usize) usize {
        return syscall2(.munmap, @ptrToInt(address), length);
    }

    pub fn poll(fds: [*]pollfd, n: nfds_t, timeout: i32) usize {
        if (@hasField(SYS, "poll")) {
            return syscall3(.poll, @ptrToInt(fds), n, @bitCast(u32, timeout));
        } else {
            return syscall5(
                .ppoll,
                @ptrToInt(fds),
                n,
                @ptrToInt(if (timeout >= 0)
                    &timespec{
                        .tv_sec = @divTrunc(timeout, 1000),
                        .tv_nsec = @rem(timeout, 1000) * 1000000,
                    }
                else
                    null),
                0,
                NSIG / 8,
            );
        }
    }

    pub fn ppoll(fds: [*]pollfd, n: nfds_t, timeout: ?*timespec, sigmask: ?*const sigset_t) usize {
        return syscall5(.ppoll, @ptrToInt(fds), n, @ptrToInt(timeout), @ptrToInt(sigmask), NSIG / 8);
    }

    pub fn read(fd: i32, buf: [*]u8, count: usize) usize {
        return syscall3(.read, @bitCast(usize, @as(isize, fd)), @ptrToInt(buf), count);
    }

    pub fn preadv(fd: i32, iov: [*]const iovec, count: usize, offset: i64) usize {
        const offset_u = @bitCast(u64, offset);
        return syscall5(
            .preadv,
            @bitCast(usize, @as(isize, fd)),
            @ptrToInt(iov),
            count,
            // Kernel expects the offset is splitted into largest natural word-size.

            // See following link for detail:

            // https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=601cc11d054ae4b5e9b5babec3d8e4667a2cb9b5

            @truncate(usize, offset_u),
            if (usize_bits < 64) @truncate(usize, offset_u >> 32) else 0,
        );
    }

    pub fn preadv2(fd: i32, iov: [*]const iovec, count: usize, offset: i64, flags: kernel_rwf) usize {
        const offset_u = @bitCast(u64, offset);
        return syscall6(
            .preadv2,
            @bitCast(usize, @as(isize, fd)),
            @ptrToInt(iov),
            count,
            // See comments in preadv

            @truncate(usize, offset_u),
            if (usize_bits < 64) @truncate(usize, offset_u >> 32) else 0,
            flags,
        );
    }

    pub fn readv(fd: i32, iov: [*]const iovec, count: usize) usize {
        return syscall3(.readv, @bitCast(usize, @as(isize, fd)), @ptrToInt(iov), count);
    }

    pub fn writev(fd: i32, iov: [*]const iovec_const, count: usize) usize {
        return syscall3(.writev, @bitCast(usize, @as(isize, fd)), @ptrToInt(iov), count);
    }

    pub fn pwritev(fd: i32, iov: [*]const iovec_const, count: usize, offset: i64) usize {
        const offset_u = @bitCast(u64, offset);
        return syscall5(
            .pwritev,
            @bitCast(usize, @as(isize, fd)),
            @ptrToInt(iov),
            count,
            // See comments in preadv

            @truncate(usize, offset_u),
            if (usize_bits < 64) @truncate(usize, offset_u >> 32) else 0,
        );
    }

    pub fn pwritev2(fd: i32, iov: [*]const iovec_const, count: usize, offset: i64, flags: kernel_rwf) usize {
        const offset_u = @bitCast(u64, offset);
        return syscall6(
            .pwritev2,
            @bitCast(usize, @as(isize, fd)),
            @ptrToInt(iov),
            count,
            // See comments in preadv

            @truncate(usize, offset_u),
            if (usize_bits < 64) @truncate(usize, offset_u >> 32) else 0,
            flags,
        );
    }

    pub fn rmdir(path: [*:0]const u8) usize {
        if (@hasField(SYS, "rmdir")) {
            return syscall1(.rmdir, @ptrToInt(path));
        } else {
            return syscall3(.unlinkat, @bitCast(usize, @as(isize, AT.FDCWD)), @ptrToInt(path), AT.REMOVEDIR);
        }
    }

    pub fn symlink(existing: [*:0]const u8, new: [*:0]const u8) usize {
        if (@hasField(SYS, "symlink")) {
            return syscall2(.symlink, @ptrToInt(existing), @ptrToInt(new));
        } else {
            return syscall3(.symlinkat, @ptrToInt(existing), @bitCast(usize, @as(isize, AT.FDCWD)), @ptrToInt(new));
        }
    }

    pub fn symlinkat(existing: [*:0]const u8, newfd: i32, newpath: [*:0]const u8) usize {
        return syscall3(.symlinkat, @ptrToInt(existing), @bitCast(usize, @as(isize, newfd)), @ptrToInt(newpath));
    }

    pub fn pread(fd: i32, buf: [*]u8, count: usize, offset: i64) usize {
        if (@hasField(SYS, "pread64") and usize_bits < 64) {
            const offset_halves = splitValue64(offset);
            if (require_aligned_register_pair) {
                return syscall6(
                    .pread64,
                    @bitCast(usize, @as(isize, fd)),
                    @ptrToInt(buf),
                    count,
                    0,
                    offset_halves[0],
                    offset_halves[1],
                );
            } else {
                return syscall5(
                    .pread64,
                    @bitCast(usize, @as(isize, fd)),
                    @ptrToInt(buf),
                    count,
                    offset_halves[0],
                    offset_halves[1],
                );
            }
        } else {
            // Some architectures (eg. 64bit SPARC) pread is called pread64.

            const syscall_number = if (!@hasField(SYS, "pread") and @hasField(SYS, "pread64"))
                .pread64
            else
                .pread;
            return syscall4(
                syscall_number,
                @bitCast(usize, @as(isize, fd)),
                @ptrToInt(buf),
                count,
                @bitCast(u64, offset),
            );
        }
    }

    pub fn access(path: [*:0]const u8, mode: u32) usize {
        if (@hasField(SYS, "access")) {
            return syscall2(.access, @ptrToInt(path), mode);
        } else {
            return syscall4(.faccessat, @bitCast(usize, @as(isize, AT.FDCWD)), @ptrToInt(path), mode, 0);
        }
    }

    pub fn faccessat(dirfd: i32, path: [*:0]const u8, mode: u32, flags: u32) usize {
        return syscall4(.faccessat, @bitCast(usize, @as(isize, dirfd)), @ptrToInt(path), mode, flags);
    }

    pub fn pipe(fd: *[2]i32) usize {
        if (comptime (native_arch.isMIPS() or native_arch.isSPARC())) {
            return syscall_pipe(fd);
        } else if (@hasField(SYS, "pipe")) {
            return syscall1(.pipe, @ptrToInt(fd));
        } else {
            return syscall2(.pipe2, @ptrToInt(fd), 0);
        }
    }

    pub fn pipe2(fd: *[2]i32, flags: u32) usize {
        return syscall2(.pipe2, @ptrToInt(fd), flags);
    }

    pub fn write(fd: i32, buf: [*]const u8, count: usize) usize {
        return syscall3(.write, @bitCast(usize, @as(isize, fd)), @ptrToInt(buf), count);
    }

    pub fn ftruncate(fd: i32, length: i64) usize {
        if (@hasField(SYS, "ftruncate64") and usize_bits < 64) {
            const length_halves = splitValue64(length);
            if (require_aligned_register_pair) {
                return syscall4(
                    .ftruncate64,
                    @bitCast(usize, @as(isize, fd)),
                    0,
                    length_halves[0],
                    length_halves[1],
                );
            } else {
                return syscall3(
                    .ftruncate64,
                    @bitCast(usize, @as(isize, fd)),
                    length_halves[0],
                    length_halves[1],
                );
            }
        } else {
            return syscall2(
                .ftruncate,
                @bitCast(usize, @as(isize, fd)),
                @bitCast(usize, length),
            );
        }
    }

    pub fn pwrite(fd: i32, buf: [*]const u8, count: usize, offset: i64) usize {
        if (@hasField(SYS, "pwrite64") and usize_bits < 64) {
            const offset_halves = splitValue64(offset);

            if (require_aligned_register_pair) {
                return syscall6(
                    .pwrite64,
                    @bitCast(usize, @as(isize, fd)),
                    @ptrToInt(buf),
                    count,
                    0,
                    offset_halves[0],
                    offset_halves[1],
                );
            } else {
                return syscall5(
                    .pwrite64,
                    @bitCast(usize, @as(isize, fd)),
                    @ptrToInt(buf),
                    count,
                    offset_halves[0],
                    offset_halves[1],
                );
            }
        } else {
            // Some architectures (eg. 64bit SPARC) pwrite is called pwrite64.

            const syscall_number = if (!@hasField(SYS, "pwrite") and @hasField(SYS, "pwrite64"))
                .pwrite64
            else
                .pwrite;
            return syscall4(
                syscall_number,
                @bitCast(usize, @as(isize, fd)),
                @ptrToInt(buf),
                count,
                @bitCast(u64, offset),
            );
        }
    }

    pub fn rename(old: [*:0]const u8, new: [*:0]const u8) usize {
        if (@hasField(SYS, "rename")) {
            return syscall2(.rename, @ptrToInt(old), @ptrToInt(new));
        } else if (@hasField(SYS, "renameat")) {
            return syscall4(.renameat, @bitCast(usize, @as(isize, AT.FDCWD)), @ptrToInt(old), @bitCast(usize, @as(isize, AT.FDCWD)), @ptrToInt(new));
        } else {
            return syscall5(.renameat2, @bitCast(usize, @as(isize, AT.FDCWD)), @ptrToInt(old), @bitCast(usize, @as(isize, AT.FDCWD)), @ptrToInt(new), 0);
        }
    }

    pub fn renameat(oldfd: i32, oldpath: [*]const u8, newfd: i32, newpath: [*]const u8) usize {
        if (@hasField(SYS, "renameat")) {
            return syscall4(
                .renameat,
                @bitCast(usize, @as(isize, oldfd)),
                @ptrToInt(oldpath),
                @bitCast(usize, @as(isize, newfd)),
                @ptrToInt(newpath),
            );
        } else {
            return syscall5(
                .renameat2,
                @bitCast(usize, @as(isize, oldfd)),
                @ptrToInt(oldpath),
                @bitCast(usize, @as(isize, newfd)),
                @ptrToInt(newpath),
                0,
            );
        }
    }

    pub fn renameat2(oldfd: i32, oldpath: [*:0]const u8, newfd: i32, newpath: [*:0]const u8, flags: u32) usize {
        return syscall5(
            .renameat2,
            @bitCast(usize, @as(isize, oldfd)),
            @ptrToInt(oldpath),
            @bitCast(usize, @as(isize, newfd)),
            @ptrToInt(newpath),
            flags,
        );
    }

    pub fn open(path: [*:0]const u8, flags: u32, perm: mode_t) usize {
        if (@hasField(SYS, "open")) {
            return syscall3(.open, @ptrToInt(path), flags, perm);
        } else {
            return syscall4(
                .openat,
                @bitCast(usize, @as(isize, AT.FDCWD)),
                @ptrToInt(path),
                flags,
                perm,
            );
        }
    }

    pub fn create(path: [*:0]const u8, perm: mode_t) usize {
        return syscall2(.creat, @ptrToInt(path), perm);
    }

    pub fn openat(dirfd: i32, path: [*:0]const u8, flags: u32, mode: mode_t) usize {
        // dirfd could be negative, for example AT.FDCWD is -100

        return syscall4(.openat, @bitCast(usize, @as(isize, dirfd)), @ptrToInt(path), flags, mode);
    }

    /// See also `clone` (from the arch-specific include)
    pub fn clone5(flags: usize, child_stack_ptr: usize, parent_tid: *i32, child_tid: *i32, newtls: usize) usize {
        return syscall5(.clone, flags, child_stack_ptr, @ptrToInt(parent_tid), @ptrToInt(child_tid), newtls);
    }

    /// See also `clone` (from the arch-specific include)
    pub fn clone2(flags: u32, child_stack_ptr: usize) usize {
        return syscall2(.clone, flags, child_stack_ptr);
    }

    pub fn close(fd: i32) usize {
        return syscall1(.close, @bitCast(usize, @as(isize, fd)));
    }

    pub fn fchmod(fd: i32, mode: mode_t) usize {
        return syscall2(.fchmod, @bitCast(usize, @as(isize, fd)), mode);
    }

    pub fn fchown(fd: i32, owner: uid_t, group: gid_t) usize {
        if (@hasField(SYS, "fchown32")) {
            return syscall3(.fchown32, @bitCast(usize, @as(isize, fd)), owner, group);
        } else {
            return syscall3(.fchown, @bitCast(usize, @as(isize, fd)), owner, group);
        }
    }

    /// Can only be called on 32 bit systems. For 64 bit see `lseek`.
    pub fn llseek(fd: i32, offset: u64, result: ?*u64, whence: usize) usize {
        // NOTE: The offset parameter splitting is independent from the target

        // endianness.

        return syscall5(
            ._llseek,
            @bitCast(usize, @as(isize, fd)),
            @truncate(usize, offset >> 32),
            @truncate(usize, offset),
            @ptrToInt(result),
            whence,
        );
    }

    /// Can only be called on 64 bit systems. For 32 bit see `llseek`.
    pub fn lseek(fd: i32, offset: i64, whence: usize) usize {
        return syscall3(.lseek, @bitCast(usize, @as(isize, fd)), @bitCast(usize, offset), whence);
    }

    pub fn exit(status: i32) noreturn {
        _ = syscall1(.exit, @bitCast(usize, @as(isize, status)));
        unreachable;
    }

    pub fn exit_group(status: i32) noreturn {
        _ = syscall1(.exit_group, @bitCast(usize, @as(isize, status)));
        unreachable;
    }

    /// flags for the `reboot' system call.
    pub const LINUX_REBOOT = struct {
        /// First magic value required to use _reboot() system call.
        pub const MAGIC1 = enum(u32) {
            MAGIC1 = 0xfee1dead,
            _,
        };

        /// Second magic value required to use _reboot() system call.
        pub const MAGIC2 = enum(u32) {
            MAGIC2 = 672274793,
            MAGIC2A = 85072278,
            MAGIC2B = 369367448,
            MAGIC2C = 537993216,
            _,
        };

        /// Commands accepted by the _reboot() system call.
        pub const CMD = enum(u32) {
            /// Restart system using default command and mode.
            RESTART = 0x01234567,

            /// Stop OS and give system control to ROM monitor, if any.
            HALT = 0xCDEF0123,

            /// Ctrl-Alt-Del sequence causes RESTART command.
            CAD_ON = 0x89ABCDEF,

            /// Ctrl-Alt-Del sequence sends SIGINT to init task.
            CAD_OFF = 0x00000000,

            /// Stop OS and remove all power from system, if possible.
            POWER_OFF = 0x4321FEDC,

            /// Restart system using given command string.
            RESTART2 = 0xA1B2C3D4,

            /// Suspend system using software suspend if compiled in.
            SW_SUSPEND = 0xD000FCE2,

            /// Restart system using a previously loaded Linux kernel
            KEXEC = 0x45584543,

            _,
        };
    };

    pub fn reboot(magic: LINUX_REBOOT.MAGIC1, magic2: LINUX_REBOOT.MAGIC2, cmd: LINUX_REBOOT.CMD, arg: ?*const anyopaque) usize {
        return std.os.linux.syscall4(
            .reboot,
            @enumToInt(magic),
            @enumToInt(magic2),
            @enumToInt(cmd),
            @ptrToInt(arg),
        );
    }

    pub fn getrandom(buf: [*]u8, count: usize, flags: u32) usize {
        return syscall3(.getrandom, @ptrToInt(buf), count, flags);
    }

    pub fn kill(pid: pid_t, sig: i32) usize {
        return syscall2(.kill, @bitCast(usize, @as(isize, pid)), @bitCast(usize, @as(isize, sig)));
    }

    pub fn tkill(tid: pid_t, sig: i32) usize {
        return syscall2(.tkill, @bitCast(usize, @as(isize, tid)), @bitCast(usize, @as(isize, sig)));
    }

    pub fn tgkill(tgid: pid_t, tid: pid_t, sig: i32) usize {
        return syscall3(.tgkill, @bitCast(usize, @as(isize, tgid)), @bitCast(usize, @as(isize, tid)), @bitCast(usize, @as(isize, sig)));
    }

    pub fn link(oldpath: [*:0]const u8, newpath: [*:0]const u8, flags: i32) usize {
        if (@hasField(SYS, "link")) {
            return syscall3(
                .link,
                @ptrToInt(oldpath),
                @ptrToInt(newpath),
                @bitCast(usize, @as(isize, flags)),
            );
        } else {
            return syscall5(
                .linkat,
                @bitCast(usize, @as(isize, AT.FDCWD)),
                @ptrToInt(oldpath),
                @bitCast(usize, @as(isize, AT.FDCWD)),
                @ptrToInt(newpath),
                @bitCast(usize, @as(isize, flags)),
            );
        }
    }

    pub fn linkat(oldfd: fd_t, oldpath: [*:0]const u8, newfd: fd_t, newpath: [*:0]const u8, flags: i32) usize {
        return syscall5(
            .linkat,
            @bitCast(usize, @as(isize, oldfd)),
            @ptrToInt(oldpath),
            @bitCast(usize, @as(isize, newfd)),
            @ptrToInt(newpath),
            @bitCast(usize, @as(isize, flags)),
        );
    }

    pub fn unlink(path: [*:0]const u8) usize {
        if (@hasField(SYS, "unlink")) {
            return syscall1(.unlink, @ptrToInt(path));
        } else {
            return syscall3(.unlinkat, @bitCast(usize, @as(isize, AT.FDCWD)), @ptrToInt(path), 0);
        }
    }

    pub fn unlinkat(dirfd: i32, path: [*:0]const u8, flags: u32) usize {
        return syscall3(.unlinkat, @bitCast(usize, @as(isize, dirfd)), @ptrToInt(path), flags);
    }

    pub fn waitpid(pid: pid_t, status: *u32, flags: u32) usize {
        return syscall4(.wait4, @bitCast(usize, @as(isize, pid)), @ptrToInt(status), flags, 0);
    }

    pub fn waitid(id_type: P, id: i32, infop: *siginfo_t, flags: u32) usize {
        return syscall5(.waitid, @enumToInt(id_type), @bitCast(usize, @as(isize, id)), @ptrToInt(infop), flags, 0);
    }

    pub fn fcntl(fd: fd_t, cmd: i32, arg: usize) usize {
        return syscall3(.fcntl, @bitCast(usize, @as(isize, fd)), @bitCast(usize, @as(isize, cmd)), arg);
    }

    pub fn flock(fd: fd_t, operation: i32) usize {
        return syscall2(.flock, @bitCast(usize, @as(isize, fd)), @bitCast(usize, @as(isize, operation)));
    }

    var vdso_clock_gettime = if (builtin.zig_backend == .stage1)
        @ptrCast(?*const anyopaque, init_vdso_clock_gettime)
    else
        @ptrCast(?*const anyopaque, &init_vdso_clock_gettime);

    // We must follow the C calling convention when we call into the VDSO

    const vdso_clock_gettime_ty = if (builtin.zig_backend == .stage1)
        fn (i32, *timespec) callconv(.C) usize
    else
        *align(1) const fn (i32, *timespec) callconv(.C) usize;

    pub fn clock_gettime(clk_id: i32, tp: *timespec) usize {
        if (@hasDecl(VDSO, "CGT_SYM")) {
            const ptr = @atomicLoad(?*const anyopaque, &vdso_clock_gettime, .Unordered);
            if (ptr) |fn_ptr| {
                const f = @ptrCast(vdso_clock_gettime_ty, fn_ptr);
                const rc = f(clk_id, tp);
                switch (rc) {
                    0, @bitCast(usize, -@as(isize, @enumToInt(E.INVAL))) => return rc,
                    else => {},
                }
            }
        }
        return syscall2(.clock_gettime, @bitCast(usize, @as(isize, clk_id)), @ptrToInt(tp));
    }

    fn init_vdso_clock_gettime(clk: i32, ts: *timespec) callconv(.C) usize {
        const ptr = @intToPtr(?*const anyopaque, vdso.lookup(VDSO.CGT_VER, VDSO.CGT_SYM));
        // Note that we may not have a VDSO at all, update the stub address anyway

        // so that clock_gettime will fall back on the good old (and slow) syscall

        @atomicStore(?*const anyopaque, &vdso_clock_gettime, ptr, .Monotonic);
        // Call into the VDSO if available

        if (ptr) |fn_ptr| {
            const f = @ptrCast(vdso_clock_gettime_ty, fn_ptr);
            return f(clk, ts);
        }
        return @bitCast(usize, -@as(isize, @enumToInt(E.NOSYS)));
    }

    pub fn clock_getres(clk_id: i32, tp: *timespec) usize {
        return syscall2(.clock_getres, @bitCast(usize, @as(isize, clk_id)), @ptrToInt(tp));
    }

    pub fn clock_settime(clk_id: i32, tp: *const timespec) usize {
        return syscall2(.clock_settime, @bitCast(usize, @as(isize, clk_id)), @ptrToInt(tp));
    }

    pub fn gettimeofday(tv: *timeval, tz: *timezone) usize {
        return syscall2(.gettimeofday, @ptrToInt(tv), @ptrToInt(tz));
    }

    pub fn settimeofday(tv: *const timeval, tz: *const timezone) usize {
        return syscall2(.settimeofday, @ptrToInt(tv), @ptrToInt(tz));
    }

    pub fn nanosleep(req: *const timespec, rem: ?*timespec) usize {
        return syscall2(.nanosleep, @ptrToInt(req), @ptrToInt(rem));
    }

    pub fn setuid(uid: uid_t) usize {
        if (@hasField(SYS, "setuid32")) {
            return syscall1(.setuid32, uid);
        } else {
            return syscall1(.setuid, uid);
        }
    }

    pub fn setgid(gid: gid_t) usize {
        if (@hasField(SYS, "setgid32")) {
            return syscall1(.setgid32, gid);
        } else {
            return syscall1(.setgid, gid);
        }
    }

    pub fn setreuid(ruid: uid_t, euid: uid_t) usize {
        if (@hasField(SYS, "setreuid32")) {
            return syscall2(.setreuid32, ruid, euid);
        } else {
            return syscall2(.setreuid, ruid, euid);
        }
    }

    pub fn setregid(rgid: gid_t, egid: gid_t) usize {
        if (@hasField(SYS, "setregid32")) {
            return syscall2(.setregid32, rgid, egid);
        } else {
            return syscall2(.setregid, rgid, egid);
        }
    }

    pub fn getuid() uid_t {
        if (@hasField(SYS, "getuid32")) {
            return @intCast(uid_t, syscall0(.getuid32));
        } else {
            return @intCast(uid_t, syscall0(.getuid));
        }
    }

    pub fn getgid() gid_t {
        if (@hasField(SYS, "getgid32")) {
            return @intCast(gid_t, syscall0(.getgid32));
        } else {
            return @intCast(gid_t, syscall0(.getgid));
        }
    }

    pub fn geteuid() uid_t {
        if (@hasField(SYS, "geteuid32")) {
            return @intCast(uid_t, syscall0(.geteuid32));
        } else {
            return @intCast(uid_t, syscall0(.geteuid));
        }
    }

    pub fn getegid() gid_t {
        if (@hasField(SYS, "getegid32")) {
            return @intCast(gid_t, syscall0(.getegid32));
        } else {
            return @intCast(gid_t, syscall0(.getegid));
        }
    }

    pub fn seteuid(euid: uid_t) usize {
        // We use setresuid here instead of setreuid to ensure that the saved uid

        // is not changed. This is what musl and recent glibc versions do as well.

        //

        // The setresuid(2) man page says that if -1 is passed the corresponding

        // id will not be changed. Since uid_t is unsigned, this wraps around to the

        // max value in C.

        comptime assert(@typeInfo(uid_t) == .Int and @typeInfo(uid_t).Int.signedness == .unsigned);
        return setresuid(std.math.maxInt(uid_t), euid, std.math.maxInt(uid_t));
    }

    pub fn setegid(egid: gid_t) usize {
        // We use setresgid here instead of setregid to ensure that the saved uid

        // is not changed. This is what musl and recent glibc versions do as well.

        //

        // The setresgid(2) man page says that if -1 is passed the corresponding

        // id will not be changed. Since gid_t is unsigned, this wraps around to the

        // max value in C.

        comptime assert(@typeInfo(uid_t) == .Int and @typeInfo(uid_t).Int.signedness == .unsigned);
        return setresgid(std.math.maxInt(gid_t), egid, std.math.maxInt(gid_t));
    }

    pub fn getresuid(ruid: *uid_t, euid: *uid_t, suid: *uid_t) usize {
        if (@hasField(SYS, "getresuid32")) {
            return syscall3(.getresuid32, @ptrToInt(ruid), @ptrToInt(euid), @ptrToInt(suid));
        } else {
            return syscall3(.getresuid, @ptrToInt(ruid), @ptrToInt(euid), @ptrToInt(suid));
        }
    }

    pub fn getresgid(rgid: *gid_t, egid: *gid_t, sgid: *gid_t) usize {
        if (@hasField(SYS, "getresgid32")) {
            return syscall3(.getresgid32, @ptrToInt(rgid), @ptrToInt(egid), @ptrToInt(sgid));
        } else {
            return syscall3(.getresgid, @ptrToInt(rgid), @ptrToInt(egid), @ptrToInt(sgid));
        }
    }

    pub fn setresuid(ruid: uid_t, euid: uid_t, suid: uid_t) usize {
        if (@hasField(SYS, "setresuid32")) {
            return syscall3(.setresuid32, ruid, euid, suid);
        } else {
            return syscall3(.setresuid, ruid, euid, suid);
        }
    }

    pub fn setresgid(rgid: gid_t, egid: gid_t, sgid: gid_t) usize {
        if (@hasField(SYS, "setresgid32")) {
            return syscall3(.setresgid32, rgid, egid, sgid);
        } else {
            return syscall3(.setresgid, rgid, egid, sgid);
        }
    }

    pub fn getgroups(size: usize, list: *gid_t) usize {
        if (@hasField(SYS, "getgroups32")) {
            return syscall2(.getgroups32, size, @ptrToInt(list));
        } else {
            return syscall2(.getgroups, size, @ptrToInt(list));
        }
    }

    pub fn setgroups(size: usize, list: [*]const gid_t) usize {
        if (@hasField(SYS, "setgroups32")) {
            return syscall2(.setgroups32, size, @ptrToInt(list));
        } else {
            return syscall2(.setgroups, size, @ptrToInt(list));
        }
    }

    pub fn getpid() pid_t {
        return @bitCast(pid_t, @truncate(u32, syscall0(.getpid)));
    }

    pub fn gettid() pid_t {
        return @bitCast(pid_t, @truncate(u32, syscall0(.gettid)));
    }

    pub fn sigprocmask(flags: u32, noalias set: ?*const sigset_t, noalias oldset: ?*sigset_t) usize {
        return syscall4(.rt_sigprocmask, flags, @ptrToInt(set), @ptrToInt(oldset), NSIG / 8);
    }

    pub fn sigaction(sig: u6, noalias act: ?*const Sigaction, noalias oact: ?*Sigaction) usize {
        assert(sig >= 1);
        assert(sig != SIG.KILL);
        assert(sig != SIG.STOP);

        var ksa: k_sigaction = undefined;
        var oldksa: k_sigaction = undefined;
        const mask_size = @sizeOf(@TypeOf(ksa.mask));

        if (act) |new| {
            const restore_rt_ptr = if (builtin.zig_backend == .stage1) restore_rt else &restore_rt;
            const restore_ptr = if (builtin.zig_backend == .stage1) restore else &restore;
            const restorer_fn = if ((new.flags & SA.SIGINFO) != 0) restore_rt_ptr else restore_ptr;
            ksa = k_sigaction{
                .handler = new.handler.handler,
                .flags = new.flags | SA.RESTORER,
                .mask = undefined,
                .restorer = @ptrCast(k_sigaction_funcs.restorer, restorer_fn),
            };
            @memcpy(@ptrCast([*]u8, &ksa.mask), @ptrCast([*]const u8, &new.mask), mask_size);
        }

        const ksa_arg = if (act != null) @ptrToInt(&ksa) else 0;
        const oldksa_arg = if (oact != null) @ptrToInt(&oldksa) else 0;

        const result = switch (native_arch) {
            // The sparc version of rt_sigaction needs the restorer function to be passed as an argument too.

            .sparc, .sparc64 => syscall5(.rt_sigaction, sig, ksa_arg, oldksa_arg, @ptrToInt(ksa.restorer), mask_size),
            else => syscall4(.rt_sigaction, sig, ksa_arg, oldksa_arg, mask_size),
        };
        if (getErrno(result) != .SUCCESS) return result;

        if (oact) |old| {
            old.handler.handler = oldksa.handler;
            old.flags = @truncate(c_uint, oldksa.flags);
            @memcpy(@ptrCast([*]u8, &old.mask), @ptrCast([*]const u8, &oldksa.mask), mask_size);
        }

        return 0;
    }

    const usize_bits = @typeInfo(usize).Int.bits;

    pub fn sigaddset(set: *sigset_t, sig: u6) void {
        const s = sig - 1;
        // shift in musl: s&8*sizeof *set->__bits-1

        const shift = @intCast(u5, s & (usize_bits - 1));
        const val = @intCast(u32, 1) << shift;
        (set.*)[@intCast(usize, s) / usize_bits] |= val;
    }

    pub fn sigismember(set: *const sigset_t, sig: u6) bool {
        const s = sig - 1;
        return ((set.*)[@intCast(usize, s) / usize_bits] & (@intCast(usize, 1) << (s & (usize_bits - 1)))) != 0;
    }

    pub fn getsockname(fd: i32, noalias addr: *sockaddr, noalias len: *socklen_t) usize {
        if (native_arch == .i386) {
            return socketcall(SC.getsockname, &[3]usize{ @bitCast(usize, @as(isize, fd)), @ptrToInt(addr), @ptrToInt(len) });
        }
        return syscall3(.getsockname, @bitCast(usize, @as(isize, fd)), @ptrToInt(addr), @ptrToInt(len));
    }

    pub fn getpeername(fd: i32, noalias addr: *sockaddr, noalias len: *socklen_t) usize {
        if (native_arch == .i386) {
            return socketcall(SC.getpeername, &[3]usize{ @bitCast(usize, @as(isize, fd)), @ptrToInt(addr), @ptrToInt(len) });
        }
        return syscall3(.getpeername, @bitCast(usize, @as(isize, fd)), @ptrToInt(addr), @ptrToInt(len));
    }

    pub fn socket(domain: u32, socket_type: u32, protocol: u32) usize {
        if (native_arch == .i386) {
            return socketcall(SC.socket, &[3]usize{ domain, socket_type, protocol });
        }
        return syscall3(.socket, domain, socket_type, protocol);
    }

    pub fn setsockopt(fd: i32, level: u32, optname: u32, optval: [*]const u8, optlen: socklen_t) usize {
        if (native_arch == .i386) {
            return socketcall(SC.setsockopt, &[5]usize{ @bitCast(usize, @as(isize, fd)), level, optname, @ptrToInt(optval), @intCast(usize, optlen) });
        }
        return syscall5(.setsockopt, @bitCast(usize, @as(isize, fd)), level, optname, @ptrToInt(optval), @intCast(usize, optlen));
    }

    pub fn getsockopt(fd: i32, level: u32, optname: u32, noalias optval: [*]u8, noalias optlen: *socklen_t) usize {
        if (native_arch == .i386) {
            return socketcall(SC.getsockopt, &[5]usize{ @bitCast(usize, @as(isize, fd)), level, optname, @ptrToInt(optval), @ptrToInt(optlen) });
        }
        return syscall5(.getsockopt, @bitCast(usize, @as(isize, fd)), level, optname, @ptrToInt(optval), @ptrToInt(optlen));
    }

    pub fn sendmsg(fd: i32, msg: *const std.x.os.Socket.Message, flags: c_int) usize {
        if (native_arch == .i386) {
            return socketcall(SC.sendmsg, &[3]usize{ @bitCast(usize, @as(isize, fd)), @ptrToInt(msg), @bitCast(usize, @as(isize, flags)) });
        }
        return syscall3(.sendmsg, @bitCast(usize, @as(isize, fd)), @ptrToInt(msg), @bitCast(usize, @as(isize, flags)));
    }

    pub fn sendmmsg(fd: i32, msgvec: [*]mmsghdr_const, vlen: u32, flags: u32) usize {
        if (@typeInfo(usize).Int.bits > @typeInfo(@TypeOf(mmsghdr(undefined).msg_len)).Int.bits) {
            // workaround kernel brokenness:

            // if adding up all iov_len overflows a i32 then split into multiple calls

            // see https://www.openwall.com/lists/musl/2014/06/07/5

            const kvlen = if (vlen > IOV_MAX) IOV_MAX else vlen; // matches kernel

            var next_unsent: usize = 0;
            for (msgvec[0..kvlen]) |*msg, i| {
                var size: i32 = 0;
                const msg_iovlen = @intCast(usize, msg.msg_hdr.msg_iovlen); // kernel side this is treated as unsigned

                for (msg.msg_hdr.msg_iov[0..msg_iovlen]) |iov| {
                    if (iov.iov_len > std.math.maxInt(i32) or @addWithOverflow(i32, size, @intCast(i32, iov.iov_len), &size)) {
                        // batch-send all messages up to the current message

                        if (next_unsent < i) {
                            const batch_size = i - next_unsent;
                            const r = syscall4(.sendmmsg, @bitCast(usize, @as(isize, fd)), @ptrToInt(&msgvec[next_unsent]), batch_size, flags);
                            if (getErrno(r) != 0) return next_unsent;
                            if (r < batch_size) return next_unsent + r;
                        }
                        // send current message as own packet

                        const r = sendmsg(fd, &msg.msg_hdr, flags);
                        if (getErrno(r) != 0) return r;
                        // Linux limits the total bytes sent by sendmsg to INT_MAX, so this cast is safe.

                        msg.msg_len = @intCast(u32, r);
                        next_unsent = i + 1;
                        break;
                    }
                }
            }
            if (next_unsent < kvlen or next_unsent == 0) { // want to make sure at least one syscall occurs (e.g. to trigger MSG.EOR)

                const batch_size = kvlen - next_unsent;
                const r = syscall4(.sendmmsg, @bitCast(usize, @as(isize, fd)), @ptrToInt(&msgvec[next_unsent]), batch_size, flags);
                if (getErrno(r) != 0) return r;
                return next_unsent + r;
            }
            return kvlen;
        }
        return syscall4(.sendmmsg, @bitCast(usize, @as(isize, fd)), @ptrToInt(msgvec), vlen, flags);
    }

    pub fn connect(fd: i32, addr: *const anyopaque, len: socklen_t) usize {
        if (native_arch == .i386) {
            return socketcall(SC.connect, &[3]usize{ @bitCast(usize, @as(isize, fd)), @ptrToInt(addr), len });
        }
        return syscall3(.connect, @bitCast(usize, @as(isize, fd)), @ptrToInt(addr), len);
    }

    pub fn recvmsg(fd: i32, msg: *std.x.os.Socket.Message, flags: c_int) usize {
        if (native_arch == .i386) {
            return socketcall(SC.recvmsg, &[3]usize{ @bitCast(usize, @as(isize, fd)), @ptrToInt(msg), @bitCast(usize, @as(isize, flags)) });
        }
        return syscall3(.recvmsg, @bitCast(usize, @as(isize, fd)), @ptrToInt(msg), @bitCast(usize, @as(isize, flags)));
    }

    pub fn recvfrom(fd: i32, noalias buf: [*]u8, len: usize, flags: u32, noalias addr: ?*sockaddr, noalias alen: ?*socklen_t) usize {
        if (native_arch == .i386) {
            return socketcall(SC.recvfrom, &[6]usize{ @bitCast(usize, @as(isize, fd)), @ptrToInt(buf), len, flags, @ptrToInt(addr), @ptrToInt(alen) });
        }
        return syscall6(.recvfrom, @bitCast(usize, @as(isize, fd)), @ptrToInt(buf), len, flags, @ptrToInt(addr), @ptrToInt(alen));
    }

    pub fn shutdown(fd: i32, how: i32) usize {
        if (native_arch == .i386) {
            return socketcall(SC.shutdown, &[2]usize{ @bitCast(usize, @as(isize, fd)), @bitCast(usize, @as(isize, how)) });
        }
        return syscall2(.shutdown, @bitCast(usize, @as(isize, fd)), @bitCast(usize, @as(isize, how)));
    }

    pub fn bind(fd: i32, addr: *const sockaddr, len: socklen_t) usize {
        if (native_arch == .i386) {
            return socketcall(SC.bind, &[3]usize{ @bitCast(usize, @as(isize, fd)), @ptrToInt(addr), @intCast(usize, len) });
        }
        return syscall3(.bind, @bitCast(usize, @as(isize, fd)), @ptrToInt(addr), @intCast(usize, len));
    }

    pub fn listen(fd: i32, backlog: u32) usize {
        if (native_arch == .i386) {
            return socketcall(SC.listen, &[2]usize{ @bitCast(usize, @as(isize, fd)), backlog });
        }
        return syscall2(.listen, @bitCast(usize, @as(isize, fd)), backlog);
    }

    pub fn sendto(fd: i32, buf: [*]const u8, len: usize, flags: u32, addr: ?*const sockaddr, alen: socklen_t) usize {
        if (native_arch == .i386) {
            return socketcall(SC.sendto, &[6]usize{ @bitCast(usize, @as(isize, fd)), @ptrToInt(buf), len, flags, @ptrToInt(addr), @intCast(usize, alen) });
        }
        return syscall6(.sendto, @bitCast(usize, @as(isize, fd)), @ptrToInt(buf), len, flags, @ptrToInt(addr), @intCast(usize, alen));
    }

    pub fn sendfile(outfd: i32, infd: i32, offset: ?*i64, count: usize) usize {
        if (@hasField(SYS, "sendfile64")) {
            return syscall4(
                .sendfile64,
                @bitCast(usize, @as(isize, outfd)),
                @bitCast(usize, @as(isize, infd)),
                @ptrToInt(offset),
                count,
            );
        } else {
            return syscall4(
                .sendfile,
                @bitCast(usize, @as(isize, outfd)),
                @bitCast(usize, @as(isize, infd)),
                @ptrToInt(offset),
                count,
            );
        }
    }

    pub fn socketpair(domain: i32, socket_type: i32, protocol: i32, fd: *[2]i32) usize {
        if (native_arch == .i386) {
            return socketcall(SC.socketpair, &[4]usize{ @intCast(usize, domain), @intCast(usize, socket_type), @intCast(usize, protocol), @ptrToInt(fd) });
        }
        return syscall4(.socketpair, @intCast(usize, domain), @intCast(usize, socket_type), @intCast(usize, protocol), @ptrToInt(fd));
    }

    pub fn accept(fd: i32, noalias addr: ?*sockaddr, noalias len: ?*socklen_t) usize {
        if (native_arch == .i386) {
            return socketcall(SC.accept, &[4]usize{ fd, addr, len, 0 });
        }
        return accept4(fd, addr, len, 0);
    }

    pub fn accept4(fd: i32, noalias addr: ?*sockaddr, noalias len: ?*socklen_t, flags: u32) usize {
        if (native_arch == .i386) {
            return socketcall(SC.accept4, &[4]usize{ @bitCast(usize, @as(isize, fd)), @ptrToInt(addr), @ptrToInt(len), flags });
        }
        return syscall4(.accept4, @bitCast(usize, @as(isize, fd)), @ptrToInt(addr), @ptrToInt(len), flags);
    }

    pub fn fstat(fd: i32, stat_buf: *Stat) usize {
        if (@hasField(SYS, "fstat64")) {
            return syscall2(.fstat64, @bitCast(usize, @as(isize, fd)), @ptrToInt(stat_buf));
        } else {
            return syscall2(.fstat, @bitCast(usize, @as(isize, fd)), @ptrToInt(stat_buf));
        }
    }

    pub fn stat(pathname: [*:0]const u8, statbuf: *Stat) usize {
        if (@hasField(SYS, "stat64")) {
            return syscall2(.stat64, @ptrToInt(pathname), @ptrToInt(statbuf));
        } else {
            return syscall2(.stat, @ptrToInt(pathname), @ptrToInt(statbuf));
        }
    }

    pub fn lstat(pathname: [*:0]const u8, statbuf: *Stat) usize {
        if (@hasField(SYS, "lstat64")) {
            return syscall2(.lstat64, @ptrToInt(pathname), @ptrToInt(statbuf));
        } else {
            return syscall2(.lstat, @ptrToInt(pathname), @ptrToInt(statbuf));
        }
    }

    pub fn fstatat(dirfd: i32, path: [*:0]const u8, stat_buf: *Stat, flags: u32) usize {
        if (@hasField(SYS, "fstatat64")) {
            return syscall4(.fstatat64, @bitCast(usize, @as(isize, dirfd)), @ptrToInt(path), @ptrToInt(stat_buf), flags);
        } else {
            return syscall4(.fstatat, @bitCast(usize, @as(isize, dirfd)), @ptrToInt(path), @ptrToInt(stat_buf), flags);
        }
    }

    pub fn statx(dirfd: i32, path: [*]const u8, flags: u32, mask: u32, statx_buf: *Statx) usize {
        if (@hasField(SYS, "statx")) {
            return syscall5(
                .statx,
                @bitCast(usize, @as(isize, dirfd)),
                @ptrToInt(path),
                flags,
                mask,
                @ptrToInt(statx_buf),
            );
        }
        return @bitCast(usize, -@as(isize, @enumToInt(E.NOSYS)));
    }

    pub fn listxattr(path: [*:0]const u8, list: [*]u8, size: usize) usize {
        return syscall3(.listxattr, @ptrToInt(path), @ptrToInt(list), size);
    }

    pub fn llistxattr(path: [*:0]const u8, list: [*]u8, size: usize) usize {
        return syscall3(.llistxattr, @ptrToInt(path), @ptrToInt(list), size);
    }

    pub fn flistxattr(fd: usize, list: [*]u8, size: usize) usize {
        return syscall3(.flistxattr, fd, @ptrToInt(list), size);
    }

    pub fn getxattr(path: [*:0]const u8, name: [*:0]const u8, value: [*]u8, size: usize) usize {
        return syscall4(.getxattr, @ptrToInt(path), @ptrToInt(name), @ptrToInt(value), size);
    }

    pub fn lgetxattr(path: [*:0]const u8, name: [*:0]const u8, value: [*]u8, size: usize) usize {
        return syscall4(.lgetxattr, @ptrToInt(path), @ptrToInt(name), @ptrToInt(value), size);
    }

    pub fn fgetxattr(fd: usize, name: [*:0]const u8, value: [*]u8, size: usize) usize {
        return syscall4(.lgetxattr, fd, @ptrToInt(name), @ptrToInt(value), size);
    }

    pub fn setxattr(path: [*:0]const u8, name: [*:0]const u8, value: *const void, size: usize, flags: usize) usize {
        return syscall5(.setxattr, @ptrToInt(path), @ptrToInt(name), @ptrToInt(value), size, flags);
    }

    pub fn lsetxattr(path: [*:0]const u8, name: [*:0]const u8, value: *const void, size: usize, flags: usize) usize {
        return syscall5(.lsetxattr, @ptrToInt(path), @ptrToInt(name), @ptrToInt(value), size, flags);
    }

    pub fn fsetxattr(fd: usize, name: [*:0]const u8, value: *const void, size: usize, flags: usize) usize {
        return syscall5(.fsetxattr, fd, @ptrToInt(name), @ptrToInt(value), size, flags);
    }

    pub fn removexattr(path: [*:0]const u8, name: [*:0]const u8) usize {
        return syscall2(.removexattr, @ptrToInt(path), @ptrToInt(name));
    }

    pub fn lremovexattr(path: [*:0]const u8, name: [*:0]const u8) usize {
        return syscall2(.lremovexattr, @ptrToInt(path), @ptrToInt(name));
    }

    pub fn fremovexattr(fd: usize, name: [*:0]const u8) usize {
        return syscall2(.fremovexattr, fd, @ptrToInt(name));
    }

    pub fn sched_yield() usize {
        return syscall0(.sched_yield);
    }

    pub fn sched_getaffinity(pid: pid_t, size: usize, set: *cpu_set_t) usize {
        const rc = syscall3(.sched_getaffinity, @bitCast(usize, @as(isize, pid)), size, @ptrToInt(set));
        if (@bitCast(isize, rc) < 0) return rc;
        if (rc < size) @memset(@ptrCast([*]u8, set) + rc, 0, size - rc);
        return 0;
    }

    pub fn epoll_create() usize {
        return epoll_create1(0);
    }

    pub fn epoll_create1(flags: usize) usize {
        return syscall1(.epoll_create1, flags);
    }

    pub fn epoll_ctl(epoll_fd: i32, op: u32, fd: i32, ev: ?*epoll_event) usize {
        return syscall4(.epoll_ctl, @bitCast(usize, @as(isize, epoll_fd)), @intCast(usize, op), @bitCast(usize, @as(isize, fd)), @ptrToInt(ev));
    }

    pub fn epoll_wait(epoll_fd: i32, events: [*]epoll_event, maxevents: u32, timeout: i32) usize {
        return epoll_pwait(epoll_fd, events, maxevents, timeout, null);
    }

    pub fn epoll_pwait(epoll_fd: i32, events: [*]epoll_event, maxevents: u32, timeout: i32, sigmask: ?*const sigset_t) usize {
        return syscall6(
            .epoll_pwait,
            @bitCast(usize, @as(isize, epoll_fd)),
            @ptrToInt(events),
            @intCast(usize, maxevents),
            @bitCast(usize, @as(isize, timeout)),
            @ptrToInt(sigmask),
            @sizeOf(sigset_t),
        );
    }

    pub fn eventfd(count: u32, flags: u32) usize {
        return syscall2(.eventfd2, count, flags);
    }

    pub fn timerfd_create(clockid: i32, flags: u32) usize {
        return syscall2(.timerfd_create, @bitCast(usize, @as(isize, clockid)), flags);
    }

    pub const itimerspec = extern struct {
        it_interval: timespec,
        it_value: timespec,
    };

    pub fn timerfd_gettime(fd: i32, curr_value: *itimerspec) usize {
        return syscall2(.timerfd_gettime, @bitCast(usize, @as(isize, fd)), @ptrToInt(curr_value));
    }

    pub fn timerfd_settime(fd: i32, flags: u32, new_value: *const itimerspec, old_value: ?*itimerspec) usize {
        return syscall4(.timerfd_settime, @bitCast(usize, @as(isize, fd)), flags, @ptrToInt(new_value), @ptrToInt(old_value));
    }

    pub fn unshare(flags: usize) usize {
        return syscall1(.unshare, flags);
    }

    pub fn capget(hdrp: *cap_user_header_t, datap: *cap_user_data_t) usize {
        return syscall2(.capget, @ptrToInt(hdrp), @ptrToInt(datap));
    }

    pub fn capset(hdrp: *cap_user_header_t, datap: *const cap_user_data_t) usize {
        return syscall2(.capset, @ptrToInt(hdrp), @ptrToInt(datap));
    }

    pub fn sigaltstack(ss: ?*stack_t, old_ss: ?*stack_t) usize {
        return syscall2(.sigaltstack, @ptrToInt(ss), @ptrToInt(old_ss));
    }

    pub fn uname(uts: *utsname) usize {
        return syscall1(.uname, @ptrToInt(uts));
    }

    pub fn io_uring_setup(entries: u32, p: *io_uring_params) usize {
        return syscall2(.io_uring_setup, entries, @ptrToInt(p));
    }

    pub fn io_uring_enter(fd: i32, to_submit: u32, min_complete: u32, flags: u32, sig: ?*sigset_t) usize {
        return syscall6(.io_uring_enter, @bitCast(usize, @as(isize, fd)), to_submit, min_complete, flags, @ptrToInt(sig), NSIG / 8);
    }

    pub fn io_uring_register(fd: i32, opcode: IORING_REGISTER, arg: ?*const anyopaque, nr_args: u32) usize {
        return syscall4(.io_uring_register, @bitCast(usize, @as(isize, fd)), @enumToInt(opcode), @ptrToInt(arg), nr_args);
    }

    pub fn memfd_create(name: [*:0]const u8, flags: u32) usize {
        return syscall2(.memfd_create, @ptrToInt(name), flags);
    }

    pub fn getrusage(who: i32, usage: *rusage) usize {
        return syscall2(.getrusage, @bitCast(usize, @as(isize, who)), @ptrToInt(usage));
    }

    pub fn tcgetattr(fd: fd_t, termios_p: *termios) usize {
        return syscall3(.ioctl, @bitCast(usize, @as(isize, fd)), T.CGETS, @ptrToInt(termios_p));
    }

    pub fn tcsetattr(fd: fd_t, optional_action: TCSA, termios_p: *const termios) usize {
        return syscall3(.ioctl, @bitCast(usize, @as(isize, fd)), T.CSETS + @enumToInt(optional_action), @ptrToInt(termios_p));
    }

    pub fn tcdrain(fd: fd_t) usize {
        return syscall3(.ioctl, @bitCast(usize, @as(isize, fd)), T.CSBRK, 1);
    }

    pub fn ioctl(fd: fd_t, request: u32, arg: usize) usize {
        return syscall3(.ioctl, @bitCast(usize, @as(isize, fd)), request, arg);
    }

    pub fn signalfd(fd: fd_t, mask: *const sigset_t, flags: u32) usize {
        return syscall4(.signalfd4, @bitCast(usize, @as(isize, fd)), @ptrToInt(mask), NSIG / 8, flags);
    }

    pub fn copy_file_range(fd_in: fd_t, off_in: ?*i64, fd_out: fd_t, off_out: ?*i64, len: usize, flags: u32) usize {
        return syscall6(
            .copy_file_range,
            @bitCast(usize, @as(isize, fd_in)),
            @ptrToInt(off_in),
            @bitCast(usize, @as(isize, fd_out)),
            @ptrToInt(off_out),
            len,
            flags,
        );
    }

    pub fn bpf(cmd: BPF.Cmd, attr: *BPF.Attr, size: u32) usize {
        return syscall3(.bpf, @enumToInt(cmd), @ptrToInt(attr), size);
    }

    pub fn sync() void {
        _ = syscall0(.sync);
    }

    pub fn syncfs(fd: fd_t) usize {
        return syscall1(.syncfs, @bitCast(usize, @as(isize, fd)));
    }

    pub fn fsync(fd: fd_t) usize {
        return syscall1(.fsync, @bitCast(usize, @as(isize, fd)));
    }

    pub fn fdatasync(fd: fd_t) usize {
        return syscall1(.fdatasync, @bitCast(usize, @as(isize, fd)));
    }

    pub fn prctl(option: i32, arg2: usize, arg3: usize, arg4: usize, arg5: usize) usize {
        return syscall5(.prctl, @bitCast(usize, @as(isize, option)), arg2, arg3, arg4, arg5);
    }

    pub fn getrlimit(resource: rlimit_resource, rlim: *rlimit) usize {
        // use prlimit64 to have 64 bit limits on 32 bit platforms

        return prlimit(0, resource, null, rlim);
    }

    pub fn setrlimit(resource: rlimit_resource, rlim: *const rlimit) usize {
        // use prlimit64 to have 64 bit limits on 32 bit platforms

        return prlimit(0, resource, rlim, null);
    }

    pub fn prlimit(pid: pid_t, resource: rlimit_resource, new_limit: ?*const rlimit, old_limit: ?*rlimit) usize {
        return syscall4(
            .prlimit64,
            @bitCast(usize, @as(isize, pid)),
            @bitCast(usize, @as(isize, @enumToInt(resource))),
            @ptrToInt(new_limit),
            @ptrToInt(old_limit),
        );
    }

    pub fn madvise(address: [*]u8, len: usize, advice: u32) usize {
        return syscall3(.madvise, @ptrToInt(address), len, advice);
    }

    pub fn pidfd_open(pid: pid_t, flags: u32) usize {
        return syscall2(.pidfd_open, @bitCast(usize, @as(isize, pid)), flags);
    }

    pub fn pidfd_getfd(pidfd: fd_t, targetfd: fd_t, flags: u32) usize {
        return syscall3(
            .pidfd_getfd,
            @bitCast(usize, @as(isize, pidfd)),
            @bitCast(usize, @as(isize, targetfd)),
            flags,
        );
    }

    pub fn pidfd_send_signal(pidfd: fd_t, sig: i32, info: ?*siginfo_t, flags: u32) usize {
        return syscall4(
            .pidfd_send_signal,
            @bitCast(usize, @as(isize, pidfd)),
            @bitCast(usize, @as(isize, sig)),
            @ptrToInt(info),
            flags,
        );
    }

    pub fn process_vm_readv(pid: pid_t, local: [*]const iovec, local_count: usize, remote: [*]const iovec, remote_count: usize, flags: usize) usize {
        return syscall6(
            .process_vm_readv,
            @bitCast(usize, @as(isize, pid)),
            @ptrToInt(local),
            local_count,
            @ptrToInt(remote),
            remote_count,
            flags,
        );
    }

    pub fn process_vm_writev(pid: pid_t, local: [*]const iovec, local_count: usize, remote: [*]const iovec, remote_count: usize, flags: usize) usize {
        return syscall6(
            .process_vm_writev,
            @bitCast(usize, @as(isize, pid)),
            @ptrToInt(local),
            local_count,
            @ptrToInt(remote),
            remote_count,
            flags,
        );
    }

    pub fn fadvise(fd: fd_t, offset: i64, len: i64, advice: usize) usize {
        if (comptime builtin.cpu.arch.isMIPS()) {
            // MIPS requires a 7 argument syscall

            const offset_halves = splitValue64(offset);
            const length_halves = splitValue64(len);

            return syscall7(
                .fadvise64,
                @bitCast(usize, @as(isize, fd)),
                0,
                offset_halves[0],
                offset_halves[1],
                length_halves[0],
                length_halves[1],
                advice,
            );
        } else if (comptime builtin.cpu.arch.isARM()) {
            // ARM reorders the arguments

            const offset_halves = splitValue64(offset);
            const length_halves = splitValue64(len);

            return syscall6(
                .fadvise64_64,
                @bitCast(usize, @as(isize, fd)),
                advice,
                offset_halves[0],
                offset_halves[1],
                length_halves[0],
                length_halves[1],
            );
        } else if (@hasField(SYS, "fadvise64_64") and usize_bits != 64) {
            // The extra usize check is needed to avoid SPARC64 because it provides both

            // fadvise64 and fadvise64_64 but the latter behaves differently than other platforms.

            const offset_halves = splitValue64(offset);
            const length_halves = splitValue64(len);

            return syscall6(
                .fadvise64_64,
                @bitCast(usize, @as(isize, fd)),
                offset_halves[0],
                offset_halves[1],
                length_halves[0],
                length_halves[1],
                advice,
            );
        } else {
            return syscall4(
                .fadvise64,
                @bitCast(usize, @as(isize, fd)),
                @bitCast(usize, offset),
                @bitCast(usize, len),
                advice,
            );
        }
    }

    pub fn perf_event_open(
        attr: *perf_event_attr,
        pid: pid_t,
        cpu: i32,
        group_fd: fd_t,
        flags: usize,
    ) usize {
        return syscall5(
            .perf_event_open,
            @ptrToInt(attr),
            @bitCast(usize, @as(isize, pid)),
            @bitCast(usize, @as(isize, cpu)),
            @bitCast(usize, @as(isize, group_fd)),
            flags,
        );
    }

    pub fn seccomp(operation: u32, flags: u32, args: ?*const anyopaque) usize {
        return syscall3(.seccomp, operation, flags, @ptrToInt(args));
    }

    pub const E = switch (native_arch) {
        .mips, .mipsel => @import("linux/errno/mips.zig").E,
        .sparc, .sparcel, .sparc64 => @import("linux/errno/sparc.zig").E,
        else => @import("linux/errno/generic.zig").E,
    };

    pub const pid_t = i32;
    pub const fd_t = i32;
    pub const uid_t = u32;
    pub const gid_t = u32;
    pub const clock_t = isize;

    pub const NAME_MAX = 255;
    pub const PATH_MAX = 4096;
    pub const IOV_MAX = 1024;

    /// Largest hardware address length
    /// e.g. a mac address is a type of hardware address
    pub const MAX_ADDR_LEN = 32;

    pub const STDIN_FILENO = 0;
    pub const STDOUT_FILENO = 1;
    pub const STDERR_FILENO = 2;

    pub const AT = struct {
        /// Special value used to indicate openat should use the current working directory
        pub const FDCWD = -100;

        /// Do not follow symbolic links
        pub const SYMLINK_NOFOLLOW = 0x100;

        /// Remove directory instead of unlinking file
        pub const REMOVEDIR = 0x200;

        /// Follow symbolic links.
        pub const SYMLINK_FOLLOW = 0x400;

        /// Suppress terminal automount traversal
        pub const NO_AUTOMOUNT = 0x800;

        /// Allow empty relative pathname
        pub const EMPTY_PATH = 0x1000;

        /// Type of synchronisation required from statx()
        pub const STATX_SYNC_TYPE = 0x6000;

        /// - Do whatever stat() does
        pub const STATX_SYNC_AS_STAT = 0x0000;

        /// - Force the attributes to be sync'd with the server
        pub const STATX_FORCE_SYNC = 0x2000;

        /// - Don't sync attributes with the server
        pub const STATX_DONT_SYNC = 0x4000;

        /// Apply to the entire subtree
        pub const RECURSIVE = 0x8000;
    };

    pub const FALLOC = struct {
        /// Default is extend size
        pub const FL_KEEP_SIZE = 0x01;

        /// De-allocates range
        pub const FL_PUNCH_HOLE = 0x02;

        /// Reserved codepoint
        pub const FL_NO_HIDE_STALE = 0x04;

        /// Removes a range of a file without leaving a hole in the file
        pub const FL_COLLAPSE_RANGE = 0x08;

        /// Converts a range of file to zeros preferably without issuing data IO
        pub const FL_ZERO_RANGE = 0x10;

        /// Inserts space within the file size without overwriting any existing data
        pub const FL_INSERT_RANGE = 0x20;

        /// Unshares shared blocks within the file size without overwriting any existing data
        pub const FL_UNSHARE_RANGE = 0x40;
    };

    pub const FUTEX = struct {
        pub const WAIT = 0;
        pub const WAKE = 1;
        pub const FD = 2;
        pub const REQUEUE = 3;
        pub const CMP_REQUEUE = 4;
        pub const WAKE_OP = 5;
        pub const LOCK_PI = 6;
        pub const UNLOCK_PI = 7;
        pub const TRYLOCK_PI = 8;
        pub const WAIT_BITSET = 9;
        pub const WAKE_BITSET = 10;
        pub const WAIT_REQUEUE_PI = 11;
        pub const CMP_REQUEUE_PI = 12;

        pub const PRIVATE_FLAG = 128;

        pub const CLOCK_REALTIME = 256;
    };

    pub const PROT = struct {
        /// page can not be accessed
        pub const NONE = 0x0;
        /// page can be read
        pub const READ = 0x1;
        /// page can be written
        pub const WRITE = 0x2;
        /// page can be executed
        pub const EXEC = 0x4;
        /// page may be used for atomic ops
        pub const SEM = switch (native_arch) {
            // TODO: also xtensa

            .mips, .mipsel, .mips64, .mips64el => 0x10,
            else => 0x8,
        };
        /// mprotect flag: extend change to start of growsdown vma
        pub const GROWSDOWN = 0x01000000;
        /// mprotect flag: extend change to end of growsup vma
        pub const GROWSUP = 0x02000000;
    };

    pub const FD_CLOEXEC = 1;

    pub const F_OK = 0;
    pub const X_OK = 1;
    pub const W_OK = 2;
    pub const R_OK = 4;

    pub const W = struct {
        pub const NOHANG = 1;
        pub const UNTRACED = 2;
        pub const STOPPED = 2;
        pub const EXITED = 4;
        pub const CONTINUED = 8;
        pub const NOWAIT = 0x1000000;

        pub fn EXITSTATUS(s: u32) u8 {
            return @intCast(u8, (s & 0xff00) >> 8);
        }
        pub fn TERMSIG(s: u32) u32 {
            return s & 0x7f;
        }
        pub fn STOPSIG(s: u32) u32 {
            return EXITSTATUS(s);
        }
        pub fn IFEXITED(s: u32) bool {
            return TERMSIG(s) == 0;
        }
        pub fn IFSTOPPED(s: u32) bool {
            return @truncate(u16, ((s & 0xffff) *% 0x10001) >> 8) > 0x7f00;
        }
        pub fn IFSIGNALED(s: u32) bool {
            return (s & 0xffff) -% 1 < 0xff;
        }
    };

    // waitid id types

    pub const P = enum(c_uint) {
        ALL = 0,
        PID = 1,
        PGID = 2,
        PIDFD = 3,
        _,
    };

    pub const SA = if (is_mips) struct {
        pub const NOCLDSTOP = 1;
        pub const NOCLDWAIT = 0x10000;
        pub const SIGINFO = 8;
        pub const RESTART = 0x10000000;
        pub const RESETHAND = 0x80000000;
        pub const ONSTACK = 0x08000000;
        pub const NODEFER = 0x40000000;
        pub const RESTORER = 0x04000000;
    } else if (is_sparc) struct {
        pub const NOCLDSTOP = 0x8;
        pub const NOCLDWAIT = 0x100;
        pub const SIGINFO = 0x200;
        pub const RESTART = 0x2;
        pub const RESETHAND = 0x4;
        pub const ONSTACK = 0x1;
        pub const NODEFER = 0x20;
        pub const RESTORER = 0x04000000;
    } else struct {
        pub const NOCLDSTOP = 1;
        pub const NOCLDWAIT = 2;
        pub const SIGINFO = 4;
        pub const RESTART = 0x10000000;
        pub const RESETHAND = 0x80000000;
        pub const ONSTACK = 0x08000000;
        pub const NODEFER = 0x40000000;
        pub const RESTORER = 0x04000000;
    };

    pub const SIG = if (is_mips) struct {
        pub const BLOCK = 1;
        pub const UNBLOCK = 2;
        pub const SETMASK = 3;

        pub const HUP = 1;
        pub const INT = 2;
        pub const QUIT = 3;
        pub const ILL = 4;
        pub const TRAP = 5;
        pub const ABRT = 6;
        pub const IOT = ABRT;
        pub const BUS = 7;
        pub const FPE = 8;
        pub const KILL = 9;
        pub const USR1 = 10;
        pub const SEGV = 11;
        pub const USR2 = 12;
        pub const PIPE = 13;
        pub const ALRM = 14;
        pub const TERM = 15;
        pub const STKFLT = 16;
        pub const CHLD = 17;
        pub const CONT = 18;
        pub const STOP = 19;
        pub const TSTP = 20;
        pub const TTIN = 21;
        pub const TTOU = 22;
        pub const URG = 23;
        pub const XCPU = 24;
        pub const XFSZ = 25;
        pub const VTALRM = 26;
        pub const PROF = 27;
        pub const WINCH = 28;
        pub const IO = 29;
        pub const POLL = 29;
        pub const PWR = 30;
        pub const SYS = 31;
        pub const UNUSED = SIG.SYS;

        pub const ERR = @intToPtr(?Sigaction.handler_fn, maxInt(usize));
        pub const DFL = @intToPtr(?Sigaction.handler_fn, 0);
        pub const IGN = @intToPtr(?Sigaction.handler_fn, 1);
    } else if (is_sparc) struct {
        pub const BLOCK = 1;
        pub const UNBLOCK = 2;
        pub const SETMASK = 4;

        pub const HUP = 1;
        pub const INT = 2;
        pub const QUIT = 3;
        pub const ILL = 4;
        pub const TRAP = 5;
        pub const ABRT = 6;
        pub const EMT = 7;
        pub const FPE = 8;
        pub const KILL = 9;
        pub const BUS = 10;
        pub const SEGV = 11;
        pub const SYS = 12;
        pub const PIPE = 13;
        pub const ALRM = 14;
        pub const TERM = 15;
        pub const URG = 16;
        pub const STOP = 17;
        pub const TSTP = 18;
        pub const CONT = 19;
        pub const CHLD = 20;
        pub const TTIN = 21;
        pub const TTOU = 22;
        pub const POLL = 23;
        pub const XCPU = 24;
        pub const XFSZ = 25;
        pub const VTALRM = 26;
        pub const PROF = 27;
        pub const WINCH = 28;
        pub const LOST = 29;
        pub const USR1 = 30;
        pub const USR2 = 31;
        pub const IOT = ABRT;
        pub const CLD = CHLD;
        pub const PWR = LOST;
        pub const IO = SIG.POLL;

        pub const ERR = @intToPtr(?Sigaction.handler_fn, maxInt(usize));
        pub const DFL = @intToPtr(?Sigaction.handler_fn, 0);
        pub const IGN = @intToPtr(?Sigaction.handler_fn, 1);
    } else struct {
        pub const BLOCK = 0;
        pub const UNBLOCK = 1;
        pub const SETMASK = 2;

        pub const HUP = 1;
        pub const INT = 2;
        pub const QUIT = 3;
        pub const ILL = 4;
        pub const TRAP = 5;
        pub const ABRT = 6;
        pub const IOT = ABRT;
        pub const BUS = 7;
        pub const FPE = 8;
        pub const KILL = 9;
        pub const USR1 = 10;
        pub const SEGV = 11;
        pub const USR2 = 12;
        pub const PIPE = 13;
        pub const ALRM = 14;
        pub const TERM = 15;
        pub const STKFLT = 16;
        pub const CHLD = 17;
        pub const CONT = 18;
        pub const STOP = 19;
        pub const TSTP = 20;
        pub const TTIN = 21;
        pub const TTOU = 22;
        pub const URG = 23;
        pub const XCPU = 24;
        pub const XFSZ = 25;
        pub const VTALRM = 26;
        pub const PROF = 27;
        pub const WINCH = 28;
        pub const IO = 29;
        pub const POLL = 29;
        pub const PWR = 30;
        pub const SYS = 31;
        pub const UNUSED = SIG.SYS;

        pub const ERR = @intToPtr(?Sigaction.handler_fn, maxInt(usize));
        pub const DFL = @intToPtr(?Sigaction.handler_fn, 0);
        pub const IGN = @intToPtr(?Sigaction.handler_fn, 1);
    };

    pub const kernel_rwf = u32;

    pub const RWF = struct {
        /// high priority request, poll if possible
        pub const HIPRI: kernel_rwf = 0x00000001;

        /// per-IO O.DSYNC
        pub const DSYNC: kernel_rwf = 0x00000002;

        /// per-IO O.SYNC
        pub const SYNC: kernel_rwf = 0x00000004;

        /// per-IO, return -EAGAIN if operation would block
        pub const NOWAIT: kernel_rwf = 0x00000008;

        /// per-IO O.APPEND
        pub const APPEND: kernel_rwf = 0x00000010;
    };

    pub const SEEK = struct {
        pub const SET = 0;
        pub const CUR = 1;
        pub const END = 2;
    };

    pub const SHUT = struct {
        pub const RD = 0;
        pub const WR = 1;
        pub const RDWR = 2;
    };

    pub const SOCK = struct {
        pub const STREAM = if (is_mips) 2 else 1;
        pub const DGRAM = if (is_mips) 1 else 2;
        pub const RAW = 3;
        pub const RDM = 4;
        pub const SEQPACKET = 5;
        pub const DCCP = 6;
        pub const PACKET = 10;
        pub const CLOEXEC = if (is_sparc) 0o20000000 else 0o2000000;
        pub const NONBLOCK = if (is_mips) 0o200 else if (is_sparc) 0o40000 else 0o4000;
    };

    pub const TCP = struct {
        /// Turn off Nagle's algorithm
        pub const NODELAY = 1;
        /// Limit MSS
        pub const MAXSEG = 2;
        /// Never send partially complete segments.
        pub const CORK = 3;
        /// Start keeplives after this period, in seconds
        pub const KEEPIDLE = 4;
        /// Interval between keepalives
        pub const KEEPINTVL = 5;
        /// Number of keepalives before death
        pub const KEEPCNT = 6;
        /// Number of SYN retransmits
        pub const SYNCNT = 7;
        /// Life time of orphaned FIN-WAIT-2 state
        pub const LINGER2 = 8;
        /// Wake up listener only when data arrive
        pub const DEFER_ACCEPT = 9;
        /// Bound advertised window
        pub const WINDOW_CLAMP = 10;
        /// Information about this connection.
        pub const INFO = 11;
        /// Block/reenable quick acks
        pub const QUICKACK = 12;
        /// Congestion control algorithm
        pub const CONGESTION = 13;
        /// TCP MD5 Signature (RFC2385)
        pub const MD5SIG = 14;
        /// Use linear timeouts for thin streams
        pub const THIN_LINEAR_TIMEOUTS = 16;
        /// Fast retrans. after 1 dupack
        pub const THIN_DUPACK = 17;
        /// How long for loss retry before timeout
        pub const USER_TIMEOUT = 18;
        /// TCP sock is under repair right now
        pub const REPAIR = 19;
        pub const REPAIR_QUEUE = 20;
        pub const QUEUE_SEQ = 21;
        pub const REPAIR_OPTIONS = 22;
        /// Enable FastOpen on listeners
        pub const FASTOPEN = 23;
        pub const TIMESTAMP = 24;
        /// limit number of unsent bytes in write queue
        pub const NOTSENT_LOWAT = 25;
        /// Get Congestion Control (optional) info
        pub const CC_INFO = 26;
        /// Record SYN headers for new connections
        pub const SAVE_SYN = 27;
        /// Get SYN headers recorded for connection
        pub const SAVED_SYN = 28;
        /// Get/set window parameters
        pub const REPAIR_WINDOW = 29;
        /// Attempt FastOpen with connect
        pub const FASTOPEN_CONNECT = 30;
        /// Attach a ULP to a TCP connection
        pub const ULP = 31;
        /// TCP MD5 Signature with extensions
        pub const MD5SIG_EXT = 32;
        /// Set the key for Fast Open (cookie)
        pub const FASTOPEN_KEY = 33;
        /// Enable TFO without a TFO cookie
        pub const FASTOPEN_NO_COOKIE = 34;
        pub const ZEROCOPY_RECEIVE = 35;
        /// Notify bytes available to read as a cmsg on read
        pub const INQ = 36;
        pub const CM_INQ = INQ;
        /// delay outgoing packets by XX usec
        pub const TX_DELAY = 37;

        pub const REPAIR_ON = 1;
        pub const REPAIR_OFF = 0;
        /// Turn off without window probes
        pub const REPAIR_OFF_NO_WP = -1;
    };

    pub const PF = struct {
        pub const UNSPEC = 0;
        pub const LOCAL = 1;
        pub const UNIX = LOCAL;
        pub const FILE = LOCAL;
        pub const INET = 2;
        pub const AX25 = 3;
        pub const IPX = 4;
        pub const APPLETALK = 5;
        pub const NETROM = 6;
        pub const BRIDGE = 7;
        pub const ATMPVC = 8;
        pub const X25 = 9;
        pub const INET6 = 10;
        pub const ROSE = 11;
        pub const DECnet = 12;
        pub const NETBEUI = 13;
        pub const SECURITY = 14;
        pub const KEY = 15;
        pub const NETLINK = 16;
        pub const ROUTE = PF.NETLINK;
        pub const PACKET = 17;
        pub const ASH = 18;
        pub const ECONET = 19;
        pub const ATMSVC = 20;
        pub const RDS = 21;
        pub const SNA = 22;
        pub const IRDA = 23;
        pub const PPPOX = 24;
        pub const WANPIPE = 25;
        pub const LLC = 26;
        pub const IB = 27;
        pub const MPLS = 28;
        pub const CAN = 29;
        pub const TIPC = 30;
        pub const BLUETOOTH = 31;
        pub const IUCV = 32;
        pub const RXRPC = 33;
        pub const ISDN = 34;
        pub const PHONET = 35;
        pub const IEEE802154 = 36;
        pub const CAIF = 37;
        pub const ALG = 38;
        pub const NFC = 39;
        pub const VSOCK = 40;
        pub const KCM = 41;
        pub const QIPCRTR = 42;
        pub const SMC = 43;
        pub const XDP = 44;
        pub const MAX = 45;
    };

    pub const AF = struct {
        pub const UNSPEC = PF.UNSPEC;
        pub const LOCAL = PF.LOCAL;
        pub const UNIX = AF.LOCAL;
        pub const FILE = AF.LOCAL;
        pub const INET = PF.INET;
        pub const AX25 = PF.AX25;
        pub const IPX = PF.IPX;
        pub const APPLETALK = PF.APPLETALK;
        pub const NETROM = PF.NETROM;
        pub const BRIDGE = PF.BRIDGE;
        pub const ATMPVC = PF.ATMPVC;
        pub const X25 = PF.X25;
        pub const INET6 = PF.INET6;
        pub const ROSE = PF.ROSE;
        pub const DECnet = PF.DECnet;
        pub const NETBEUI = PF.NETBEUI;
        pub const SECURITY = PF.SECURITY;
        pub const KEY = PF.KEY;
        pub const NETLINK = PF.NETLINK;
        pub const ROUTE = PF.ROUTE;
        pub const PACKET = PF.PACKET;
        pub const ASH = PF.ASH;
        pub const ECONET = PF.ECONET;
        pub const ATMSVC = PF.ATMSVC;
        pub const RDS = PF.RDS;
        pub const SNA = PF.SNA;
        pub const IRDA = PF.IRDA;
        pub const PPPOX = PF.PPPOX;
        pub const WANPIPE = PF.WANPIPE;
        pub const LLC = PF.LLC;
        pub const IB = PF.IB;
        pub const MPLS = PF.MPLS;
        pub const CAN = PF.CAN;
        pub const TIPC = PF.TIPC;
        pub const BLUETOOTH = PF.BLUETOOTH;
        pub const IUCV = PF.IUCV;
        pub const RXRPC = PF.RXRPC;
        pub const ISDN = PF.ISDN;
        pub const PHONET = PF.PHONET;
        pub const IEEE802154 = PF.IEEE802154;
        pub const CAIF = PF.CAIF;
        pub const ALG = PF.ALG;
        pub const NFC = PF.NFC;
        pub const VSOCK = PF.VSOCK;
        pub const KCM = PF.KCM;
        pub const QIPCRTR = PF.QIPCRTR;
        pub const SMC = PF.SMC;
        pub const XDP = PF.XDP;
        pub const MAX = PF.MAX;
    };

    pub const SO = struct {
        pub usingnamespace if (is_mips) struct {
            pub const DEBUG = 1;
            pub const REUSEADDR = 0x0004;
            pub const KEEPALIVE = 0x0008;
            pub const DONTROUTE = 0x0010;
            pub const BROADCAST = 0x0020;
            pub const LINGER = 0x0080;
            pub const OOBINLINE = 0x0100;
            pub const REUSEPORT = 0x0200;
            pub const SNDBUF = 0x1001;
            pub const RCVBUF = 0x1002;
            pub const SNDLOWAT = 0x1003;
            pub const RCVLOWAT = 0x1004;
            pub const RCVTIMEO = 0x1006;
            pub const SNDTIMEO = 0x1005;
            pub const ERROR = 0x1007;
            pub const TYPE = 0x1008;
            pub const ACCEPTCONN = 0x1009;
            pub const PROTOCOL = 0x1028;
            pub const DOMAIN = 0x1029;
            pub const NO_CHECK = 11;
            pub const PRIORITY = 12;
            pub const BSDCOMPAT = 14;
            pub const PASSCRED = 17;
            pub const PEERCRED = 18;
            pub const PEERSEC = 30;
            pub const SNDBUFFORCE = 31;
            pub const RCVBUFFORCE = 33;
            pub const SECURITY_AUTHENTICATION = 22;
            pub const SECURITY_ENCRYPTION_TRANSPORT = 23;
            pub const SECURITY_ENCRYPTION_NETWORK = 24;
            pub const BINDTODEVICE = 25;
            pub const ATTACH_FILTER = 26;
            pub const DETACH_FILTER = 27;
            pub const GET_FILTER = ATTACH_FILTER;
            pub const PEERNAME = 28;
            pub const TIMESTAMP_OLD = 29;
            pub const PASSSEC = 34;
            pub const TIMESTAMPNS_OLD = 35;
            pub const MARK = 36;
            pub const TIMESTAMPING_OLD = 37;
            pub const RXQ_OVFL = 40;
            pub const WIFI_STATUS = 41;
            pub const PEEK_OFF = 42;
            pub const NOFCS = 43;
            pub const LOCK_FILTER = 44;
            pub const SELECT_ERR_QUEUE = 45;
            pub const BUSY_POLL = 46;
            pub const MAX_PACING_RATE = 47;
            pub const BPF_EXTENSIONS = 48;
            pub const INCOMING_CPU = 49;
            pub const ATTACH_BPF = 50;
            pub const DETACH_BPF = DETACH_FILTER;
            pub const ATTACH_REUSEPORT_CBPF = 51;
            pub const ATTACH_REUSEPORT_EBPF = 52;
            pub const CNX_ADVICE = 53;
            pub const MEMINFO = 55;
            pub const INCOMING_NAPI_ID = 56;
            pub const COOKIE = 57;
            pub const PEERGROUPS = 59;
            pub const ZEROCOPY = 60;
            pub const TXTIME = 61;
            pub const BINDTOIFINDEX = 62;
            pub const TIMESTAMP_NEW = 63;
            pub const TIMESTAMPNS_NEW = 64;
            pub const TIMESTAMPING_NEW = 65;
            pub const RCVTIMEO_NEW = 66;
            pub const SNDTIMEO_NEW = 67;
            pub const DETACH_REUSEPORT_BPF = 68;
        } else if (is_ppc or is_ppc64) struct {
            pub const DEBUG = 1;
            pub const REUSEADDR = 2;
            pub const TYPE = 3;
            pub const ERROR = 4;
            pub const DONTROUTE = 5;
            pub const BROADCAST = 6;
            pub const SNDBUF = 7;
            pub const RCVBUF = 8;
            pub const KEEPALIVE = 9;
            pub const OOBINLINE = 10;
            pub const NO_CHECK = 11;
            pub const PRIORITY = 12;
            pub const LINGER = 13;
            pub const BSDCOMPAT = 14;
            pub const REUSEPORT = 15;
            pub const RCVLOWAT = 16;
            pub const SNDLOWAT = 17;
            pub const RCVTIMEO = 18;
            pub const SNDTIMEO = 19;
            pub const PASSCRED = 20;
            pub const PEERCRED = 21;
            pub const ACCEPTCONN = 30;
            pub const PEERSEC = 31;
            pub const SNDBUFFORCE = 32;
            pub const RCVBUFFORCE = 33;
            pub const PROTOCOL = 38;
            pub const DOMAIN = 39;
            pub const SECURITY_AUTHENTICATION = 22;
            pub const SECURITY_ENCRYPTION_TRANSPORT = 23;
            pub const SECURITY_ENCRYPTION_NETWORK = 24;
            pub const BINDTODEVICE = 25;
            pub const ATTACH_FILTER = 26;
            pub const DETACH_FILTER = 27;
            pub const GET_FILTER = ATTACH_FILTER;
            pub const PEERNAME = 28;
            pub const TIMESTAMP_OLD = 29;
            pub const PASSSEC = 34;
            pub const TIMESTAMPNS_OLD = 35;
            pub const MARK = 36;
            pub const TIMESTAMPING_OLD = 37;
            pub const RXQ_OVFL = 40;
            pub const WIFI_STATUS = 41;
            pub const PEEK_OFF = 42;
            pub const NOFCS = 43;
            pub const LOCK_FILTER = 44;
            pub const SELECT_ERR_QUEUE = 45;
            pub const BUSY_POLL = 46;
            pub const MAX_PACING_RATE = 47;
            pub const BPF_EXTENSIONS = 48;
            pub const INCOMING_CPU = 49;
            pub const ATTACH_BPF = 50;
            pub const DETACH_BPF = DETACH_FILTER;
            pub const ATTACH_REUSEPORT_CBPF = 51;
            pub const ATTACH_REUSEPORT_EBPF = 52;
            pub const CNX_ADVICE = 53;
            pub const MEMINFO = 55;
            pub const INCOMING_NAPI_ID = 56;
            pub const COOKIE = 57;
            pub const PEERGROUPS = 59;
            pub const ZEROCOPY = 60;
            pub const TXTIME = 61;
            pub const BINDTOIFINDEX = 62;
            pub const TIMESTAMP_NEW = 63;
            pub const TIMESTAMPNS_NEW = 64;
            pub const TIMESTAMPING_NEW = 65;
            pub const RCVTIMEO_NEW = 66;
            pub const SNDTIMEO_NEW = 67;
            pub const DETACH_REUSEPORT_BPF = 68;
        } else if (is_sparc) struct {
            pub const DEBUG = 1;
            pub const REUSEADDR = 4;
            pub const TYPE = 4104;
            pub const ERROR = 4103;
            pub const DONTROUTE = 16;
            pub const BROADCAST = 32;
            pub const SNDBUF = 4097;
            pub const RCVBUF = 4098;
            pub const KEEPALIVE = 8;
            pub const OOBINLINE = 256;
            pub const NO_CHECK = 11;
            pub const PRIORITY = 12;
            pub const LINGER = 128;
            pub const BSDCOMPAT = 1024;
            pub const REUSEPORT = 512;
            pub const PASSCRED = 2;
            pub const PEERCRED = 64;
            pub const RCVLOWAT = 2048;
            pub const SNDLOWAT = 4096;
            pub const RCVTIMEO = 8192;
            pub const SNDTIMEO = 16384;
            pub const ACCEPTCONN = 32768;
            pub const PEERSEC = 30;
            pub const SNDBUFFORCE = 4106;
            pub const RCVBUFFORCE = 4107;
            pub const PROTOCOL = 4136;
            pub const DOMAIN = 4137;
            pub const SECURITY_AUTHENTICATION = 20481;
            pub const SECURITY_ENCRYPTION_TRANSPORT = 20482;
            pub const SECURITY_ENCRYPTION_NETWORK = 20484;
            pub const BINDTODEVICE = 13;
            pub const ATTACH_FILTER = 26;
            pub const DETACH_FILTER = 27;
            pub const GET_FILTER = 26;
            pub const PEERNAME = 28;
            pub const TIMESTAMP_OLD = 29;
            pub const PASSSEC = 31;
            pub const TIMESTAMPNS_OLD = 33;
            pub const MARK = 34;
            pub const TIMESTAMPING_OLD = 35;
            pub const RXQ_OVFL = 36;
            pub const WIFI_STATUS = 37;
            pub const PEEK_OFF = 38;
            pub const NOFCS = 39;
            pub const LOCK_FILTER = 40;
            pub const SELECT_ERR_QUEUE = 41;
            pub const BUSY_POLL = 48;
            pub const MAX_PACING_RATE = 49;
            pub const BPF_EXTENSIONS = 50;
            pub const INCOMING_CPU = 51;
            pub const ATTACH_BPF = 52;
            pub const DETACH_BPF = 27;
            pub const ATTACH_REUSEPORT_CBPF = 53;
            pub const ATTACH_REUSEPORT_EBPF = 54;
            pub const CNX_ADVICE = 55;
            pub const MEMINFO = 57;
            pub const INCOMING_NAPI_ID = 58;
            pub const COOKIE = 59;
            pub const PEERGROUPS = 61;
            pub const ZEROCOPY = 62;
            pub const TXTIME = 63;
            pub const BINDTOIFINDEX = 65;
            pub const TIMESTAMP_NEW = 70;
            pub const TIMESTAMPNS_NEW = 66;
            pub const TIMESTAMPING_NEW = 67;
            pub const RCVTIMEO_NEW = 68;
            pub const SNDTIMEO_NEW = 69;
            pub const DETACH_REUSEPORT_BPF = 71;
        } else struct {
            pub const DEBUG = 1;
            pub const REUSEADDR = 2;
            pub const TYPE = 3;
            pub const ERROR = 4;
            pub const DONTROUTE = 5;
            pub const BROADCAST = 6;
            pub const SNDBUF = 7;
            pub const RCVBUF = 8;
            pub const KEEPALIVE = 9;
            pub const OOBINLINE = 10;
            pub const NO_CHECK = 11;
            pub const PRIORITY = 12;
            pub const LINGER = 13;
            pub const BSDCOMPAT = 14;
            pub const REUSEPORT = 15;
            pub const PASSCRED = 16;
            pub const PEERCRED = 17;
            pub const RCVLOWAT = 18;
            pub const SNDLOWAT = 19;
            pub const RCVTIMEO = 20;
            pub const SNDTIMEO = 21;
            pub const ACCEPTCONN = 30;
            pub const PEERSEC = 31;
            pub const SNDBUFFORCE = 32;
            pub const RCVBUFFORCE = 33;
            pub const PROTOCOL = 38;
            pub const DOMAIN = 39;
            pub const SECURITY_AUTHENTICATION = 22;
            pub const SECURITY_ENCRYPTION_TRANSPORT = 23;
            pub const SECURITY_ENCRYPTION_NETWORK = 24;
            pub const BINDTODEVICE = 25;
            pub const ATTACH_FILTER = 26;
            pub const DETACH_FILTER = 27;
            pub const GET_FILTER = ATTACH_FILTER;
            pub const PEERNAME = 28;
            pub const TIMESTAMP_OLD = 29;
            pub const PASSSEC = 34;
            pub const TIMESTAMPNS_OLD = 35;
            pub const MARK = 36;
            pub const TIMESTAMPING_OLD = 37;
            pub const RXQ_OVFL = 40;
            pub const WIFI_STATUS = 41;
            pub const PEEK_OFF = 42;
            pub const NOFCS = 43;
            pub const LOCK_FILTER = 44;
            pub const SELECT_ERR_QUEUE = 45;
            pub const BUSY_POLL = 46;
            pub const MAX_PACING_RATE = 47;
            pub const BPF_EXTENSIONS = 48;
            pub const INCOMING_CPU = 49;
            pub const ATTACH_BPF = 50;
            pub const DETACH_BPF = DETACH_FILTER;
            pub const ATTACH_REUSEPORT_CBPF = 51;
            pub const ATTACH_REUSEPORT_EBPF = 52;
            pub const CNX_ADVICE = 53;
            pub const MEMINFO = 55;
            pub const INCOMING_NAPI_ID = 56;
            pub const COOKIE = 57;
            pub const PEERGROUPS = 59;
            pub const ZEROCOPY = 60;
            pub const TXTIME = 61;
            pub const BINDTOIFINDEX = 62;
            pub const TIMESTAMP_NEW = 63;
            pub const TIMESTAMPNS_NEW = 64;
            pub const TIMESTAMPING_NEW = 65;
            pub const RCVTIMEO_NEW = 66;
            pub const SNDTIMEO_NEW = 67;
            pub const DETACH_REUSEPORT_BPF = 68;
        };
    };

    pub const SCM = struct {
        pub const WIFI_STATUS = SO.WIFI_STATUS;
        pub const TIMESTAMPING_OPT_STATS = 54;
        pub const TIMESTAMPING_PKTINFO = 58;
        pub const TXTIME = SO.TXTIME;
    };

    pub const SOL = struct {
        pub const SOCKET = if (is_mips or is_sparc) 65535 else 1;

        pub const IP = 0;
        pub const IPV6 = 41;
        pub const ICMPV6 = 58;

        pub const RAW = 255;
        pub const DECNET = 261;
        pub const X25 = 262;
        pub const PACKET = 263;
        pub const ATM = 264;
        pub const AAL = 265;
        pub const IRDA = 266;
        pub const NETBEUI = 267;
        pub const LLC = 268;
        pub const DCCP = 269;
        pub const NETLINK = 270;
        pub const TIPC = 271;
        pub const RXRPC = 272;
        pub const PPPOL2TP = 273;
        pub const BLUETOOTH = 274;
        pub const PNPIPE = 275;
        pub const RDS = 276;
        pub const IUCV = 277;
        pub const CAIF = 278;
        pub const ALG = 279;
        pub const NFC = 280;
        pub const KCM = 281;
        pub const TLS = 282;
        pub const XDP = 283;
    };

    pub const SOMAXCONN = 128;

    pub const IP = struct {
        pub const TOS = 1;
        pub const TTL = 2;
        pub const HDRINCL = 3;
        pub const OPTIONS = 4;
        pub const ROUTER_ALERT = 5;
        pub const RECVOPTS = 6;
        pub const RETOPTS = 7;
        pub const PKTINFO = 8;
        pub const PKTOPTIONS = 9;
        pub const PMTUDISC = 10;
        pub const MTU_DISCOVER = 10;
        pub const RECVERR = 11;
        pub const RECVTTL = 12;
        pub const RECVTOS = 13;
        pub const MTU = 14;
        pub const FREEBIND = 15;
        pub const IPSEC_POLICY = 16;
        pub const XFRM_POLICY = 17;
        pub const PASSSEC = 18;
        pub const TRANSPARENT = 19;
        pub const ORIGDSTADDR = 20;
        pub const RECVORIGDSTADDR = IP.ORIGDSTADDR;
        pub const MINTTL = 21;
        pub const NODEFRAG = 22;
        pub const CHECKSUM = 23;
        pub const BIND_ADDRESS_NO_PORT = 24;
        pub const RECVFRAGSIZE = 25;
        pub const MULTICAST_IF = 32;
        pub const MULTICAST_TTL = 33;
        pub const MULTICAST_LOOP = 34;
        pub const ADD_MEMBERSHIP = 35;
        pub const DROP_MEMBERSHIP = 36;
        pub const UNBLOCK_SOURCE = 37;
        pub const BLOCK_SOURCE = 38;
        pub const ADD_SOURCE_MEMBERSHIP = 39;
        pub const DROP_SOURCE_MEMBERSHIP = 40;
        pub const MSFILTER = 41;
        pub const MULTICAST_ALL = 49;
        pub const UNICAST_IF = 50;

        pub const RECVRETOPTS = IP.RETOPTS;

        pub const PMTUDISC_DONT = 0;
        pub const PMTUDISC_WANT = 1;
        pub const PMTUDISC_DO = 2;
        pub const PMTUDISC_PROBE = 3;
        pub const PMTUDISC_INTERFACE = 4;
        pub const PMTUDISC_OMIT = 5;

        pub const DEFAULT_MULTICAST_TTL = 1;
        pub const DEFAULT_MULTICAST_LOOP = 1;
        pub const MAX_MEMBERSHIPS = 20;
    };

    /// IPv6 socket options
    pub const IPV6 = struct {
        pub const ADDRFORM = 1;
        pub const @"2292PKTINFO" = 2;
        pub const @"2292HOPOPTS" = 3;
        pub const @"2292DSTOPTS" = 4;
        pub const @"2292RTHDR" = 5;
        pub const @"2292PKTOPTIONS" = 6;
        pub const CHECKSUM = 7;
        pub const @"2292HOPLIMIT" = 8;
        pub const NEXTHOP = 9;
        pub const AUTHHDR = 10;
        pub const FLOWINFO = 11;

        pub const UNICAST_HOPS = 16;
        pub const MULTICAST_IF = 17;
        pub const MULTICAST_HOPS = 18;
        pub const MULTICAST_LOOP = 19;
        pub const ADD_MEMBERSHIP = 20;
        pub const DROP_MEMBERSHIP = 21;
        pub const ROUTER_ALERT = 22;
        pub const MTU_DISCOVER = 23;
        pub const MTU = 24;
        pub const RECVERR = 25;
        pub const V6ONLY = 26;
        pub const JOIN_ANYCAST = 27;
        pub const LEAVE_ANYCAST = 28;

        // IPV6.MTU_DISCOVER values

        pub const PMTUDISC_DONT = 0;
        pub const PMTUDISC_WANT = 1;
        pub const PMTUDISC_DO = 2;
        pub const PMTUDISC_PROBE = 3;
        pub const PMTUDISC_INTERFACE = 4;
        pub const PMTUDISC_OMIT = 5;

        // Flowlabel

        pub const FLOWLABEL_MGR = 32;
        pub const FLOWINFO_SEND = 33;
        pub const IPSEC_POLICY = 34;
        pub const XFRM_POLICY = 35;
        pub const HDRINCL = 36;

        // Advanced API (RFC3542) (1)

        pub const RECVPKTINFO = 49;
        pub const PKTINFO = 50;
        pub const RECVHOPLIMIT = 51;
        pub const HOPLIMIT = 52;
        pub const RECVHOPOPTS = 53;
        pub const HOPOPTS = 54;
        pub const RTHDRDSTOPTS = 55;
        pub const RECVRTHDR = 56;
        pub const RTHDR = 57;
        pub const RECVDSTOPTS = 58;
        pub const DSTOPTS = 59;
        pub const RECVPATHMTU = 60;
        pub const PATHMTU = 61;
        pub const DONTFRAG = 62;

        // Advanced API (RFC3542) (2)

        pub const RECVTCLASS = 66;
        pub const TCLASS = 67;

        pub const AUTOFLOWLABEL = 70;

        // RFC5014: Source address selection

        pub const ADDR_PREFERENCES = 72;

        pub const PREFER_SRC_TMP = 0x0001;
        pub const PREFER_SRC_PUBLIC = 0x0002;
        pub const PREFER_SRC_PUBTMP_DEFAULT = 0x0100;
        pub const PREFER_SRC_COA = 0x0004;
        pub const PREFER_SRC_HOME = 0x0400;
        pub const PREFER_SRC_CGA = 0x0008;
        pub const PREFER_SRC_NONCGA = 0x0800;

        // RFC5082: Generalized Ttl Security Mechanism

        pub const MINHOPCOUNT = 73;

        pub const ORIGDSTADDR = 74;
        pub const RECVORIGDSTADDR = IPV6.ORIGDSTADDR;
        pub const TRANSPARENT = 75;
        pub const UNICAST_IF = 76;
        pub const RECVFRAGSIZE = 77;
        pub const FREEBIND = 78;
    };

    pub const MSG = struct {
        pub const OOB = 0x0001;
        pub const PEEK = 0x0002;
        pub const DONTROUTE = 0x0004;
        pub const CTRUNC = 0x0008;
        pub const PROXY = 0x0010;
        pub const TRUNC = 0x0020;
        pub const DONTWAIT = 0x0040;
        pub const EOR = 0x0080;
        pub const WAITALL = 0x0100;
        pub const FIN = 0x0200;
        pub const SYN = 0x0400;
        pub const CONFIRM = 0x0800;
        pub const RST = 0x1000;
        pub const ERRQUEUE = 0x2000;
        pub const NOSIGNAL = 0x4000;
        pub const MORE = 0x8000;
        pub const WAITFORONE = 0x10000;
        pub const BATCH = 0x40000;
        pub const ZEROCOPY = 0x4000000;
        pub const FASTOPEN = 0x20000000;
        pub const CMSG_CLOEXEC = 0x40000000;
    };

    pub const DT = struct {
        pub const UNKNOWN = 0;
        pub const FIFO = 1;
        pub const CHR = 2;
        pub const DIR = 4;
        pub const BLK = 6;
        pub const REG = 8;
        pub const LNK = 10;
        pub const SOCK = 12;
        pub const WHT = 14;
    };

    pub const T = struct {
        pub const CGETS = if (is_mips) 0x540D else 0x5401;
        pub const CSETS = 0x5402;
        pub const CSETSW = 0x5403;
        pub const CSETSF = 0x5404;
        pub const CGETA = 0x5405;
        pub const CSETA = 0x5406;
        pub const CSETAW = 0x5407;
        pub const CSETAF = 0x5408;
        pub const CSBRK = 0x5409;
        pub const CXONC = 0x540A;
        pub const CFLSH = 0x540B;
        pub const IOCEXCL = 0x540C;
        pub const IOCNXCL = 0x540D;
        pub const IOCSCTTY = 0x540E;
        pub const IOCGPGRP = 0x540F;
        pub const IOCSPGRP = 0x5410;
        pub const IOCOUTQ = if (is_mips) 0x7472 else 0x5411;
        pub const IOCSTI = 0x5412;
        pub const IOCGWINSZ = if (is_mips or is_ppc64) 0x40087468 else 0x5413;
        pub const IOCSWINSZ = if (is_mips or is_ppc64) 0x80087467 else 0x5414;
        pub const IOCMGET = 0x5415;
        pub const IOCMBIS = 0x5416;
        pub const IOCMBIC = 0x5417;
        pub const IOCMSET = 0x5418;
        pub const IOCGSOFTCAR = 0x5419;
        pub const IOCSSOFTCAR = 0x541A;
        pub const FIONREAD = if (is_mips) 0x467F else 0x541B;
        pub const IOCINQ = FIONREAD;
        pub const IOCLINUX = 0x541C;
        pub const IOCCONS = 0x541D;
        pub const IOCGSERIAL = 0x541E;
        pub const IOCSSERIAL = 0x541F;
        pub const IOCPKT = 0x5420;
        pub const FIONBIO = 0x5421;
        pub const IOCNOTTY = 0x5422;
        pub const IOCSETD = 0x5423;
        pub const IOCGETD = 0x5424;
        pub const CSBRKP = 0x5425;
        pub const IOCSBRK = 0x5427;
        pub const IOCCBRK = 0x5428;
        pub const IOCGSID = 0x5429;
        pub const IOCGRS485 = 0x542E;
        pub const IOCSRS485 = 0x542F;
        pub const IOCGPTN = IOCTL.IOR('T', 0x30, c_uint);
        pub const IOCSPTLCK = IOCTL.IOW('T', 0x31, c_int);
        pub const IOCGDEV = IOCTL.IOR('T', 0x32, c_uint);
        pub const CGETX = 0x5432;
        pub const CSETX = 0x5433;
        pub const CSETXF = 0x5434;
        pub const CSETXW = 0x5435;
        pub const IOCSIG = IOCTL.IOW('T', 0x36, c_int);
        pub const IOCVHANGUP = 0x5437;
        pub const IOCGPKT = IOCTL.IOR('T', 0x38, c_int);
        pub const IOCGPTLCK = IOCTL.IOR('T', 0x39, c_int);
        pub const IOCGEXCL = IOCTL.IOR('T', 0x40, c_int);
    };

    pub const EPOLL = struct {
        pub const CLOEXEC = O.CLOEXEC;

        pub const CTL_ADD = 1;
        pub const CTL_DEL = 2;
        pub const CTL_MOD = 3;

        pub const IN = 0x001;
        pub const PRI = 0x002;
        pub const OUT = 0x004;
        pub const RDNORM = 0x040;
        pub const RDBAND = 0x080;
        pub const WRNORM = if (is_mips) 0x004 else 0x100;
        pub const WRBAND = if (is_mips) 0x100 else 0x200;
        pub const MSG = 0x400;
        pub const ERR = 0x008;
        pub const HUP = 0x010;
        pub const RDHUP = 0x2000;
        pub const EXCLUSIVE = (@as(u32, 1) << 28);
        pub const WAKEUP = (@as(u32, 1) << 29);
        pub const ONESHOT = (@as(u32, 1) << 30);
        pub const ET = (@as(u32, 1) << 31);
    };

    pub const CLOCK = struct {
        pub const REALTIME = 0;
        pub const MONOTONIC = 1;
        pub const PROCESS_CPUTIME_ID = 2;
        pub const THREAD_CPUTIME_ID = 3;
        pub const MONOTONIC_RAW = 4;
        pub const REALTIME_COARSE = 5;
        pub const MONOTONIC_COARSE = 6;
        pub const BOOTTIME = 7;
        pub const REALTIME_ALARM = 8;
        pub const BOOTTIME_ALARM = 9;
        pub const SGI_CYCLE = 10;
        pub const TAI = 11;
    };

    pub const CSIGNAL = 0x000000ff;

    pub const CLONE = struct {
        pub const VM = 0x00000100;
        pub const FS = 0x00000200;
        pub const FILES = 0x00000400;
        pub const SIGHAND = 0x00000800;
        pub const PIDFD = 0x00001000;
        pub const PTRACE = 0x00002000;
        pub const VFORK = 0x00004000;
        pub const PARENT = 0x00008000;
        pub const THREAD = 0x00010000;
        pub const NEWNS = 0x00020000;
        pub const SYSVSEM = 0x00040000;
        pub const SETTLS = 0x00080000;
        pub const PARENT_SETTID = 0x00100000;
        pub const CHILD_CLEARTID = 0x00200000;
        pub const DETACHED = 0x00400000;
        pub const UNTRACED = 0x00800000;
        pub const CHILD_SETTID = 0x01000000;
        pub const NEWCGROUP = 0x02000000;
        pub const NEWUTS = 0x04000000;
        pub const NEWIPC = 0x08000000;
        pub const NEWUSER = 0x10000000;
        pub const NEWPID = 0x20000000;
        pub const NEWNET = 0x40000000;
        pub const IO = 0x80000000;

        // Flags for the clone3() syscall.

        /// Clear any signal handler and reset to SIG_DFL.
        pub const CLEAR_SIGHAND = 0x100000000;
        /// Clone into a specific cgroup given the right permissions.
        pub const INTO_CGROUP = 0x200000000;

        // cloning flags intersect with CSIGNAL so can be used with unshare and clone3 syscalls only.

        /// New time namespace
        pub const NEWTIME = 0x00000080;
    };

    pub const EFD = struct {
        pub const SEMAPHORE = 1;
        pub const CLOEXEC = O.CLOEXEC;
        pub const NONBLOCK = O.NONBLOCK;
    };

    pub const MS = struct {
        pub const RDONLY = 1;
        pub const NOSUID = 2;
        pub const NODEV = 4;
        pub const NOEXEC = 8;
        pub const SYNCHRONOUS = 16;
        pub const REMOUNT = 32;
        pub const MANDLOCK = 64;
        pub const DIRSYNC = 128;
        pub const NOATIME = 1024;
        pub const NODIRATIME = 2048;
        pub const BIND = 4096;
        pub const MOVE = 8192;
        pub const REC = 16384;
        pub const SILENT = 32768;
        pub const POSIXACL = (1 << 16);
        pub const UNBINDABLE = (1 << 17);
        pub const PRIVATE = (1 << 18);
        pub const SLAVE = (1 << 19);
        pub const SHARED = (1 << 20);
        pub const RELATIME = (1 << 21);
        pub const KERNMOUNT = (1 << 22);
        pub const I_VERSION = (1 << 23);
        pub const STRICTATIME = (1 << 24);
        pub const LAZYTIME = (1 << 25);
        pub const NOREMOTELOCK = (1 << 27);
        pub const NOSEC = (1 << 28);
        pub const BORN = (1 << 29);
        pub const ACTIVE = (1 << 30);
        pub const NOUSER = (1 << 31);

        pub const RMT_MASK = (RDONLY | SYNCHRONOUS | MANDLOCK | I_VERSION | LAZYTIME);

        pub const MGC_VAL = 0xc0ed0000;
        pub const MGC_MSK = 0xffff0000;
    };

    pub const MNT = struct {
        pub const FORCE = 1;
        pub const DETACH = 2;
        pub const EXPIRE = 4;
    };

    pub const UMOUNT_NOFOLLOW = 8;

    pub const IN = struct {
        pub const CLOEXEC = O.CLOEXEC;
        pub const NONBLOCK = O.NONBLOCK;

        pub const ACCESS = 0x00000001;
        pub const MODIFY = 0x00000002;
        pub const ATTRIB = 0x00000004;
        pub const CLOSE_WRITE = 0x00000008;
        pub const CLOSE_NOWRITE = 0x00000010;
        pub const CLOSE = CLOSE_WRITE | CLOSE_NOWRITE;
        pub const OPEN = 0x00000020;
        pub const MOVED_FROM = 0x00000040;
        pub const MOVED_TO = 0x00000080;
        pub const MOVE = MOVED_FROM | MOVED_TO;
        pub const CREATE = 0x00000100;
        pub const DELETE = 0x00000200;
        pub const DELETE_SELF = 0x00000400;
        pub const MOVE_SELF = 0x00000800;
        pub const ALL_EVENTS = 0x00000fff;

        pub const UNMOUNT = 0x00002000;
        pub const Q_OVERFLOW = 0x00004000;
        pub const IGNORED = 0x00008000;

        pub const ONLYDIR = 0x01000000;
        pub const DONT_FOLLOW = 0x02000000;
        pub const EXCL_UNLINK = 0x04000000;
        pub const MASK_CREATE = 0x10000000;
        pub const MASK_ADD = 0x20000000;

        pub const ISDIR = 0x40000000;
        pub const ONESHOT = 0x80000000;
    };

    pub const S = struct {
        pub const IFMT = 0o170000;

        pub const IFDIR = 0o040000;
        pub const IFCHR = 0o020000;
        pub const IFBLK = 0o060000;
        pub const IFREG = 0o100000;
        pub const IFIFO = 0o010000;
        pub const IFLNK = 0o120000;
        pub const IFSOCK = 0o140000;

        pub const ISUID = 0o4000;
        pub const ISGID = 0o2000;
        pub const ISVTX = 0o1000;
        pub const IRUSR = 0o400;
        pub const IWUSR = 0o200;
        pub const IXUSR = 0o100;
        pub const IRWXU = 0o700;
        pub const IRGRP = 0o040;
        pub const IWGRP = 0o020;
        pub const IXGRP = 0o010;
        pub const IRWXG = 0o070;
        pub const IROTH = 0o004;
        pub const IWOTH = 0o002;
        pub const IXOTH = 0o001;
        pub const IRWXO = 0o007;

        pub fn ISREG(m: mode_t) bool {
            return m & IFMT == IFREG;
        }

        pub fn ISDIR(m: mode_t) bool {
            return m & IFMT == IFDIR;
        }

        pub fn ISCHR(m: mode_t) bool {
            return m & IFMT == IFCHR;
        }

        pub fn ISBLK(m: mode_t) bool {
            return m & IFMT == IFBLK;
        }

        pub fn ISFIFO(m: mode_t) bool {
            return m & IFMT == IFIFO;
        }

        pub fn ISLNK(m: mode_t) bool {
            return m & IFMT == IFLNK;
        }

        pub fn ISSOCK(m: mode_t) bool {
            return m & IFMT == IFSOCK;
        }
    };

    pub const UTIME = struct {
        pub const NOW = 0x3fffffff;
        pub const OMIT = 0x3ffffffe;
    };

    pub const TFD = struct {
        pub const NONBLOCK = O.NONBLOCK;
        pub const CLOEXEC = O.CLOEXEC;

        pub const TIMER_ABSTIME = 1;
        pub const TIMER_CANCEL_ON_SET = (1 << 1);
    };

    pub const winsize = extern struct {
        ws_row: u16,
        ws_col: u16,
        ws_xpixel: u16,
        ws_ypixel: u16,
    };

    /// NSIG is the total number of signals defined.
    /// As signal numbers are sequential, NSIG is one greater than the largest defined signal number.
    pub const NSIG = if (is_mips) 128 else 65;

    pub const sigset_t = [1024 / 32]u32;

    pub const all_mask: sigset_t = [_]u32{0xffffffff} ** @typeInfo(sigset_t).Array.len;
    pub const app_mask: sigset_t = [2]u32{ 0xfffffffc, 0x7fffffff } ++ [_]u32{0xffffffff} ** 30;

    const k_sigaction_funcs = struct {
        const handler = ?std.meta.FnPtr(fn (c_int) callconv(.C) void);
        const restorer = std.meta.FnPtr(fn () callconv(.C) void);
    };

    pub const k_sigaction = switch (native_arch) {
        .mips, .mipsel => extern struct {
            flags: c_uint,
            handler: k_sigaction_funcs.handler,
            mask: [4]c_ulong,
            restorer: k_sigaction_funcs.restorer,
        },
        .mips64, .mips64el => extern struct {
            flags: c_uint,
            handler: k_sigaction_funcs.handler,
            mask: [2]c_ulong,
            restorer: k_sigaction_funcs.restorer,
        },
        else => extern struct {
            handler: k_sigaction_funcs.handler,
            flags: c_ulong,
            restorer: k_sigaction_funcs.restorer,
            mask: [2]c_uint,
        },
    };

    /// Renamed from `sigaction` to `Sigaction` to avoid conflict with the syscall.
    pub const Sigaction = extern struct {
        pub const handler_fn = std.meta.FnPtr(fn (c_int) callconv(.C) void);
        pub const sigaction_fn = std.meta.FnPtr(fn (c_int, *const siginfo_t, ?*const anyopaque) callconv(.C) void);

        handler: extern union {
            handler: ?handler_fn,
            sigaction: ?sigaction_fn,
        },
        mask: sigset_t,
        flags: c_uint,
        restorer: ?std.meta.FnPtr(fn () callconv(.C) void) = null,
    };

    pub const empty_sigset = [_]u32{0} ** @typeInfo(sigset_t).Array.len;

    pub const SFD = struct {
        pub const CLOEXEC = O.CLOEXEC;
        pub const NONBLOCK = O.NONBLOCK;
    };

    pub const signalfd_siginfo = extern struct {
        signo: u32,
        errno: i32,
        code: i32,
        pid: u32,
        uid: uid_t,
        fd: i32,
        tid: u32,
        band: u32,
        overrun: u32,
        trapno: u32,
        status: i32,
        int: i32,
        ptr: u64,
        utime: u64,
        stime: u64,
        addr: u64,
        addr_lsb: u16,
        __pad2: u16,
        syscall: i32,
        call_addr: u64,
        native_arch: u32,
        __pad: [28]u8,
    };

    pub const in_port_t = u16;
    pub const sa_family_t = u16;
    pub const socklen_t = u32;

    pub const sockaddr = extern struct {
        family: sa_family_t,
        data: [14]u8,

        pub const SS_MAXSIZE = 128;
        pub const storage = std.x.os.Socket.Address.Native.Storage;

        /// IPv4 socket address
        pub const in = extern struct {
            family: sa_family_t = AF.INET,
            port: in_port_t,
            addr: u32,
            zero: [8]u8 = [8]u8{ 0, 0, 0, 0, 0, 0, 0, 0 },
        };

        /// IPv6 socket address
        pub const in6 = extern struct {
            family: sa_family_t = AF.INET6,
            port: in_port_t,
            flowinfo: u32,
            addr: [16]u8,
            scope_id: u32,
        };

        /// UNIX domain socket address
        pub const un = extern struct {
            family: sa_family_t = AF.UNIX,
            path: [108]u8,
        };

        /// Packet socket address
        pub const ll = extern struct {
            family: sa_family_t = AF.PACKET,
            protocol: u16,
            ifindex: i32,
            hatype: u16,
            pkttype: u8,
            halen: u8,
            addr: [8]u8,
        };

        /// Netlink socket address
        pub const nl = extern struct {
            family: sa_family_t = AF.NETLINK,
            __pad1: c_ushort = 0,

            /// port ID
            pid: u32,

            /// multicast groups mask
            groups: u32,
        };

        pub const xdp = extern struct {
            family: u16 = AF.XDP,
            flags: u16,
            ifindex: u32,
            queue_id: u32,
            shared_umem_fd: u32,
        };

        /// Address structure for vSockets
        pub const vm = extern struct {
            family: sa_family_t = AF.VSOCK,
            reserved1: u16 = 0,
            port: u32,
            cid: u32,
            flags: u8,

            /// The total size of this structure should be exactly the same as that of struct sockaddr.
            zero: [3]u8 = [_]u8{0} ** 3,
            comptime {
                std.debug.assert(@sizeOf(vm) == @sizeOf(sockaddr));
            }
        };
    };

    pub const mmsghdr = extern struct {
        msg_hdr: msghdr,
        msg_len: u32,
    };

    pub const mmsghdr_const = extern struct {
        msg_hdr: msghdr_const,
        msg_len: u32,
    };

    pub const epoll_data = extern union {
        ptr: usize,
        fd: i32,
        @"u32": u32,
        @"u64": u64,
    };

    pub const epoll_event = switch (builtin.zig_backend) {
        // stage1 crashes with the align(4) field so we have this workaround

        .stage1 => switch (native_arch) {
            .x86_64 => packed struct {
                events: u32,
                data: epoll_data,
            },
            else => extern struct {
                events: u32,
                data: epoll_data,
            },
        },
        else => extern struct {
            events: u32,
            data: epoll_data align(switch (native_arch) {
                .x86_64 => 4,
                else => @alignOf(epoll_data),
            }),
        },
    };

    pub const VFS_CAP_REVISION_MASK = 0xFF000000;
    pub const VFS_CAP_REVISION_SHIFT = 24;
    pub const VFS_CAP_FLAGS_MASK = ~VFS_CAP_REVISION_MASK;
    pub const VFS_CAP_FLAGS_EFFECTIVE = 0x000001;

    pub const VFS_CAP_REVISION_1 = 0x01000000;
    pub const VFS_CAP_U32_1 = 1;
    pub const XATTR_CAPS_SZ_1 = @sizeOf(u32) * (1 + 2 * VFS_CAP_U32_1);

    pub const VFS_CAP_REVISION_2 = 0x02000000;
    pub const VFS_CAP_U32_2 = 2;
    pub const XATTR_CAPS_SZ_2 = @sizeOf(u32) * (1 + 2 * VFS_CAP_U32_2);

    pub const XATTR_CAPS_SZ = XATTR_CAPS_SZ_2;
    pub const VFS_CAP_U32 = VFS_CAP_U32_2;
    pub const VFS_CAP_REVISION = VFS_CAP_REVISION_2;

    pub const vfs_cap_data = extern struct {
        //all of these are mandated as little endian

        //when on disk.

        const Data = struct {
            permitted: u32,
            inheritable: u32,
        };

        magic_etc: u32,
        data: [VFS_CAP_U32]Data,
    };

    pub const CAP = struct {
        pub const CHOWN = 0;
        pub const DAC_OVERRIDE = 1;
        pub const DAC_READ_SEARCH = 2;
        pub const FOWNER = 3;
        pub const FSETID = 4;
        pub const KILL = 5;
        pub const SETGID = 6;
        pub const SETUID = 7;
        pub const SETPCAP = 8;
        pub const LINUX_IMMUTABLE = 9;
        pub const NET_BIND_SERVICE = 10;
        pub const NET_BROADCAST = 11;
        pub const NET_ADMIN = 12;
        pub const NET_RAW = 13;
        pub const IPC_LOCK = 14;
        pub const IPC_OWNER = 15;
        pub const SYS_MODULE = 16;
        pub const SYS_RAWIO = 17;
        pub const SYS_CHROOT = 18;
        pub const SYS_PTRACE = 19;
        pub const SYS_PACCT = 20;
        pub const SYS_ADMIN = 21;
        pub const SYS_BOOT = 22;
        pub const SYS_NICE = 23;
        pub const SYS_RESOURCE = 24;
        pub const SYS_TIME = 25;
        pub const SYS_TTY_CONFIG = 26;
        pub const MKNOD = 27;
        pub const LEASE = 28;
        pub const AUDIT_WRITE = 29;
        pub const AUDIT_CONTROL = 30;
        pub const SETFCAP = 31;
        pub const MAC_OVERRIDE = 32;
        pub const MAC_ADMIN = 33;
        pub const SYSLOG = 34;
        pub const WAKE_ALARM = 35;
        pub const BLOCK_SUSPEND = 36;
        pub const AUDIT_READ = 37;
        pub const LAST_CAP = AUDIT_READ;

        pub fn valid(x: u8) bool {
            return x >= 0 and x <= LAST_CAP;
        }

        pub fn TO_MASK(cap: u8) u32 {
            return @as(u32, 1) << @intCast(u5, cap & 31);
        }

        pub fn TO_INDEX(cap: u8) u8 {
            return cap >> 5;
        }
    };

    pub const cap_t = extern struct {
        hdrp: *cap_user_header_t,
        datap: *cap_user_data_t,
    };

    pub const cap_user_header_t = extern struct {
        version: u32,
        pid: usize,
    };

    pub const cap_user_data_t = extern struct {
        effective: u32,
        permitted: u32,
        inheritable: u32,
    };

    pub const inotify_event = extern struct {
        wd: i32,
        mask: u32,
        cookie: u32,
        len: u32,
        //name: [?]u8,

    };

    pub const dirent64 = extern struct {
        d_ino: u64,
        d_off: u64,
        d_reclen: u16,
        d_type: u8,
        d_name: u8, // field address is the address of first byte of name https://github.com/ziglang/zig/issues/173

        pub fn reclen(self: dirent64) u16 {
            return self.d_reclen;
        }
    };

    pub const dl_phdr_info = extern struct {
        dlpi_addr: usize,
        dlpi_name: ?[*:0]const u8,
        dlpi_phdr: [*]std.elf.Phdr,
        dlpi_phnum: u16,
    };

    pub const CPU_SETSIZE = 128;
    pub const cpu_set_t = [CPU_SETSIZE / @sizeOf(usize)]usize;
    pub const cpu_count_t = std.meta.Int(.unsigned, std.math.log2(CPU_SETSIZE * 8));

    pub fn CPU_COUNT(set: cpu_set_t) cpu_count_t {
        var sum: cpu_count_t = 0;
        for (set) |x| {
            sum += @popCount(x);
        }
        return sum;
    }

    pub const MINSIGSTKSZ = switch (native_arch) {
        .i386, .x86_64, .arm, .mipsel => 2048,
        .aarch64 => 5120,
        else => @compileError("MINSIGSTKSZ not defined for this architecture"),
    };
    pub const SIGSTKSZ = switch (native_arch) {
        .i386, .x86_64, .arm, .mipsel => 8192,
        .aarch64 => 16384,
        else => @compileError("SIGSTKSZ not defined for this architecture"),
    };

    pub const SS_ONSTACK = 1;
    pub const SS_DISABLE = 2;
    pub const SS_AUTODISARM = 1 << 31;

    pub const stack_t = if (is_mips)
        // IRIX compatible stack_t

        extern struct {
            sp: [*]u8,
            size: usize,
            flags: i32,
        }
    else
        extern struct {
            sp: [*]u8,
            flags: i32,
            size: usize,
        };

    pub const sigval = extern union {
        int: i32,
        ptr: *anyopaque,
    };

    const siginfo_fields_union = extern union {
        pad: [128 - 2 * @sizeOf(c_int) - @sizeOf(c_long)]u8,
        common: extern struct {
            first: extern union {
                piduid: extern struct {
                    pid: pid_t,
                    uid: uid_t,
                },
                timer: extern struct {
                    timerid: i32,
                    overrun: i32,
                },
            },
            second: extern union {
                value: sigval,
                sigchld: extern struct {
                    status: i32,
                    utime: clock_t,
                    stime: clock_t,
                },
            },
        },
        sigfault: extern struct {
            addr: *anyopaque,
            addr_lsb: i16,
            first: extern union {
                addr_bnd: extern struct {
                    lower: *anyopaque,
                    upper: *anyopaque,
                },
                pkey: u32,
            },
        },
        sigpoll: extern struct {
            band: isize,
            fd: i32,
        },
        sigsys: extern struct {
            call_addr: *anyopaque,
            syscall: i32,
            native_arch: u32,
        },
    };

    pub const siginfo_t = if (is_mips)
        extern struct {
            signo: i32,
            code: i32,
            errno: i32,
            fields: siginfo_fields_union,
        }
    else
        extern struct {
            signo: i32,
            errno: i32,
            code: i32,
            fields: siginfo_fields_union,
        };

    pub const io_uring_params = extern struct {
        sq_entries: u32,
        cq_entries: u32,
        flags: u32,
        sq_thread_cpu: u32,
        sq_thread_idle: u32,
        features: u32,
        wq_fd: u32,
        resv: [3]u32,
        sq_off: io_sqring_offsets,
        cq_off: io_cqring_offsets,
    };

    // io_uring_params.features flags

    pub const IORING_FEAT_SINGLE_MMAP = 1 << 0;
    pub const IORING_FEAT_NODROP = 1 << 1;
    pub const IORING_FEAT_SUBMIT_STABLE = 1 << 2;
    pub const IORING_FEAT_RW_CUR_POS = 1 << 3;
    pub const IORING_FEAT_CUR_PERSONALITY = 1 << 4;
    pub const IORING_FEAT_FAST_POLL = 1 << 5;
    pub const IORING_FEAT_POLL_32BITS = 1 << 6;
    pub const IORING_FEAT_SQPOLL_NONFIXED = 1 << 7;
    pub const IORING_FEAT_EXT_ARG = 1 << 8;
    pub const IORING_FEAT_NATIVE_WORKERS = 1 << 9;
    pub const IORING_FEAT_RSRC_TAGS = 1 << 10;
    pub const IORING_FEAT_CQE_SKIP = 1 << 11;
    pub const IORING_FEAT_LINKED_FILE = 1 << 12;

    // io_uring_params.flags

    /// io_context is polled
    pub const IORING_SETUP_IOPOLL = 1 << 0;

    /// SQ poll thread
    pub const IORING_SETUP_SQPOLL = 1 << 1;

    /// sq_thread_cpu is valid
    pub const IORING_SETUP_SQ_AFF = 1 << 2;

    /// app defines CQ size
    pub const IORING_SETUP_CQSIZE = 1 << 3;

    /// clamp SQ/CQ ring sizes
    pub const IORING_SETUP_CLAMP = 1 << 4;

    /// attach to existing wq
    pub const IORING_SETUP_ATTACH_WQ = 1 << 5;

    /// start with ring disabled
    pub const IORING_SETUP_R_DISABLED = 1 << 6;

    /// continue submit on error
    pub const IORING_SETUP_SUBMIT_ALL = 1 << 7;

    /// Cooperative task running. When requests complete, they often require
    /// forcing the submitter to transition to the kernel to complete. If this
    /// flag is set, work will be done when the task transitions anyway, rather
    /// than force an inter-processor interrupt reschedule. This avoids interrupting
    /// a task running in userspace, and saves an IPI.
    pub const IORING_SETUP_COOP_TASKRUN = 1 << 8;

    /// If COOP_TASKRUN is set, get notified if task work is available for
    /// running and a kernel transition would be needed to run it. This sets
    /// IORING_SQ_TASKRUN in the sq ring flags. Not valid with COOP_TASKRUN.
    pub const IORING_SETUP_TASKRUN_FLAG = 1 << 9;

    /// SQEs are 128 byte
    pub const IORING_SETUP_SQE128 = 1 << 10;
    /// CQEs are 32 byte
    pub const IORING_SETUP_CQE32 = 1 << 11;

    pub const io_sqring_offsets = extern struct {
        /// offset of ring head
        head: u32,

        /// offset of ring tail
        tail: u32,

        /// ring mask value
        ring_mask: u32,

        /// entries in ring
        ring_entries: u32,

        /// ring flags
        flags: u32,

        /// number of sqes not submitted
        dropped: u32,

        /// sqe index array
        array: u32,

        resv1: u32,
        resv2: u64,
    };

    // io_sqring_offsets.flags

    /// needs io_uring_enter wakeup
    pub const IORING_SQ_NEED_WAKEUP = 1 << 0;
    /// kernel has cqes waiting beyond the cq ring
    pub const IORING_SQ_CQ_OVERFLOW = 1 << 1;
    /// task should enter the kernel
    pub const IORING_SQ_TASKRUN = 1 << 2;

    pub const io_cqring_offsets = extern struct {
        head: u32,
        tail: u32,
        ring_mask: u32,
        ring_entries: u32,
        overflow: u32,
        cqes: u32,
        resv: [2]u64,
    };

    pub const io_uring_sqe = extern struct {
        opcode: IORING_OP,
        flags: u8,
        ioprio: u16,
        fd: i32,
        off: u64,
        addr: u64,
        len: u32,
        rw_flags: u32,
        user_data: u64,
        buf_index: u16,
        personality: u16,
        splice_fd_in: i32,
        __pad2: [2]u64,
    };

    pub const IOSQE_BIT = enum(u8) {
        FIXED_FILE,
        IO_DRAIN,
        IO_LINK,
        IO_HARDLINK,
        ASYNC,
        BUFFER_SELECT,
        CQE_SKIP_SUCCESS,

        _,
    };

    // io_uring_sqe.flags

    /// use fixed fileset
    pub const IOSQE_FIXED_FILE = 1 << @enumToInt(IOSQE_BIT.FIXED_FILE);

    /// issue after inflight IO
    pub const IOSQE_IO_DRAIN = 1 << @enumToInt(IOSQE_BIT.IO_DRAIN);

    /// links next sqe
    pub const IOSQE_IO_LINK = 1 << @enumToInt(IOSQE_BIT.IO_LINK);

    /// like LINK, but stronger
    pub const IOSQE_IO_HARDLINK = 1 << @enumToInt(IOSQE_BIT.IO_HARDLINK);

    /// always go async
    pub const IOSQE_ASYNC = 1 << @enumToInt(IOSQE_BIT.ASYNC);

    /// select buffer from buf_group
    pub const IOSQE_BUFFER_SELECT = 1 << @enumToInt(IOSQE_BIT.BUFFER_SELECT);

    /// don't post CQE if request succeeded
    /// Available since Linux 5.17
    pub const IOSQE_CQE_SKIP_SUCCESS = 1 << @enumToInt(IOSQE_BIT.CQE_SKIP_SUCCESS);

    pub const IORING_OP = enum(u8) {
        NOP,
        READV,
        WRITEV,
        FSYNC,
        READ_FIXED,
        WRITE_FIXED,
        POLL_ADD,
        POLL_REMOVE,
        SYNC_FILE_RANGE,
        SENDMSG,
        RECVMSG,
        TIMEOUT,
        TIMEOUT_REMOVE,
        ACCEPT,
        ASYNC_CANCEL,
        LINK_TIMEOUT,
        CONNECT,
        FALLOCATE,
        OPENAT,
        CLOSE,
        FILES_UPDATE,
        STATX,
        READ,
        WRITE,
        FADVISE,
        MADVISE,
        SEND,
        RECV,
        OPENAT2,
        EPOLL_CTL,
        SPLICE,
        PROVIDE_BUFFERS,
        REMOVE_BUFFERS,
        TEE,
        SHUTDOWN,
        RENAMEAT,
        UNLINKAT,
        MKDIRAT,
        SYMLINKAT,
        LINKAT,

        _,
    };

    // io_uring_sqe.fsync_flags (rw_flags in the Zig struct)

    pub const IORING_FSYNC_DATASYNC = 1 << 0;

    // io_uring_sqe.timeout_flags (rw_flags in the Zig struct)

    pub const IORING_TIMEOUT_ABS = 1 << 0;
    pub const IORING_TIMEOUT_UPDATE = 1 << 1; // Available since Linux 5.11

    pub const IORING_TIMEOUT_BOOTTIME = 1 << 2; // Available since Linux 5.15

    pub const IORING_TIMEOUT_REALTIME = 1 << 3; // Available since Linux 5.15

    pub const IORING_LINK_TIMEOUT_UPDATE = 1 << 4; // Available since Linux 5.15

    pub const IORING_TIMEOUT_ETIME_SUCCESS = 1 << 5; // Available since Linux 5.16

    pub const IORING_TIMEOUT_CLOCK_MASK = IORING_TIMEOUT_BOOTTIME | IORING_TIMEOUT_REALTIME;
    pub const IORING_TIMEOUT_UPDATE_MASK = IORING_TIMEOUT_UPDATE | IORING_LINK_TIMEOUT_UPDATE;

    // io_uring_sqe.splice_flags (rw_flags in the Zig struct)

    // extends splice(2) flags

    pub const IORING_SPLICE_F_FD_IN_FIXED = 1 << 31;

    // POLL_ADD flags.

    // Note that since sqe->poll_events (rw_flags in the Zig struct) is the flag space, the command flags for POLL_ADD are stored in sqe->len.

    /// Multishot poll. Sets IORING_CQE_F_MORE if the poll handler will continue to report CQEs on behalf of the same SQE.
    pub const IORING_POLL_ADD_MULTI = 1 << 0;
    /// Update existing poll request, matching sqe->addr as the old user_data field.
    pub const IORING_POLL_UPDATE_EVENTS = 1 << 1;
    pub const IORING_POLL_UPDATE_USER_DATA = 1 << 2;

    // ASYNC_CANCEL flags.

    /// Cancel all requests that match the given key
    pub const IORING_ASYNC_CANCEL_ALL = 1 << 0;
    /// Key off 'fd' for cancelation rather than the request 'user_data'.
    pub const IORING_ASYNC_CANCEL_FD = 1 << 1;
    /// Match any request
    pub const IORING_ASYNC_CANCEL_ANY = 1 << 2;

    // send/sendmsg and recv/recvmsg flags (sqe->ioprio)

    /// If set, instead of first attempting to send or receive and arm poll if that yields an -EAGAIN result,
    /// arm poll upfront and skip the initial transfer attempt.
    pub const IORING_RECVSEND_POLL_FIRST = 1 << 0;
    /// Multishot recv. Sets IORING_CQE_F_MORE if the handler will continue to report CQEs on behalf of the same SQE.
    pub const IORING_RECV_MULTISHOT = 1 << 1;

    /// accept flags stored in sqe->ioprio
    pub const IORING_ACCEPT_MULTISHOT = 1 << 0;

    // IO completion data structure (Completion Queue Entry)

    pub const io_uring_cqe = extern struct {
        /// io_uring_sqe.data submission passed back
        user_data: u64,

        /// result code for this event
        res: i32,
        flags: u32,

        pub fn err(self: io_uring_cqe) E {
            if (self.res > -4096 and self.res < 0) {
                return @intToEnum(E, -self.res);
            }
            return .SUCCESS;
        }
    };

    // io_uring_cqe.flags

    /// If set, the upper 16 bits are the buffer ID
    pub const IORING_CQE_F_BUFFER = 1 << 0;
    /// If set, parent SQE will generate more CQE entries.
    /// Avaiable since Linux 5.13.
    pub const IORING_CQE_F_MORE = 1 << 1;
    /// If set, more data to read after socket recv
    pub const IORING_CQE_F_SOCK_NONEMPTY = 1 << 2;
    /// Set for notification CQEs. Can be used to distinct them from sends.
    pub const IORING_CQE_F_NOTIF = 1 << 3;

    /// Magic offsets for the application to mmap the data it needs
    pub const IORING_OFF_SQ_RING = 0;
    pub const IORING_OFF_CQ_RING = 0x8000000;
    pub const IORING_OFF_SQES = 0x10000000;

    // io_uring_enter flags

    pub const IORING_ENTER_GETEVENTS = 1 << 0;
    pub const IORING_ENTER_SQ_WAKEUP = 1 << 1;
    pub const IORING_ENTER_SQ_WAIT = 1 << 2;
    pub const IORING_ENTER_EXT_ARG = 1 << 3;
    pub const IORING_ENTER_REGISTERED_RING = 1 << 4;

    // io_uring_register opcodes and arguments

    pub const IORING_REGISTER = enum(u8) {
        REGISTER_BUFFERS,
        UNREGISTER_BUFFERS,
        REGISTER_FILES,
        UNREGISTER_FILES,
        REGISTER_EVENTFD,
        UNREGISTER_EVENTFD,
        REGISTER_FILES_UPDATE,
        REGISTER_EVENTFD_ASYNC,
        REGISTER_PROBE,
        REGISTER_PERSONALITY,
        UNREGISTER_PERSONALITY,
        REGISTER_RESTRICTIONS,
        REGISTER_ENABLE_RINGS,

        // extended with tagging

        IORING_REGISTER_FILES2,
        IORING_REGISTER_FILES_UPDATE2,
        IORING_REGISTER_BUFFERS2,
        IORING_REGISTER_BUFFERS_UPDATE,

        // set/clear io-wq thread affinities

        IORING_REGISTER_IOWQ_AFF,
        IORING_UNREGISTER_IOWQ_AFF,

        // set/get max number of io-wq workers

        IORING_REGISTER_IOWQ_MAX_WORKERS,

        // register/unregister io_uring fd with the ring

        IORING_REGISTER_RING_FDS,
        IORING_UNREGISTER_RING_FDS,

        // register ring based provide buffer group

        IORING_REGISTER_PBUF_RING,
        IORING_UNREGISTER_PBUF_RING,

        // sync cancelation API

        IORING_REGISTER_SYNC_CANCEL,

        // register a range of fixed file slots for automatic slot allocation

        IORING_REGISTER_FILE_ALLOC_RANGE,

        _,
    };

    pub const io_uring_files_update = extern struct {
        offset: u32,
        resv: u32,
        fds: u64,
    };

    pub const IO_URING_OP_SUPPORTED = 1 << 0;

    pub const io_uring_probe_op = extern struct {
        op: IORING_OP,

        resv: u8,

        /// IO_URING_OP_* flags
        flags: u16,

        resv2: u32,
    };

    pub const io_uring_probe = extern struct {
        /// last opcode supported
        last_op: IORING_OP,

        /// Number of io_uring_probe_op following
        ops_len: u8,

        resv: u16,
        resv2: u32[3],

        // Followed by up to `ops_len` io_uring_probe_op structures

    };

    pub const io_uring_restriction = extern struct {
        opcode: u16,
        arg: extern union {
            /// IORING_RESTRICTION_REGISTER_OP
            register_op: IORING_REGISTER,

            /// IORING_RESTRICTION_SQE_OP
            sqe_op: IORING_OP,

            /// IORING_RESTRICTION_SQE_FLAGS_*
            sqe_flags: u8,
        },
        resv: u8,
        resv2: u32[3],
    };

    /// io_uring_restriction->opcode values
    pub const IORING_RESTRICTION = enum(u8) {
        /// Allow an io_uring_register(2) opcode
        REGISTER_OP = 0,

        /// Allow an sqe opcode
        SQE_OP = 1,

        /// Allow sqe flags
        SQE_FLAGS_ALLOWED = 2,

        /// Require sqe flags (these flags must be set on each submission)
        SQE_FLAGS_REQUIRED = 3,

        _,
    };

    pub const utsname = extern struct {
        sysname: [64:0]u8,
        nodename: [64:0]u8,
        release: [64:0]u8,
        version: [64:0]u8,
        machine: [64:0]u8,
        domainname: [64:0]u8,
    };
    pub const HOST_NAME_MAX = 64;

    pub const STATX_TYPE = 0x0001;
    pub const STATX_MODE = 0x0002;
    pub const STATX_NLINK = 0x0004;
    pub const STATX_UID = 0x0008;
    pub const STATX_GID = 0x0010;
    pub const STATX_ATIME = 0x0020;
    pub const STATX_MTIME = 0x0040;
    pub const STATX_CTIME = 0x0080;
    pub const STATX_INO = 0x0100;
    pub const STATX_SIZE = 0x0200;
    pub const STATX_BLOCKS = 0x0400;
    pub const STATX_BASIC_STATS = 0x07ff;

    pub const STATX_BTIME = 0x0800;

    pub const STATX_ATTR_COMPRESSED = 0x0004;
    pub const STATX_ATTR_IMMUTABLE = 0x0010;
    pub const STATX_ATTR_APPEND = 0x0020;
    pub const STATX_ATTR_NODUMP = 0x0040;
    pub const STATX_ATTR_ENCRYPTED = 0x0800;
    pub const STATX_ATTR_AUTOMOUNT = 0x1000;

    pub const statx_timestamp = extern struct {
        tv_sec: i64,
        tv_nsec: u32,
        __pad1: u32,
    };

    /// Renamed to `Statx` to not conflict with the `statx` function.
    pub const Statx = extern struct {
        /// Mask of bits indicating filled fields
        mask: u32,

        /// Block size for filesystem I/O
        blksize: u32,

        /// Extra file attribute indicators
        attributes: u64,

        /// Number of hard links
        nlink: u32,

        /// User ID of owner
        uid: uid_t,

        /// Group ID of owner
        gid: gid_t,

        /// File type and mode
        mode: u16,
        __pad1: u16,

        /// Inode number
        ino: u64,

        /// Total size in bytes
        size: u64,

        /// Number of 512B blocks allocated
        blocks: u64,

        /// Mask to show what's supported in `attributes`.
        attributes_mask: u64,

        /// Last access file timestamp
        atime: statx_timestamp,

        /// Creation file timestamp
        btime: statx_timestamp,

        /// Last status change file timestamp
        ctime: statx_timestamp,

        /// Last modification file timestamp
        mtime: statx_timestamp,

        /// Major ID, if this file represents a device.
        rdev_major: u32,

        /// Minor ID, if this file represents a device.
        rdev_minor: u32,

        /// Major ID of the device containing the filesystem where this file resides.
        dev_major: u32,

        /// Minor ID of the device containing the filesystem where this file resides.
        dev_minor: u32,

        __pad2: [14]u64,
    };

    pub const addrinfo = extern struct {
        flags: i32,
        family: i32,
        socktype: i32,
        protocol: i32,
        addrlen: socklen_t,
        addr: ?*sockaddr,
        canonname: ?[*:0]u8,
        next: ?*addrinfo,
    };

    pub const IPPORT_RESERVED = 1024;

    pub const IPPROTO = struct {
        pub const IP = 0;
        pub const HOPOPTS = 0;
        pub const ICMP = 1;
        pub const IGMP = 2;
        pub const IPIP = 4;
        pub const TCP = 6;
        pub const EGP = 8;
        pub const PUP = 12;
        pub const UDP = 17;
        pub const IDP = 22;
        pub const TP = 29;
        pub const DCCP = 33;
        pub const IPV6 = 41;
        pub const ROUTING = 43;
        pub const FRAGMENT = 44;
        pub const RSVP = 46;
        pub const GRE = 47;
        pub const ESP = 50;
        pub const AH = 51;
        pub const ICMPV6 = 58;
        pub const NONE = 59;
        pub const DSTOPTS = 60;
        pub const MTP = 92;
        pub const BEETPH = 94;
        pub const ENCAP = 98;
        pub const PIM = 103;
        pub const COMP = 108;
        pub const SCTP = 132;
        pub const MH = 135;
        pub const UDPLITE = 136;
        pub const MPLS = 137;
        pub const RAW = 255;
        pub const MAX = 256;
    };

    pub const RR = struct {
        pub const A = 1;
        pub const CNAME = 5;
        pub const AAAA = 28;
    };

    pub const tcp_repair_opt = extern struct {
        opt_code: u32,
        opt_val: u32,
    };

    pub const tcp_repair_window = extern struct {
        snd_wl1: u32,
        snd_wnd: u32,
        max_window: u32,
        rcv_wnd: u32,
        rcv_wup: u32,
    };

    pub const TcpRepairOption = enum {
        TCP_NO_QUEUE,
        TCP_RECV_QUEUE,
        TCP_SEND_QUEUE,
        TCP_QUEUES_NR,
    };

    /// why fastopen failed from client perspective
    pub const tcp_fastopen_client_fail = enum {
        /// catch-all
        TFO_STATUS_UNSPEC,
        /// if not in TFO_CLIENT_NO_COOKIE mode
        TFO_COOKIE_UNAVAILABLE,
        /// SYN-ACK did not ack SYN data
        TFO_DATA_NOT_ACKED,
        /// SYN-ACK did not ack SYN data after timeout
        TFO_SYN_RETRANSMITTED,
    };

    /// for TCP_INFO socket option
    pub const TCPI_OPT_TIMESTAMPS = 1;
    pub const TCPI_OPT_SACK = 2;
    pub const TCPI_OPT_WSCALE = 4;
    /// ECN was negociated at TCP session init
    pub const TCPI_OPT_ECN = 8;
    /// we received at least one packet with ECT
    pub const TCPI_OPT_ECN_SEEN = 16;
    /// SYN-ACK acked data in SYN sent or rcvd
    pub const TCPI_OPT_SYN_DATA = 32;

    pub const nfds_t = usize;
    pub const pollfd = extern struct {
        fd: fd_t,
        events: i16,
        revents: i16,
    };

    pub const POLL = struct {
        pub const IN = 0x001;
        pub const PRI = 0x002;
        pub const OUT = 0x004;
        pub const ERR = 0x008;
        pub const HUP = 0x010;
        pub const NVAL = 0x020;
        pub const RDNORM = 0x040;
        pub const RDBAND = 0x080;
    };

    pub const HUGETLB_FLAG_ENCODE_SHIFT = 26;
    pub const HUGETLB_FLAG_ENCODE_MASK = 0x3f;
    pub const HUGETLB_FLAG_ENCODE_64KB = 16 << HUGETLB_FLAG_ENCODE_SHIFT;
    pub const HUGETLB_FLAG_ENCODE_512KB = 19 << HUGETLB_FLAG_ENCODE_SHIFT;
    pub const HUGETLB_FLAG_ENCODE_1MB = 20 << HUGETLB_FLAG_ENCODE_SHIFT;
    pub const HUGETLB_FLAG_ENCODE_2MB = 21 << HUGETLB_FLAG_ENCODE_SHIFT;
    pub const HUGETLB_FLAG_ENCODE_8MB = 23 << HUGETLB_FLAG_ENCODE_SHIFT;
    pub const HUGETLB_FLAG_ENCODE_16MB = 24 << HUGETLB_FLAG_ENCODE_SHIFT;
    pub const HUGETLB_FLAG_ENCODE_32MB = 25 << HUGETLB_FLAG_ENCODE_SHIFT;
    pub const HUGETLB_FLAG_ENCODE_256MB = 28 << HUGETLB_FLAG_ENCODE_SHIFT;
    pub const HUGETLB_FLAG_ENCODE_512MB = 29 << HUGETLB_FLAG_ENCODE_SHIFT;
    pub const HUGETLB_FLAG_ENCODE_1GB = 30 << HUGETLB_FLAG_ENCODE_SHIFT;
    pub const HUGETLB_FLAG_ENCODE_2GB = 31 << HUGETLB_FLAG_ENCODE_SHIFT;
    pub const HUGETLB_FLAG_ENCODE_16GB = 34 << HUGETLB_FLAG_ENCODE_SHIFT;

    pub const MFD = struct {
        pub const CLOEXEC = 0x0001;
        pub const ALLOW_SEALING = 0x0002;
        pub const HUGETLB = 0x0004;
        pub const ALL_FLAGS = CLOEXEC | ALLOW_SEALING | HUGETLB;

        pub const HUGE_SHIFT = HUGETLB_FLAG_ENCODE_SHIFT;
        pub const HUGE_MASK = HUGETLB_FLAG_ENCODE_MASK;
        pub const HUGE_64KB = HUGETLB_FLAG_ENCODE_64KB;
        pub const HUGE_512KB = HUGETLB_FLAG_ENCODE_512KB;
        pub const HUGE_1MB = HUGETLB_FLAG_ENCODE_1MB;
        pub const HUGE_2MB = HUGETLB_FLAG_ENCODE_2MB;
        pub const HUGE_8MB = HUGETLB_FLAG_ENCODE_8MB;
        pub const HUGE_16MB = HUGETLB_FLAG_ENCODE_16MB;
        pub const HUGE_32MB = HUGETLB_FLAG_ENCODE_32MB;
        pub const HUGE_256MB = HUGETLB_FLAG_ENCODE_256MB;
        pub const HUGE_512MB = HUGETLB_FLAG_ENCODE_512MB;
        pub const HUGE_1GB = HUGETLB_FLAG_ENCODE_1GB;
        pub const HUGE_2GB = HUGETLB_FLAG_ENCODE_2GB;
        pub const HUGE_16GB = HUGETLB_FLAG_ENCODE_16GB;
    };

    pub const rusage = extern struct {
        utime: timeval,
        stime: timeval,
        maxrss: isize,
        ixrss: isize,
        idrss: isize,
        isrss: isize,
        minflt: isize,
        majflt: isize,
        nswap: isize,
        inblock: isize,
        oublock: isize,
        msgsnd: isize,
        msgrcv: isize,
        nsignals: isize,
        nvcsw: isize,
        nivcsw: isize,
        __reserved: [16]isize = [1]isize{0} ** 16,

        pub const SELF = 0;
        pub const CHILDREN = -1;
        pub const THREAD = 1;
    };

    pub const cc_t = u8;
    pub const speed_t = u32;
    pub const tcflag_t = u32;

    pub const NCCS = 32;

    pub const B0 = 0o0000000;
    pub const B50 = 0o0000001;
    pub const B75 = 0o0000002;
    pub const B110 = 0o0000003;
    pub const B134 = 0o0000004;
    pub const B150 = 0o0000005;
    pub const B200 = 0o0000006;
    pub const B300 = 0o0000007;
    pub const B600 = 0o0000010;
    pub const B1200 = 0o0000011;
    pub const B1800 = 0o0000012;
    pub const B2400 = 0o0000013;
    pub const B4800 = 0o0000014;
    pub const B9600 = 0o0000015;
    pub const B19200 = 0o0000016;
    pub const B38400 = 0o0000017;
    pub const BOTHER = 0o0010000;
    pub const B57600 = 0o0010001;
    pub const B115200 = 0o0010002;
    pub const B230400 = 0o0010003;
    pub const B460800 = 0o0010004;
    pub const B500000 = 0o0010005;
    pub const B576000 = 0o0010006;
    pub const B921600 = 0o0010007;
    pub const B1000000 = 0o0010010;
    pub const B1152000 = 0o0010011;
    pub const B1500000 = 0o0010012;
    pub const B2000000 = 0o0010013;
    pub const B2500000 = 0o0010014;
    pub const B3000000 = 0o0010015;
    pub const B3500000 = 0o0010016;
    pub const B4000000 = 0o0010017;

    pub const V = switch (native_arch) {
        .powerpc, .powerpc64, .powerpc64le => struct {
            pub const INTR = 0;
            pub const QUIT = 1;
            pub const ERASE = 2;
            pub const KILL = 3;
            pub const EOF = 4;
            pub const MIN = 5;
            pub const EOL = 6;
            pub const TIME = 7;
            pub const EOL2 = 8;
            pub const SWTC = 9;
            pub const WERASE = 10;
            pub const REPRINT = 11;
            pub const SUSP = 12;
            pub const START = 13;
            pub const STOP = 14;
            pub const LNEXT = 15;
            pub const DISCARD = 16;
        },
        .sparc, .sparc64 => struct {
            pub const INTR = 0;
            pub const QUIT = 1;
            pub const ERASE = 2;
            pub const KILL = 3;
            pub const EOF = 4;
            pub const EOL = 5;
            pub const EOL2 = 6;
            pub const SWTC = 7;
            pub const START = 8;
            pub const STOP = 9;
            pub const SUSP = 10;
            pub const DSUSP = 11;
            pub const REPRINT = 12;
            pub const DISCARD = 13;
            pub const WERASE = 14;
            pub const LNEXT = 15;
            pub const MIN = EOF;
            pub const TIME = EOL;
        },
        .mips, .mipsel, .mips64, .mips64el => struct {
            pub const INTR = 0;
            pub const QUIT = 1;
            pub const ERASE = 2;
            pub const KILL = 3;
            pub const MIN = 4;
            pub const TIME = 5;
            pub const EOL2 = 6;
            pub const SWTC = 7;
            pub const SWTCH = 7;
            pub const START = 8;
            pub const STOP = 9;
            pub const SUSP = 10;
            pub const REPRINT = 12;
            pub const DISCARD = 13;
            pub const WERASE = 14;
            pub const LNEXT = 15;
            pub const EOF = 16;
            pub const EOL = 17;
        },
        else => struct {
            pub const INTR = 0;
            pub const QUIT = 1;
            pub const ERASE = 2;
            pub const KILL = 3;
            pub const EOF = 4;
            pub const TIME = 5;
            pub const MIN = 6;
            pub const SWTC = 7;
            pub const START = 8;
            pub const STOP = 9;
            pub const SUSP = 10;
            pub const EOL = 11;
            pub const REPRINT = 12;
            pub const DISCARD = 13;
            pub const WERASE = 14;
            pub const LNEXT = 15;
            pub const EOL2 = 16;
        },
    };

    pub const IGNBRK: tcflag_t = 1;
    pub const BRKINT: tcflag_t = 2;
    pub const IGNPAR: tcflag_t = 4;
    pub const PARMRK: tcflag_t = 8;
    pub const INPCK: tcflag_t = 16;
    pub const ISTRIP: tcflag_t = 32;
    pub const INLCR: tcflag_t = 64;
    pub const IGNCR: tcflag_t = 128;
    pub const ICRNL: tcflag_t = 256;
    pub const IUCLC: tcflag_t = 512;
    pub const IXON: tcflag_t = 1024;
    pub const IXANY: tcflag_t = 2048;
    pub const IXOFF: tcflag_t = 4096;
    pub const IMAXBEL: tcflag_t = 8192;
    pub const IUTF8: tcflag_t = 16384;

    pub const OPOST: tcflag_t = 1;
    pub const OLCUC: tcflag_t = 2;
    pub const ONLCR: tcflag_t = 4;
    pub const OCRNL: tcflag_t = 8;
    pub const ONOCR: tcflag_t = 16;
    pub const ONLRET: tcflag_t = 32;
    pub const OFILL: tcflag_t = 64;
    pub const OFDEL: tcflag_t = 128;
    pub const VTDLY: tcflag_t = 16384;
    pub const VT0: tcflag_t = 0;
    pub const VT1: tcflag_t = 16384;

    pub const CSIZE: tcflag_t = 48;
    pub const CS5: tcflag_t = 0;
    pub const CS6: tcflag_t = 16;
    pub const CS7: tcflag_t = 32;
    pub const CS8: tcflag_t = 48;
    pub const CSTOPB: tcflag_t = 64;
    pub const CREAD: tcflag_t = 128;
    pub const PARENB: tcflag_t = 256;
    pub const PARODD: tcflag_t = 512;
    pub const HUPCL: tcflag_t = 1024;
    pub const CLOCAL: tcflag_t = 2048;

    pub const ISIG: tcflag_t = 1;
    pub const ICANON: tcflag_t = 2;
    pub const ECHO: tcflag_t = 8;
    pub const ECHOE: tcflag_t = 16;
    pub const ECHOK: tcflag_t = 32;
    pub const ECHONL: tcflag_t = 64;
    pub const NOFLSH: tcflag_t = 128;
    pub const TOSTOP: tcflag_t = 256;
    pub const IEXTEN: tcflag_t = 32768;

    pub const TCSA = enum(c_uint) {
        NOW,
        DRAIN,
        FLUSH,
        _,
    };

    pub const termios = extern struct {
        iflag: tcflag_t,
        oflag: tcflag_t,
        cflag: tcflag_t,
        lflag: tcflag_t,
        line: cc_t,
        cc: [NCCS]cc_t,
        ispeed: speed_t,
        ospeed: speed_t,
    };

    pub const SIOCGIFINDEX = 0x8933;
    pub const IFNAMESIZE = 16;

    pub const ifmap = extern struct {
        mem_start: u32,
        mem_end: u32,
        base_addr: u16,
        irq: u8,
        dma: u8,
        port: u8,
    };

    pub const ifreq = extern struct {
        ifrn: extern union {
            name: [IFNAMESIZE]u8,
        },
        ifru: extern union {
            addr: sockaddr,
            dstaddr: sockaddr,
            broadaddr: sockaddr,
            netmask: sockaddr,
            hwaddr: sockaddr,
            flags: i16,
            ivalue: i32,
            mtu: i32,
            map: ifmap,
            slave: [IFNAMESIZE - 1:0]u8,
            newname: [IFNAMESIZE - 1:0]u8,
            data: ?[*]u8,
        },
    };

    // doc comments copied from musl

    pub const rlimit_resource = if (native_arch.isMIPS() or native_arch.isSPARC())
        arch_bits.rlimit_resource
    else
        enum(c_int) {
            /// Per-process CPU limit, in seconds.
            CPU,

            /// Largest file that can be created, in bytes.
            FSIZE,

            /// Maximum size of data segment, in bytes.
            DATA,

            /// Maximum size of stack segment, in bytes.
            STACK,

            /// Largest core file that can be created, in bytes.
            CORE,

            /// Largest resident set size, in bytes.
            /// This affects swapping; processes that are exceeding their
            /// resident set size will be more likely to have physical memory
            /// taken from them.
            RSS,

            /// Number of processes.
            NPROC,

            /// Number of open files.
            NOFILE,

            /// Locked-in-memory address space.
            MEMLOCK,

            /// Address space limit.
            AS,

            /// Maximum number of file locks.
            LOCKS,

            /// Maximum number of pending signals.
            SIGPENDING,

            /// Maximum bytes in POSIX message queues.
            MSGQUEUE,

            /// Maximum nice priority allowed to raise to.
            /// Nice levels 19 .. -20 correspond to 0 .. 39
            /// values of this resource limit.
            NICE,

            /// Maximum realtime priority allowed for non-priviledged
            /// processes.
            RTPRIO,

            /// Maximum CPU time in µs that a process scheduled under a real-time
            /// scheduling policy may consume without making a blocking system
            /// call before being forcibly descheduled.
            RTTIME,

            _,
        };

    pub const rlim_t = u64;

    pub const RLIM = struct {
        /// No limit
        pub const INFINITY = ~@as(rlim_t, 0);

        pub const SAVED_MAX = INFINITY;
        pub const SAVED_CUR = INFINITY;
    };

    pub const rlimit = extern struct {
        /// Soft limit
        cur: rlim_t,
        /// Hard limit
        max: rlim_t,
    };

    pub const MADV = struct {
        pub const NORMAL = 0;
        pub const RANDOM = 1;
        pub const SEQUENTIAL = 2;
        pub const WILLNEED = 3;
        pub const DONTNEED = 4;
        pub const FREE = 8;
        pub const REMOVE = 9;
        pub const DONTFORK = 10;
        pub const DOFORK = 11;
        pub const MERGEABLE = 12;
        pub const UNMERGEABLE = 13;
        pub const HUGEPAGE = 14;
        pub const NOHUGEPAGE = 15;
        pub const DONTDUMP = 16;
        pub const DODUMP = 17;
        pub const WIPEONFORK = 18;
        pub const KEEPONFORK = 19;
        pub const COLD = 20;
        pub const PAGEOUT = 21;
        pub const HWPOISON = 100;
        pub const SOFT_OFFLINE = 101;
    };

    pub const POSIX_FADV = switch (native_arch) {
        .s390x => if (@typeInfo(usize).Int.bits == 64) struct {
            pub const NORMAL = 0;
            pub const RANDOM = 1;
            pub const SEQUENTIAL = 2;
            pub const WILLNEED = 3;
            pub const DONTNEED = 6;
            pub const NOREUSE = 7;
        } else struct {
            pub const NORMAL = 0;
            pub const RANDOM = 1;
            pub const SEQUENTIAL = 2;
            pub const WILLNEED = 3;
            pub const DONTNEED = 4;
            pub const NOREUSE = 5;
        },
        else => struct {
            pub const NORMAL = 0;
            pub const RANDOM = 1;
            pub const SEQUENTIAL = 2;
            pub const WILLNEED = 3;
            pub const DONTNEED = 4;
            pub const NOREUSE = 5;
        },
    };

    /// The timespec struct used by the kernel.
    pub const kernel_timespec = if (@sizeOf(usize) >= 8) timespec else extern struct {
        tv_sec: i64,
        tv_nsec: i64,
    };

    pub const timespec = extern struct {
        tv_sec: isize,
        tv_nsec: isize,
    };

    pub const XDP = struct {
        pub const SHARED_UMEM = (1 << 0);
        pub const COPY = (1 << 1);
        pub const ZEROCOPY = (1 << 2);
        pub const UMEM_UNALIGNED_CHUNK_FLAG = (1 << 0);
        pub const USE_NEED_WAKEUP = (1 << 3);

        pub const MMAP_OFFSETS = 1;
        pub const RX_RING = 2;
        pub const TX_RING = 3;
        pub const UMEM_REG = 4;
        pub const UMEM_FILL_RING = 5;
        pub const UMEM_COMPLETION_RING = 6;
        pub const STATISTICS = 7;
        pub const OPTIONS = 8;

        pub const OPTIONS_ZEROCOPY = (1 << 0);

        pub const PGOFF_RX_RING = 0;
        pub const PGOFF_TX_RING = 0x80000000;
        pub const UMEM_PGOFF_FILL_RING = 0x100000000;
        pub const UMEM_PGOFF_COMPLETION_RING = 0x180000000;
    };

    pub const xdp_ring_offset = extern struct {
        producer: u64,
        consumer: u64,
        desc: u64,
        flags: u64,
    };

    pub const xdp_mmap_offsets = extern struct {
        rx: xdp_ring_offset,
        tx: xdp_ring_offset,
        fr: xdp_ring_offset,
        cr: xdp_ring_offset,
    };

    pub const xdp_umem_reg = extern struct {
        addr: u64,
        len: u64,
        chunk_size: u32,
        headroom: u32,
        flags: u32,
    };

    pub const xdp_statistics = extern struct {
        rx_dropped: u64,
        rx_invalid_descs: u64,
        tx_invalid_descs: u64,
        rx_ring_full: u64,
        rx_fill_ring_empty_descs: u64,
        tx_ring_empty_descs: u64,
    };

    pub const xdp_options = extern struct {
        flags: u32,
    };

    pub const XSK_UNALIGNED_BUF_OFFSET_SHIFT = 48;
    pub const XSK_UNALIGNED_BUF_ADDR_MASK = (1 << XSK_UNALIGNED_BUF_OFFSET_SHIFT) - 1;

    pub const xdp_desc = extern struct {
        addr: u64,
        len: u32,
        options: u32,
    };

    fn issecure_mask(comptime x: comptime_int) comptime_int {
        return 1 << x;
    }

    pub const SECUREBITS_DEFAULT = 0x00000000;

    pub const SECURE_NOROOT = 0;
    pub const SECURE_NOROOT_LOCKED = 1;

    pub const SECBIT_NOROOT = issecure_mask(SECURE_NOROOT);
    pub const SECBIT_NOROOT_LOCKED = issecure_mask(SECURE_NOROOT_LOCKED);

    pub const SECURE_NO_SETUID_FIXUP = 2;
    pub const SECURE_NO_SETUID_FIXUP_LOCKED = 3;

    pub const SECBIT_NO_SETUID_FIXUP = issecure_mask(SECURE_NO_SETUID_FIXUP);
    pub const SECBIT_NO_SETUID_FIXUP_LOCKED = issecure_mask(SECURE_NO_SETUID_FIXUP_LOCKED);

    pub const SECURE_KEEP_CAPS = 4;
    pub const SECURE_KEEP_CAPS_LOCKED = 5;

    pub const SECBIT_KEEP_CAPS = issecure_mask(SECURE_KEEP_CAPS);
    pub const SECBIT_KEEP_CAPS_LOCKED = issecure_mask(SECURE_KEEP_CAPS_LOCKED);

    pub const SECURE_NO_CAP_AMBIENT_RAISE = 6;
    pub const SECURE_NO_CAP_AMBIENT_RAISE_LOCKED = 7;

    pub const SECBIT_NO_CAP_AMBIENT_RAISE = issecure_mask(SECURE_NO_CAP_AMBIENT_RAISE);
    pub const SECBIT_NO_CAP_AMBIENT_RAISE_LOCKED = issecure_mask(SECURE_NO_CAP_AMBIENT_RAISE_LOCKED);

    pub const SECURE_ALL_BITS = issecure_mask(SECURE_NOROOT) |
        issecure_mask(SECURE_NO_SETUID_FIXUP) |
        issecure_mask(SECURE_KEEP_CAPS) |
        issecure_mask(SECURE_NO_CAP_AMBIENT_RAISE);
    pub const SECURE_ALL_LOCKS = SECURE_ALL_BITS << 1;

    pub const PR = enum(i32) {
        SET_PDEATHSIG = 1,
        GET_PDEATHSIG = 2,

        GET_DUMPABLE = 3,
        SET_DUMPABLE = 4,

        GET_UNALIGN = 5,
        SET_UNALIGN = 6,

        GET_KEEPCAPS = 7,
        SET_KEEPCAPS = 8,

        GET_FPEMU = 9,
        SET_FPEMU = 10,

        GET_FPEXC = 11,
        SET_FPEXC = 12,

        GET_TIMING = 13,
        SET_TIMING = 14,

        SET_NAME = 15,
        GET_NAME = 16,

        GET_ENDIAN = 19,
        SET_ENDIAN = 20,

        GET_SECCOMP = 21,
        SET_SECCOMP = 22,

        CAPBSET_READ = 23,
        CAPBSET_DROP = 24,

        GET_TSC = 25,
        SET_TSC = 26,

        GET_SECUREBITS = 27,
        SET_SECUREBITS = 28,

        SET_TIMERSLACK = 29,
        GET_TIMERSLACK = 30,

        TASK_PERF_EVENTS_DISABLE = 31,
        TASK_PERF_EVENTS_ENABLE = 32,

        MCE_KILL = 33,

        MCE_KILL_GET = 34,

        SET_MM = 35,

        SET_PTRACER = 0x59616d61,

        SET_CHILD_SUBREAPER = 36,
        GET_CHILD_SUBREAPER = 37,

        SET_NO_NEW_PRIVS = 38,
        GET_NO_NEW_PRIVS = 39,

        GET_TID_ADDRESS = 40,

        SET_THP_DISABLE = 41,
        GET_THP_DISABLE = 42,

        MPX_ENABLE_MANAGEMENT = 43,
        MPX_DISABLE_MANAGEMENT = 44,

        SET_FP_MODE = 45,
        GET_FP_MODE = 46,

        CAP_AMBIENT = 47,

        SVE_SET_VL = 50,
        SVE_GET_VL = 51,

        GET_SPECULATION_CTRL = 52,
        SET_SPECULATION_CTRL = 53,

        _,

        pub const UNALIGN_NOPRINT = 1;
        pub const UNALIGN_SIGBUS = 2;

        pub const FPEMU_NOPRINT = 1;
        pub const FPEMU_SIGFPE = 2;

        pub const FP_EXC_SW_ENABLE = 0x80;
        pub const FP_EXC_DIV = 0x010000;
        pub const FP_EXC_OVF = 0x020000;
        pub const FP_EXC_UND = 0x040000;
        pub const FP_EXC_RES = 0x080000;
        pub const FP_EXC_INV = 0x100000;
        pub const FP_EXC_DISABLED = 0;
        pub const FP_EXC_NONRECOV = 1;
        pub const FP_EXC_ASYNC = 2;
        pub const FP_EXC_PRECISE = 3;

        pub const TIMING_STATISTICAL = 0;
        pub const TIMING_TIMESTAMP = 1;

        pub const ENDIAN_BIG = 0;
        pub const ENDIAN_LITTLE = 1;
        pub const ENDIAN_PPC_LITTLE = 2;

        pub const TSC_ENABLE = 1;
        pub const TSC_SIGSEGV = 2;

        pub const MCE_KILL_CLEAR = 0;
        pub const MCE_KILL_SET = 1;

        pub const MCE_KILL_LATE = 0;
        pub const MCE_KILL_EARLY = 1;
        pub const MCE_KILL_DEFAULT = 2;

        pub const SET_MM_START_CODE = 1;
        pub const SET_MM_END_CODE = 2;
        pub const SET_MM_START_DATA = 3;
        pub const SET_MM_END_DATA = 4;
        pub const SET_MM_START_STACK = 5;
        pub const SET_MM_START_BRK = 6;
        pub const SET_MM_BRK = 7;
        pub const SET_MM_ARG_START = 8;
        pub const SET_MM_ARG_END = 9;
        pub const SET_MM_ENV_START = 10;
        pub const SET_MM_ENV_END = 11;
        pub const SET_MM_AUXV = 12;
        pub const SET_MM_EXE_FILE = 13;
        pub const SET_MM_MAP = 14;
        pub const SET_MM_MAP_SIZE = 15;

        pub const SET_PTRACER_ANY = std.math.maxInt(c_ulong);

        pub const FP_MODE_FR = 1 << 0;
        pub const FP_MODE_FRE = 1 << 1;

        pub const CAP_AMBIENT_IS_SET = 1;
        pub const CAP_AMBIENT_RAISE = 2;
        pub const CAP_AMBIENT_LOWER = 3;
        pub const CAP_AMBIENT_CLEAR_ALL = 4;

        pub const SVE_SET_VL_ONEXEC = 1 << 18;
        pub const SVE_VL_LEN_MASK = 0xffff;
        pub const SVE_VL_INHERIT = 1 << 17;

        pub const SPEC_STORE_BYPASS = 0;
        pub const SPEC_NOT_AFFECTED = 0;
        pub const SPEC_PRCTL = 1 << 0;
        pub const SPEC_ENABLE = 1 << 1;
        pub const SPEC_DISABLE = 1 << 2;
        pub const SPEC_FORCE_DISABLE = 1 << 3;
    };

    pub const prctl_mm_map = extern struct {
        start_code: u64,
        end_code: u64,
        start_data: u64,
        end_data: u64,
        start_brk: u64,
        brk: u64,
        start_stack: u64,
        arg_start: u64,
        arg_end: u64,
        env_start: u64,
        env_end: u64,
        auxv: *u64,
        auxv_size: u32,
        exe_fd: u32,
    };

    pub const NETLINK = struct {
        /// Routing/device hook
        pub const ROUTE = 0;

        /// Unused number
        pub const UNUSED = 1;

        /// Reserved for user mode socket protocols
        pub const USERSOCK = 2;

        /// Unused number, formerly ip_queue
        pub const FIREWALL = 3;

        /// socket monitoring
        pub const SOCK_DIAG = 4;

        /// netfilter/iptables ULOG
        pub const NFLOG = 5;

        /// ipsec
        pub const XFRM = 6;

        /// SELinux event notifications
        pub const SELINUX = 7;

        /// Open-iSCSI
        pub const ISCSI = 8;

        /// auditing
        pub const AUDIT = 9;

        pub const FIB_LOOKUP = 10;

        pub const CONNECTOR = 11;

        /// netfilter subsystem
        pub const NETFILTER = 12;

        pub const IP6_FW = 13;

        /// DECnet routing messages
        pub const DNRTMSG = 14;

        /// Kernel messages to userspace
        pub const KOBJECT_UEVENT = 15;

        pub const GENERIC = 16;

        // leave room for NETLINK_DM (DM Events)

        /// SCSI Transports
        pub const SCSITRANSPORT = 18;

        pub const ECRYPTFS = 19;

        pub const RDMA = 20;

        /// Crypto layer
        pub const CRYPTO = 21;

        /// SMC monitoring
        pub const SMC = 22;
    };

    // Flags values

    /// It is request message.
    pub const NLM_F_REQUEST = 0x01;

    /// Multipart message, terminated by NLMSG_DONE
    pub const NLM_F_MULTI = 0x02;

    /// Reply with ack, with zero or error code
    pub const NLM_F_ACK = 0x04;

    /// Echo this request
    pub const NLM_F_ECHO = 0x08;

    /// Dump was inconsistent due to sequence change
    pub const NLM_F_DUMP_INTR = 0x10;

    /// Dump was filtered as requested
    pub const NLM_F_DUMP_FILTERED = 0x20;

    // Modifiers to GET request

    /// specify tree root
    pub const NLM_F_ROOT = 0x100;

    /// return all matching
    pub const NLM_F_MATCH = 0x200;

    /// atomic GET
    pub const NLM_F_ATOMIC = 0x400;
    pub const NLM_F_DUMP = NLM_F_ROOT | NLM_F_MATCH;

    // Modifiers to NEW request

    /// Override existing
    pub const NLM_F_REPLACE = 0x100;

    /// Do not touch, if it exists
    pub const NLM_F_EXCL = 0x200;

    /// Create, if it does not exist
    pub const NLM_F_CREATE = 0x400;

    /// Add to end of list
    pub const NLM_F_APPEND = 0x800;

    // Modifiers to DELETE request

    /// Do not delete recursively
    pub const NLM_F_NONREC = 0x100;

    // Flags for ACK message

    /// request was capped
    pub const NLM_F_CAPPED = 0x100;

    /// extended ACK TVLs were included
    pub const NLM_F_ACK_TLVS = 0x200;

    pub const NetlinkMessageType = enum(u16) {
        /// < 0x10: reserved control messages
        pub const MIN_TYPE = 0x10;

        /// Nothing.
        NOOP = 0x1,

        /// Error
        ERROR = 0x2,

        /// End of a dump
        DONE = 0x3,

        /// Data lost
        OVERRUN = 0x4,

        // rtlink types

        RTM_NEWLINK = 16,
        RTM_DELLINK,
        RTM_GETLINK,
        RTM_SETLINK,

        RTM_NEWADDR = 20,
        RTM_DELADDR,
        RTM_GETADDR,

        RTM_NEWROUTE = 24,
        RTM_DELROUTE,
        RTM_GETROUTE,

        RTM_NEWNEIGH = 28,
        RTM_DELNEIGH,
        RTM_GETNEIGH,

        RTM_NEWRULE = 32,
        RTM_DELRULE,
        RTM_GETRULE,

        RTM_NEWQDISC = 36,
        RTM_DELQDISC,
        RTM_GETQDISC,

        RTM_NEWTCLASS = 40,
        RTM_DELTCLASS,
        RTM_GETTCLASS,

        RTM_NEWTFILTER = 44,
        RTM_DELTFILTER,
        RTM_GETTFILTER,

        RTM_NEWACTION = 48,
        RTM_DELACTION,
        RTM_GETACTION,

        RTM_NEWPREFIX = 52,

        RTM_GETMULTICAST = 58,

        RTM_GETANYCAST = 62,

        RTM_NEWNEIGHTBL = 64,
        RTM_GETNEIGHTBL = 66,
        RTM_SETNEIGHTBL,

        RTM_NEWNDUSEROPT = 68,

        RTM_NEWADDRLABEL = 72,
        RTM_DELADDRLABEL,
        RTM_GETADDRLABEL,

        RTM_GETDCB = 78,
        RTM_SETDCB,

        RTM_NEWNETCONF = 80,
        RTM_DELNETCONF,
        RTM_GETNETCONF = 82,

        RTM_NEWMDB = 84,
        RTM_DELMDB = 85,
        RTM_GETMDB = 86,

        RTM_NEWNSID = 88,
        RTM_DELNSID = 89,
        RTM_GETNSID = 90,

        RTM_NEWSTATS = 92,
        RTM_GETSTATS = 94,

        RTM_NEWCACHEREPORT = 96,

        RTM_NEWCHAIN = 100,
        RTM_DELCHAIN,
        RTM_GETCHAIN,

        RTM_NEWNEXTHOP = 104,
        RTM_DELNEXTHOP,
        RTM_GETNEXTHOP,

        _,
    };

    /// Netlink message header
    /// Specified in RFC 3549 Section 2.3.2
    pub const nlmsghdr = extern struct {
        /// Length of message including header
        len: u32,

        /// Message content
        @"type": NetlinkMessageType,

        /// Additional flags
        flags: u16,

        /// Sequence number
        seq: u32,

        /// Sending process port ID
        pid: u32,
    };

    pub const ifinfomsg = extern struct {
        family: u8,
        __pad1: u8 = 0,

        /// ARPHRD_*
        @"type": c_ushort,

        /// Link index
        index: c_int,

        /// IFF_* flags
        flags: c_uint,

        /// IFF_* change mask
        change: c_uint,
    };

    pub const rtattr = extern struct {
        /// Length of option
        len: c_ushort,

        /// Type of option
        @"type": IFLA,

        pub const ALIGNTO = 4;
    };

    pub const IFLA = enum(c_ushort) {
        UNSPEC,
        ADDRESS,
        BROADCAST,
        IFNAME,
        MTU,
        LINK,
        QDISC,
        STATS,
        COST,
        PRIORITY,
        MASTER,

        /// Wireless Extension event
        WIRELESS,

        /// Protocol specific information for a link
        PROTINFO,

        TXQLEN,
        MAP,
        WEIGHT,
        OPERSTATE,
        LINKMODE,
        LINKINFO,
        NET_NS_PID,
        IFALIAS,

        /// Number of VFs if device is SR-IOV PF
        NUM_VF,

        VFINFO_LIST,
        STATS64,
        VF_PORTS,
        PORT_SELF,
        AF_SPEC,

        /// Group the device belongs to
        GROUP,

        NET_NS_FD,

        /// Extended info mask, VFs, etc
        EXT_MASK,

        /// Promiscuity count: > 0 means acts PROMISC
        PROMISCUITY,

        NUM_TX_QUEUES,
        NUM_RX_QUEUES,
        CARRIER,
        PHYS_PORT_ID,
        CARRIER_CHANGES,
        PHYS_SWITCH_ID,
        LINK_NETNSID,
        PHYS_PORT_NAME,
        PROTO_DOWN,
        GSO_MAX_SEGS,
        GSO_MAX_SIZE,
        PAD,
        XDP,
        EVENT,

        NEW_NETNSID,
        IF_NETNSID,

        CARRIER_UP_COUNT,
        CARRIER_DOWN_COUNT,
        NEW_IFINDEX,
        MIN_MTU,
        MAX_MTU,

        _,

        pub const TARGET_NETNSID: IFLA = .IF_NETNSID;
    };

    pub const rtnl_link_ifmap = extern struct {
        mem_start: u64,
        mem_end: u64,
        base_addr: u64,
        irq: u16,
        dma: u8,
        port: u8,
    };

    pub const rtnl_link_stats = extern struct {
        /// total packets received
        rx_packets: u32,

        /// total packets transmitted
        tx_packets: u32,

        /// total bytes received
        rx_bytes: u32,

        /// total bytes transmitted
        tx_bytes: u32,

        /// bad packets received
        rx_errors: u32,

        /// packet transmit problems
        tx_errors: u32,

        /// no space in linux buffers
        rx_dropped: u32,

        /// no space available in linux
        tx_dropped: u32,

        /// multicast packets received
        multicast: u32,

        collisions: u32,

        // detailed rx_errors

        rx_length_errors: u32,

        /// receiver ring buff overflow
        rx_over_errors: u32,

        /// recved pkt with crc error
        rx_crc_errors: u32,

        /// recv'd frame alignment error
        rx_frame_errors: u32,

        /// recv'r fifo overrun
        rx_fifo_errors: u32,

        /// receiver missed packet
        rx_missed_errors: u32,

        // detailed tx_errors

        tx_aborted_errors: u32,
        tx_carrier_errors: u32,
        tx_fifo_errors: u32,
        tx_heartbeat_errors: u32,
        tx_window_errors: u32,

        // for cslip etc

        rx_compressed: u32,
        tx_compressed: u32,

        /// dropped, no handler found
        rx_nohandler: u32,
    };

    pub const rtnl_link_stats64 = extern struct {
        /// total packets received
        rx_packets: u64,

        /// total packets transmitted
        tx_packets: u64,

        /// total bytes received
        rx_bytes: u64,

        /// total bytes transmitted
        tx_bytes: u64,

        /// bad packets received
        rx_errors: u64,

        /// packet transmit problems
        tx_errors: u64,

        /// no space in linux buffers
        rx_dropped: u64,

        /// no space available in linux
        tx_dropped: u64,

        /// multicast packets received
        multicast: u64,

        collisions: u64,

        // detailed rx_errors

        rx_length_errors: u64,

        /// receiver ring buff overflow
        rx_over_errors: u64,

        /// recved pkt with crc error
        rx_crc_errors: u64,

        /// recv'd frame alignment error
        rx_frame_errors: u64,

        /// recv'r fifo overrun
        rx_fifo_errors: u64,

        /// receiver missed packet
        rx_missed_errors: u64,

        // detailed tx_errors

        tx_aborted_errors: u64,
        tx_carrier_errors: u64,
        tx_fifo_errors: u64,
        tx_heartbeat_errors: u64,
        tx_window_errors: u64,

        // for cslip etc

        rx_compressed: u64,
        tx_compressed: u64,

        /// dropped, no handler found
        rx_nohandler: u64,
    };

    pub const perf_event_attr = extern struct {
        /// Major type: hardware/software/tracepoint/etc.
        type: PERF.TYPE = undefined,
        /// Size of the attr structure, for fwd/bwd compat.
        size: u32 = @sizeOf(perf_event_attr),
        /// Type specific configuration information.
        config: u64 = 0,

        sample_period_or_freq: u64 = 0,
        sample_type: u64 = 0,
        read_format: u64 = 0,

        flags: packed struct {
            /// off by default
            disabled: bool = false,
            /// children inherit it
            inherit: bool = false,
            /// must always be on PMU
            pinned: bool = false,
            /// only group on PMU
            exclusive: bool = false,
            /// don't count user
            exclude_user: bool = false,
            /// ditto kernel
            exclude_kernel: bool = false,
            /// ditto hypervisor
            exclude_hv: bool = false,
            /// don't count when idle
            exclude_idle: bool = false,
            /// include mmap data
            mmap: bool = false,
            /// include comm data
            comm: bool = false,
            /// use freq, not period
            freq: bool = false,
            /// per task counts
            inherit_stat: bool = false,
            /// next exec enables
            enable_on_exec: bool = false,
            /// trace fork/exit
            task: bool = false,
            /// wakeup_watermark
            watermark: bool = false,
            /// precise_ip:
            ///
            ///  0 - SAMPLE_IP can have arbitrary skid
            ///  1 - SAMPLE_IP must have constant skid
            ///  2 - SAMPLE_IP requested to have 0 skid
            ///  3 - SAMPLE_IP must have 0 skid
            ///
            ///  See also PERF_RECORD_MISC_EXACT_IP
            /// skid constraint
            precise_ip: u2 = 0,
            /// non-exec mmap data
            mmap_data: bool = false,
            /// sample_type all events
            sample_id_all: bool = false,

            /// don't count in host
            exclude_host: bool = false,
            /// don't count in guest
            exclude_guest: bool = false,

            /// exclude kernel callchains
            exclude_callchain_kernel: bool = false,
            /// exclude user callchains
            exclude_callchain_user: bool = false,
            /// include mmap with inode data
            mmap2: bool = false,
            /// flag comm events that are due to an exec
            comm_exec: bool = false,
            /// use @clockid for time fields
            use_clockid: bool = false,
            /// context switch data
            context_switch: bool = false,
            /// Write ring buffer from end to beginning
            write_backward: bool = false,
            /// include namespaces data
            namespaces: bool = false,

            __reserved_1: u35 = 0,
        } = .{},
        /// wakeup every n events, or
        /// bytes before wakeup
        wakeup_events_or_watermark: u32 = 0,

        bp_type: u32 = 0,

        /// This field is also used for:
        /// bp_addr
        /// kprobe_func for perf_kprobe
        /// uprobe_path for perf_uprobe
        config1: u64 = 0,
        /// This field is also used for:
        /// bp_len
        /// kprobe_addr when kprobe_func == null
        /// probe_offset for perf_[k,u]probe
        config2: u64 = 0,

        /// enum perf_branch_sample_type
        branch_sample_type: u64 = 0,

        /// Defines set of user regs to dump on samples.
        /// See asm/perf_regs.h for details.
        sample_regs_user: u64 = 0,

        /// Defines size of the user stack to dump on samples.
        sample_stack_user: u32 = 0,

        clockid: i32 = 0,
        /// Defines set of regs to dump for each sample
        /// state captured on:
        ///  - precise = 0: PMU interrupt
        ///  - precise > 0: sampled instruction
        ///
        /// See asm/perf_regs.h for details.
        sample_regs_intr: u64 = 0,

        /// Wakeup watermark for AUX area
        aux_watermark: u32 = 0,
        sample_max_stack: u16 = 0,
        /// Align to u64
        __reserved_2: u16 = 0,
    };

    pub const PERF = struct {
        pub const TYPE = enum(u32) {
            HARDWARE,
            SOFTWARE,
            TRACEPOINT,
            HW_CACHE,
            RAW,
            BREAKPOINT,
            MAX,
        };

        pub const COUNT = struct {
            pub const HW = enum(u32) {
                CPU_CYCLES,
                INSTRUCTIONS,
                CACHE_REFERENCES,
                CACHE_MISSES,
                BRANCH_INSTRUCTIONS,
                BRANCH_MISSES,
                BUS_CYCLES,
                STALLED_CYCLES_FRONTEND,
                STALLED_CYCLES_BACKEND,
                REF_CPU_CYCLES,
                MAX,

                pub const CACHE = enum(u32) {
                    L1D,
                    L1I,
                    LL,
                    DTLB,
                    ITLB,
                    BPU,
                    NODE,
                    MAX,

                    pub const OP = enum(u32) {
                        READ,
                        WRITE,
                        PREFETCH,
                        MAX,
                    };

                    pub const RESULT = enum(u32) {
                        ACCESS,
                        MISS,
                        MAX,
                    };
                };
            };

            pub const SW = enum(u32) {
                CPU_CLOCK,
                TASK_CLOCK,
                PAGE_FAULTS,
                CONTEXT_SWITCHES,
                CPU_MIGRATIONS,
                PAGE_FAULTS_MIN,
                PAGE_FAULTS_MAJ,
                ALIGNMENT_FAULTS,
                EMULATION_FAULTS,
                DUMMY,
                BPF_OUTPUT,
                MAX,
            };
        };

        pub const SAMPLE = struct {
            pub const IP = 1;
            pub const TID = 2;
            pub const TIME = 4;
            pub const ADDR = 8;
            pub const READ = 16;
            pub const CALLCHAIN = 32;
            pub const ID = 64;
            pub const CPU = 128;
            pub const PERIOD = 256;
            pub const STREAM_ID = 512;
            pub const RAW = 1024;
            pub const BRANCH_STACK = 2048;
            pub const REGS_USER = 4096;
            pub const STACK_USER = 8192;
            pub const WEIGHT = 16384;
            pub const DATA_SRC = 32768;
            pub const IDENTIFIER = 65536;
            pub const TRANSACTION = 131072;
            pub const REGS_INTR = 262144;
            pub const PHYS_ADDR = 524288;
            pub const MAX = 1048576;

            pub const BRANCH = struct {
                pub const USER = 1 << 0;
                pub const KERNEL = 1 << 1;
                pub const HV = 1 << 2;
                pub const ANY = 1 << 3;
                pub const ANY_CALL = 1 << 4;
                pub const ANY_RETURN = 1 << 5;
                pub const IND_CALL = 1 << 6;
                pub const ABORT_TX = 1 << 7;
                pub const IN_TX = 1 << 8;
                pub const NO_TX = 1 << 9;
                pub const COND = 1 << 10;
                pub const CALL_STACK = 1 << 11;
                pub const IND_JUMP = 1 << 12;
                pub const CALL = 1 << 13;
                pub const NO_FLAGS = 1 << 14;
                pub const NO_CYCLES = 1 << 15;
                pub const TYPE_SAVE = 1 << 16;
                pub const MAX = 1 << 17;
            };
        };

        pub const FLAG = struct {
            pub const FD_NO_GROUP = 1 << 0;
            pub const FD_OUTPUT = 1 << 1;
            pub const PID_CGROUP = 1 << 2;
            pub const FD_CLOEXEC = 1 << 3;
        };

        pub const EVENT_IOC = struct {
            pub const ENABLE = 9216;
            pub const DISABLE = 9217;
            pub const REFRESH = 9218;
            pub const RESET = 9219;
            pub const PERIOD = 1074275332;
            pub const SET_OUTPUT = 9221;
            pub const SET_FILTER = 1074275334;
            pub const SET_BPF = 1074013192;
            pub const PAUSE_OUTPUT = 1074013193;
            pub const QUERY_BPF = 3221758986;
            pub const MODIFY_ATTRIBUTES = 1074275339;
        };

        pub const IOC_FLAG_GROUP = 1;
    };

    // TODO: Add the rest of the AUDIT defines?

    pub const AUDIT = struct {
        pub const ARCH = enum(u32) {
            const @"64BIT" = 0x80000000;
            const LE = 0x40000000;

            pub const current: AUDIT.ARCH = switch (native_arch) {
                .i386 => .I386,
                .x86_64 => .X86_64,
                .aarch64 => .AARCH64,
                .arm, .thumb => .ARM,
                .riscv64 => .RISCV64,
                .sparc64 => .SPARC64,
                .mips => .MIPS,
                .mipsel => .MIPSEL,
                .powerpc => .PPC,
                .powerpc64 => .PPC64,
                .powerpc64le => .PPC64LE,
                else => @compileError("unsupported architecture"),
            };

            AARCH64 = toAudit(.aarch64),
            ARM = toAudit(.arm),
            ARMEB = toAudit(.armeb),
            CSKY = toAudit(.csky),
            HEXAGON = @enumToInt(std.elf.EM.HEXAGON),
            I386 = toAudit(.i386),
            M68K = toAudit(.m68k),
            MIPS = toAudit(.mips),
            MIPSEL = toAudit(.mips) | LE,
            MIPS64 = toAudit(.mips64),
            MIPSEL64 = toAudit(.mips64) | LE,
            PPC = toAudit(.powerpc),
            PPC64 = toAudit(.powerpc64),
            PPC64LE = toAudit(.powerpc64le),
            RISCV32 = toAudit(.riscv32),
            RISCV64 = toAudit(.riscv64),
            S390X = toAudit(.s390x),
            SPARC = toAudit(.sparc),
            SPARC64 = toAudit(.sparc64),
            X86_64 = toAudit(.x86_64),

            fn toAudit(arch: std.Target.Cpu.Arch) u32 {
                var res: u32 = @enumToInt(arch.toElfMachine());
                if (arch.endian() == .Little) res |= LE;
                if (arch.ptrBitWidth() == 64) res |= @"64BIT";

                return res;
            }
        };
    };