    //! This file is auto-generated by tools/update_cpu_features.zig.

    const std = @import("../std.zig");
    const CpuFeature = std.Target.Cpu.Feature;
    const CpuModel = std.Target.Cpu.Model;

    pub const Feature = enum {
        addsubiw,
        avr0,
        avr1,
        avr2,
        avr25,
        avr3,
        avr31,
        avr35,
        avr4,
        avr5,
        avr51,
        avr6,
        avrtiny,
        @"break",
        des,
        eijmpcall,
        elpm,
        elpmx,
        ijmpcall,
        jmpcall,
        lpm,
        lpmx,
        memmappedregs,
        movw,
        mul,
        rmw,
        smallstack,
        special,
        spm,
        spmx,
        sram,
        tinyencoding,
        xmega,
        xmega3,
        xmegau,
    };

    pub const featureSet = CpuFeature.feature_set_fns(Feature).featureSet;
    pub const featureSetHas = CpuFeature.feature_set_fns(Feature).featureSetHas;
    pub const featureSetHasAny = CpuFeature.feature_set_fns(Feature).featureSetHasAny;
    pub const featureSetHasAll = CpuFeature.feature_set_fns(Feature).featureSetHasAll;

    pub const all_features = blk: {
        const len = @typeInfo(Feature).Enum.fields.len;
        std.debug.assert(len <= CpuFeature.Set.needed_bit_count);
        var result: [len]CpuFeature = undefined;
        result[@enumToInt(Feature.addsubiw)] = .{
            .llvm_name = "addsubiw",
            .description = "Enable 16-bit register-immediate addition and subtraction instructions",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.avr0)] = .{
            .llvm_name = "avr0",
            .description = "The device is a part of the avr0 family",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.avr1)] = .{
            .llvm_name = "avr1",
            .description = "The device is a part of the avr1 family",
            .dependencies = featureSet(&[_]Feature{
                .avr0,
                .lpm,
                .memmappedregs,
            }),
        };
        result[@enumToInt(Feature.avr2)] = .{
            .llvm_name = "avr2",
            .description = "The device is a part of the avr2 family",
            .dependencies = featureSet(&[_]Feature{
                .addsubiw,
                .avr1,
                .ijmpcall,
                .sram,
            }),
        };
        result[@enumToInt(Feature.avr25)] = .{
            .llvm_name = "avr25",
            .description = "The device is a part of the avr25 family",
            .dependencies = featureSet(&[_]Feature{
                .avr2,
                .@"break",
                .lpmx,
                .movw,
                .spm,
            }),
        };
        result[@enumToInt(Feature.avr3)] = .{
            .llvm_name = "avr3",
            .description = "The device is a part of the avr3 family",
            .dependencies = featureSet(&[_]Feature{
                .avr2,
                .jmpcall,
            }),
        };
        result[@enumToInt(Feature.avr31)] = .{
            .llvm_name = "avr31",
            .description = "The device is a part of the avr31 family",
            .dependencies = featureSet(&[_]Feature{
                .avr3,
                .elpm,
            }),
        };
        result[@enumToInt(Feature.avr35)] = .{
            .llvm_name = "avr35",
            .description = "The device is a part of the avr35 family",
            .dependencies = featureSet(&[_]Feature{
                .avr3,
                .@"break",
                .lpmx,
                .movw,
                .spm,
            }),
        };
        result[@enumToInt(Feature.avr4)] = .{
            .llvm_name = "avr4",
            .description = "The device is a part of the avr4 family",
            .dependencies = featureSet(&[_]Feature{
                .avr2,
                .@"break",
                .lpmx,
                .movw,
                .mul,
                .spm,
            }),
        };
        result[@enumToInt(Feature.avr5)] = .{
            .llvm_name = "avr5",
            .description = "The device is a part of the avr5 family",
            .dependencies = featureSet(&[_]Feature{
                .avr3,
                .@"break",
                .lpmx,
                .movw,
                .mul,
                .spm,
            }),
        };
        result[@enumToInt(Feature.avr51)] = .{
            .llvm_name = "avr51",
            .description = "The device is a part of the avr51 family",
            .dependencies = featureSet(&[_]Feature{
                .avr5,
                .elpm,
                .elpmx,
            }),
        };
        result[@enumToInt(Feature.avr6)] = .{
            .llvm_name = "avr6",
            .description = "The device is a part of the avr6 family",
            .dependencies = featureSet(&[_]Feature{
                .avr51,
            }),
        };
        result[@enumToInt(Feature.avrtiny)] = .{
            .llvm_name = "avrtiny",
            .description = "The device is a part of the avrtiny family",
            .dependencies = featureSet(&[_]Feature{
                .avr0,
                .@"break",
                .smallstack,
                .sram,
                .tinyencoding,
            }),
        };
        result[@enumToInt(Feature.@"break")] = .{
            .llvm_name = "break",
            .description = "The device supports the `BREAK` debugging instruction",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.des)] = .{
            .llvm_name = "des",
            .description = "The device supports the `DES k` encryption instruction",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.eijmpcall)] = .{
            .llvm_name = "eijmpcall",
            .description = "The device supports the `EIJMP`/`EICALL` instructions",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.elpm)] = .{
            .llvm_name = "elpm",
            .description = "The device supports the ELPM instruction",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.elpmx)] = .{
            .llvm_name = "elpmx",
            .description = "The device supports the `ELPM Rd, Z[+]` instructions",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.ijmpcall)] = .{
            .llvm_name = "ijmpcall",
            .description = "The device supports `IJMP`/`ICALL`instructions",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.jmpcall)] = .{
            .llvm_name = "jmpcall",
            .description = "The device supports the `JMP` and `CALL` instructions",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.lpm)] = .{
            .llvm_name = "lpm",
            .description = "The device supports the `LPM` instruction",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.lpmx)] = .{
            .llvm_name = "lpmx",
            .description = "The device supports the `LPM Rd, Z[+]` instruction",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.memmappedregs)] = .{
            .llvm_name = "memmappedregs",
            .description = "The device has CPU registers mapped in data address space",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.movw)] = .{
            .llvm_name = "movw",
            .description = "The device supports the 16-bit MOVW instruction",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.mul)] = .{
            .llvm_name = "mul",
            .description = "The device supports the multiplication instructions",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.rmw)] = .{
            .llvm_name = "rmw",
            .description = "The device supports the read-write-modify instructions: XCH, LAS, LAC, LAT",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.smallstack)] = .{
            .llvm_name = "smallstack",
            .description = "The device has an 8-bit stack pointer",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.special)] = .{
            .llvm_name = "special",
            .description = "Enable use of the entire instruction set - used for debugging",
            .dependencies = featureSet(&[_]Feature{
                .addsubiw,
                .@"break",
                .des,
                .eijmpcall,
                .elpm,
                .elpmx,
                .ijmpcall,
                .jmpcall,
                .lpm,
                .lpmx,
                .memmappedregs,
                .movw,
                .mul,
                .rmw,
                .spm,
                .spmx,
                .sram,
            }),
        };
        result[@enumToInt(Feature.spm)] = .{
            .llvm_name = "spm",
            .description = "The device supports the `SPM` instruction",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.spmx)] = .{
            .llvm_name = "spmx",
            .description = "The device supports the `SPM Z+` instruction",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.sram)] = .{
            .llvm_name = "sram",
            .description = "The device has random access memory",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.tinyencoding)] = .{
            .llvm_name = "tinyencoding",
            .description = "The device has Tiny core specific instruction encodings",
            .dependencies = featureSet(&[_]Feature{}),
        };
        result[@enumToInt(Feature.xmega)] = .{
            .llvm_name = "xmega",
            .description = "The device is a part of the xmega family",
            .dependencies = featureSet(&[_]Feature{
                .addsubiw,
                .avr0,
                .@"break",
                .des,
                .eijmpcall,
                .elpm,
                .elpmx,
                .ijmpcall,
                .jmpcall,
                .lpm,
                .lpmx,
                .movw,
                .mul,
                .spm,
                .spmx,
                .sram,
            }),
        };
        result[@enumToInt(Feature.xmega3)] = .{
            .llvm_name = "xmega3",
            .description = "The device is a part of the xmega3 family",
            .dependencies = featureSet(&[_]Feature{
                .addsubiw,
                .avr0,
                .@"break",
                .ijmpcall,
                .jmpcall,
                .lpm,
                .lpmx,
                .movw,
                .mul,
                .sram,
            }),
        };
        result[@enumToInt(Feature.xmegau)] = .{
            .llvm_name = "xmegau",
            .description = "The device is a part of the xmegau family",
            .dependencies = featureSet(&[_]Feature{
                .rmw,
                .xmega,
            }),
        };
        const ti = @typeInfo(Feature);
        for (result) |*elem, i| {
            elem.index = i;
            elem.name = ti.Enum.fields[i].name;
        }
        break :blk result;
    };

    pub const cpu = struct {
        pub const at43usb320 = CpuModel{
            .name = "at43usb320",
            .llvm_name = "at43usb320",
            .features = featureSet(&[_]Feature{
                .avr31,
            }),
        };
        pub const at43usb355 = CpuModel{
            .name = "at43usb355",
            .llvm_name = "at43usb355",
            .features = featureSet(&[_]Feature{
                .avr3,
            }),
        };
        pub const at76c711 = CpuModel{
            .name = "at76c711",
            .llvm_name = "at76c711",
            .features = featureSet(&[_]Feature{
                .avr3,
            }),
        };
        pub const at86rf401 = CpuModel{
            .name = "at86rf401",
            .llvm_name = "at86rf401",
            .features = featureSet(&[_]Feature{
                .avr2,
                .lpmx,
                .movw,
            }),
        };
        pub const at90c8534 = CpuModel{
            .name = "at90c8534",
            .llvm_name = "at90c8534",
            .features = featureSet(&[_]Feature{
                .avr2,
            }),
        };
        pub const at90can128 = CpuModel{
            .name = "at90can128",
            .llvm_name = "at90can128",
            .features = featureSet(&[_]Feature{
                .avr51,
            }),
        };
        pub const at90can32 = CpuModel{
            .name = "at90can32",
            .llvm_name = "at90can32",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const at90can64 = CpuModel{
            .name = "at90can64",
            .llvm_name = "at90can64",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const at90pwm1 = CpuModel{
            .name = "at90pwm1",
            .llvm_name = "at90pwm1",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const at90pwm161 = CpuModel{
            .name = "at90pwm161",
            .llvm_name = "at90pwm161",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const at90pwm2 = CpuModel{
            .name = "at90pwm2",
            .llvm_name = "at90pwm2",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const at90pwm216 = CpuModel{
            .name = "at90pwm216",
            .llvm_name = "at90pwm216",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const at90pwm2b = CpuModel{
            .name = "at90pwm2b",
            .llvm_name = "at90pwm2b",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const at90pwm3 = CpuModel{
            .name = "at90pwm3",
            .llvm_name = "at90pwm3",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const at90pwm316 = CpuModel{
            .name = "at90pwm316",
            .llvm_name = "at90pwm316",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const at90pwm3b = CpuModel{
            .name = "at90pwm3b",
            .llvm_name = "at90pwm3b",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const at90pwm81 = CpuModel{
            .name = "at90pwm81",
            .llvm_name = "at90pwm81",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const at90s1200 = CpuModel{
            .name = "at90s1200",
            .llvm_name = "at90s1200",
            .features = featureSet(&[_]Feature{
                .avr0,
                .smallstack,
            }),
        };
        pub const at90s2313 = CpuModel{
            .name = "at90s2313",
            .llvm_name = "at90s2313",
            .features = featureSet(&[_]Feature{
                .avr2,
                .smallstack,
            }),
        };
        pub const at90s2323 = CpuModel{
            .name = "at90s2323",
            .llvm_name = "at90s2323",
            .features = featureSet(&[_]Feature{
                .avr2,
                .smallstack,
            }),
        };
        pub const at90s2333 = CpuModel{
            .name = "at90s2333",
            .llvm_name = "at90s2333",
            .features = featureSet(&[_]Feature{
                .avr2,
                .smallstack,
            }),
        };
        pub const at90s2343 = CpuModel{
            .name = "at90s2343",
            .llvm_name = "at90s2343",
            .features = featureSet(&[_]Feature{
                .avr2,
                .smallstack,
            }),
        };
        pub const at90s4414 = CpuModel{
            .name = "at90s4414",
            .llvm_name = "at90s4414",
            .features = featureSet(&[_]Feature{
                .avr2,
                .smallstack,
            }),
        };
        pub const at90s4433 = CpuModel{
            .name = "at90s4433",
            .llvm_name = "at90s4433",
            .features = featureSet(&[_]Feature{
                .avr2,
                .smallstack,
            }),
        };
        pub const at90s4434 = CpuModel{
            .name = "at90s4434",
            .llvm_name = "at90s4434",
            .features = featureSet(&[_]Feature{
                .avr2,
                .smallstack,
            }),
        };
        pub const at90s8515 = CpuModel{
            .name = "at90s8515",
            .llvm_name = "at90s8515",
            .features = featureSet(&[_]Feature{
                .avr2,
            }),
        };
        pub const at90s8535 = CpuModel{
            .name = "at90s8535",
            .llvm_name = "at90s8535",
            .features = featureSet(&[_]Feature{
                .avr2,
            }),
        };
        pub const at90scr100 = CpuModel{
            .name = "at90scr100",
            .llvm_name = "at90scr100",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const at90usb1286 = CpuModel{
            .name = "at90usb1286",
            .llvm_name = "at90usb1286",
            .features = featureSet(&[_]Feature{
                .avr51,
            }),
        };
        pub const at90usb1287 = CpuModel{
            .name = "at90usb1287",
            .llvm_name = "at90usb1287",
            .features = featureSet(&[_]Feature{
                .avr51,
            }),
        };
        pub const at90usb162 = CpuModel{
            .name = "at90usb162",
            .llvm_name = "at90usb162",
            .features = featureSet(&[_]Feature{
                .avr35,
            }),
        };
        pub const at90usb646 = CpuModel{
            .name = "at90usb646",
            .llvm_name = "at90usb646",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const at90usb647 = CpuModel{
            .name = "at90usb647",
            .llvm_name = "at90usb647",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const at90usb82 = CpuModel{
            .name = "at90usb82",
            .llvm_name = "at90usb82",
            .features = featureSet(&[_]Feature{
                .avr35,
            }),
        };
        pub const at94k = CpuModel{
            .name = "at94k",
            .llvm_name = "at94k",
            .features = featureSet(&[_]Feature{
                .avr3,
                .lpmx,
                .movw,
                .mul,
            }),
        };
        pub const ata5272 = CpuModel{
            .name = "ata5272",
            .llvm_name = "ata5272",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const ata5505 = CpuModel{
            .name = "ata5505",
            .llvm_name = "ata5505",
            .features = featureSet(&[_]Feature{
                .avr35,
            }),
        };
        pub const ata5702m322 = CpuModel{
            .name = "ata5702m322",
            .llvm_name = "ata5702m322",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const ata5782 = CpuModel{
            .name = "ata5782",
            .llvm_name = "ata5782",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const ata5790 = CpuModel{
            .name = "ata5790",
            .llvm_name = "ata5790",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const ata5790n = CpuModel{
            .name = "ata5790n",
            .llvm_name = "ata5790n",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const ata5791 = CpuModel{
            .name = "ata5791",
            .llvm_name = "ata5791",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const ata5795 = CpuModel{
            .name = "ata5795",
            .llvm_name = "ata5795",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const ata5831 = CpuModel{
            .name = "ata5831",
            .llvm_name = "ata5831",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const ata6285 = CpuModel{
            .name = "ata6285",
            .llvm_name = "ata6285",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const ata6286 = CpuModel{
            .name = "ata6286",
            .llvm_name = "ata6286",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const ata6289 = CpuModel{
            .name = "ata6289",
            .llvm_name = "ata6289",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const ata6612c = CpuModel{
            .name = "ata6612c",
            .llvm_name = "ata6612c",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const ata6613c = CpuModel{
            .name = "ata6613c",
            .llvm_name = "ata6613c",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const ata6614q = CpuModel{
            .name = "ata6614q",
            .llvm_name = "ata6614q",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const ata6616c = CpuModel{
            .name = "ata6616c",
            .llvm_name = "ata6616c",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const ata6617c = CpuModel{
            .name = "ata6617c",
            .llvm_name = "ata6617c",
            .features = featureSet(&[_]Feature{
                .avr35,
            }),
        };
        pub const ata664251 = CpuModel{
            .name = "ata664251",
            .llvm_name = "ata664251",
            .features = featureSet(&[_]Feature{
                .avr35,
            }),
        };
        pub const ata8210 = CpuModel{
            .name = "ata8210",
            .llvm_name = "ata8210",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const ata8510 = CpuModel{
            .name = "ata8510",
            .llvm_name = "ata8510",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega103 = CpuModel{
            .name = "atmega103",
            .llvm_name = "atmega103",
            .features = featureSet(&[_]Feature{
                .avr31,
            }),
        };
        pub const atmega128 = CpuModel{
            .name = "atmega128",
            .llvm_name = "atmega128",
            .features = featureSet(&[_]Feature{
                .avr51,
            }),
        };
        pub const atmega1280 = CpuModel{
            .name = "atmega1280",
            .llvm_name = "atmega1280",
            .features = featureSet(&[_]Feature{
                .avr51,
            }),
        };
        pub const atmega1281 = CpuModel{
            .name = "atmega1281",
            .llvm_name = "atmega1281",
            .features = featureSet(&[_]Feature{
                .avr51,
            }),
        };
        pub const atmega1284 = CpuModel{
            .name = "atmega1284",
            .llvm_name = "atmega1284",
            .features = featureSet(&[_]Feature{
                .avr51,
            }),
        };
        pub const atmega1284p = CpuModel{
            .name = "atmega1284p",
            .llvm_name = "atmega1284p",
            .features = featureSet(&[_]Feature{
                .avr51,
            }),
        };
        pub const atmega1284rfr2 = CpuModel{
            .name = "atmega1284rfr2",
            .llvm_name = "atmega1284rfr2",
            .features = featureSet(&[_]Feature{
                .avr51,
            }),
        };
        pub const atmega128a = CpuModel{
            .name = "atmega128a",
            .llvm_name = "atmega128a",
            .features = featureSet(&[_]Feature{
                .avr51,
            }),
        };
        pub const atmega128rfa1 = CpuModel{
            .name = "atmega128rfa1",
            .llvm_name = "atmega128rfa1",
            .features = featureSet(&[_]Feature{
                .avr51,
            }),
        };
        pub const atmega128rfr2 = CpuModel{
            .name = "atmega128rfr2",
            .llvm_name = "atmega128rfr2",
            .features = featureSet(&[_]Feature{
                .avr51,
            }),
        };
        pub const atmega16 = CpuModel{
            .name = "atmega16",
            .llvm_name = "atmega16",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega1608 = CpuModel{
            .name = "atmega1608",
            .llvm_name = "atmega1608",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const atmega1609 = CpuModel{
            .name = "atmega1609",
            .llvm_name = "atmega1609",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const atmega161 = CpuModel{
            .name = "atmega161",
            .llvm_name = "atmega161",
            .features = featureSet(&[_]Feature{
                .avr3,
                .lpmx,
                .movw,
                .mul,
                .spm,
            }),
        };
        pub const atmega162 = CpuModel{
            .name = "atmega162",
            .llvm_name = "atmega162",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega163 = CpuModel{
            .name = "atmega163",
            .llvm_name = "atmega163",
            .features = featureSet(&[_]Feature{
                .avr3,
                .lpmx,
                .movw,
                .mul,
                .spm,
            }),
        };
        pub const atmega164a = CpuModel{
            .name = "atmega164a",
            .llvm_name = "atmega164a",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega164p = CpuModel{
            .name = "atmega164p",
            .llvm_name = "atmega164p",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega164pa = CpuModel{
            .name = "atmega164pa",
            .llvm_name = "atmega164pa",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega165 = CpuModel{
            .name = "atmega165",
            .llvm_name = "atmega165",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega165a = CpuModel{
            .name = "atmega165a",
            .llvm_name = "atmega165a",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega165p = CpuModel{
            .name = "atmega165p",
            .llvm_name = "atmega165p",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega165pa = CpuModel{
            .name = "atmega165pa",
            .llvm_name = "atmega165pa",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega168 = CpuModel{
            .name = "atmega168",
            .llvm_name = "atmega168",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega168a = CpuModel{
            .name = "atmega168a",
            .llvm_name = "atmega168a",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega168p = CpuModel{
            .name = "atmega168p",
            .llvm_name = "atmega168p",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega168pa = CpuModel{
            .name = "atmega168pa",
            .llvm_name = "atmega168pa",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega168pb = CpuModel{
            .name = "atmega168pb",
            .llvm_name = "atmega168pb",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega169 = CpuModel{
            .name = "atmega169",
            .llvm_name = "atmega169",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega169a = CpuModel{
            .name = "atmega169a",
            .llvm_name = "atmega169a",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega169p = CpuModel{
            .name = "atmega169p",
            .llvm_name = "atmega169p",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega169pa = CpuModel{
            .name = "atmega169pa",
            .llvm_name = "atmega169pa",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega16a = CpuModel{
            .name = "atmega16a",
            .llvm_name = "atmega16a",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega16hva = CpuModel{
            .name = "atmega16hva",
            .llvm_name = "atmega16hva",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega16hva2 = CpuModel{
            .name = "atmega16hva2",
            .llvm_name = "atmega16hva2",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega16hvb = CpuModel{
            .name = "atmega16hvb",
            .llvm_name = "atmega16hvb",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega16hvbrevb = CpuModel{
            .name = "atmega16hvbrevb",
            .llvm_name = "atmega16hvbrevb",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega16m1 = CpuModel{
            .name = "atmega16m1",
            .llvm_name = "atmega16m1",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega16u2 = CpuModel{
            .name = "atmega16u2",
            .llvm_name = "atmega16u2",
            .features = featureSet(&[_]Feature{
                .avr35,
            }),
        };
        pub const atmega16u4 = CpuModel{
            .name = "atmega16u4",
            .llvm_name = "atmega16u4",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega2560 = CpuModel{
            .name = "atmega2560",
            .llvm_name = "atmega2560",
            .features = featureSet(&[_]Feature{
                .avr6,
            }),
        };
        pub const atmega2561 = CpuModel{
            .name = "atmega2561",
            .llvm_name = "atmega2561",
            .features = featureSet(&[_]Feature{
                .avr6,
            }),
        };
        pub const atmega2564rfr2 = CpuModel{
            .name = "atmega2564rfr2",
            .llvm_name = "atmega2564rfr2",
            .features = featureSet(&[_]Feature{
                .avr6,
            }),
        };
        pub const atmega256rfr2 = CpuModel{
            .name = "atmega256rfr2",
            .llvm_name = "atmega256rfr2",
            .features = featureSet(&[_]Feature{
                .avr6,
            }),
        };
        pub const atmega32 = CpuModel{
            .name = "atmega32",
            .llvm_name = "atmega32",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega3208 = CpuModel{
            .name = "atmega3208",
            .llvm_name = "atmega3208",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const atmega3209 = CpuModel{
            .name = "atmega3209",
            .llvm_name = "atmega3209",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const atmega323 = CpuModel{
            .name = "atmega323",
            .llvm_name = "atmega323",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega324a = CpuModel{
            .name = "atmega324a",
            .llvm_name = "atmega324a",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega324p = CpuModel{
            .name = "atmega324p",
            .llvm_name = "atmega324p",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega324pa = CpuModel{
            .name = "atmega324pa",
            .llvm_name = "atmega324pa",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega324pb = CpuModel{
            .name = "atmega324pb",
            .llvm_name = "atmega324pb",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega325 = CpuModel{
            .name = "atmega325",
            .llvm_name = "atmega325",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega3250 = CpuModel{
            .name = "atmega3250",
            .llvm_name = "atmega3250",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega3250a = CpuModel{
            .name = "atmega3250a",
            .llvm_name = "atmega3250a",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega3250p = CpuModel{
            .name = "atmega3250p",
            .llvm_name = "atmega3250p",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega3250pa = CpuModel{
            .name = "atmega3250pa",
            .llvm_name = "atmega3250pa",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega325a = CpuModel{
            .name = "atmega325a",
            .llvm_name = "atmega325a",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega325p = CpuModel{
            .name = "atmega325p",
            .llvm_name = "atmega325p",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega325pa = CpuModel{
            .name = "atmega325pa",
            .llvm_name = "atmega325pa",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega328 = CpuModel{
            .name = "atmega328",
            .llvm_name = "atmega328",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega328p = CpuModel{
            .name = "atmega328p",
            .llvm_name = "atmega328p",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega328pb = CpuModel{
            .name = "atmega328pb",
            .llvm_name = "atmega328pb",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega329 = CpuModel{
            .name = "atmega329",
            .llvm_name = "atmega329",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega3290 = CpuModel{
            .name = "atmega3290",
            .llvm_name = "atmega3290",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega3290a = CpuModel{
            .name = "atmega3290a",
            .llvm_name = "atmega3290a",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega3290p = CpuModel{
            .name = "atmega3290p",
            .llvm_name = "atmega3290p",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega3290pa = CpuModel{
            .name = "atmega3290pa",
            .llvm_name = "atmega3290pa",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega329a = CpuModel{
            .name = "atmega329a",
            .llvm_name = "atmega329a",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega329p = CpuModel{
            .name = "atmega329p",
            .llvm_name = "atmega329p",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega329pa = CpuModel{
            .name = "atmega329pa",
            .llvm_name = "atmega329pa",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega32a = CpuModel{
            .name = "atmega32a",
            .llvm_name = "atmega32a",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega32c1 = CpuModel{
            .name = "atmega32c1",
            .llvm_name = "atmega32c1",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega32hvb = CpuModel{
            .name = "atmega32hvb",
            .llvm_name = "atmega32hvb",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega32hvbrevb = CpuModel{
            .name = "atmega32hvbrevb",
            .llvm_name = "atmega32hvbrevb",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega32m1 = CpuModel{
            .name = "atmega32m1",
            .llvm_name = "atmega32m1",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega32u2 = CpuModel{
            .name = "atmega32u2",
            .llvm_name = "atmega32u2",
            .features = featureSet(&[_]Feature{
                .avr35,
            }),
        };
        pub const atmega32u4 = CpuModel{
            .name = "atmega32u4",
            .llvm_name = "atmega32u4",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega32u6 = CpuModel{
            .name = "atmega32u6",
            .llvm_name = "atmega32u6",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega406 = CpuModel{
            .name = "atmega406",
            .llvm_name = "atmega406",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega48 = CpuModel{
            .name = "atmega48",
            .llvm_name = "atmega48",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const atmega4808 = CpuModel{
            .name = "atmega4808",
            .llvm_name = "atmega4808",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const atmega4809 = CpuModel{
            .name = "atmega4809",
            .llvm_name = "atmega4809",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const atmega48a = CpuModel{
            .name = "atmega48a",
            .llvm_name = "atmega48a",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const atmega48p = CpuModel{
            .name = "atmega48p",
            .llvm_name = "atmega48p",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const atmega48pa = CpuModel{
            .name = "atmega48pa",
            .llvm_name = "atmega48pa",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const atmega48pb = CpuModel{
            .name = "atmega48pb",
            .llvm_name = "atmega48pb",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const atmega64 = CpuModel{
            .name = "atmega64",
            .llvm_name = "atmega64",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega640 = CpuModel{
            .name = "atmega640",
            .llvm_name = "atmega640",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega644 = CpuModel{
            .name = "atmega644",
            .llvm_name = "atmega644",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega644a = CpuModel{
            .name = "atmega644a",
            .llvm_name = "atmega644a",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega644p = CpuModel{
            .name = "atmega644p",
            .llvm_name = "atmega644p",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega644pa = CpuModel{
            .name = "atmega644pa",
            .llvm_name = "atmega644pa",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega644rfr2 = CpuModel{
            .name = "atmega644rfr2",
            .llvm_name = "atmega644rfr2",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega645 = CpuModel{
            .name = "atmega645",
            .llvm_name = "atmega645",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega6450 = CpuModel{
            .name = "atmega6450",
            .llvm_name = "atmega6450",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega6450a = CpuModel{
            .name = "atmega6450a",
            .llvm_name = "atmega6450a",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega6450p = CpuModel{
            .name = "atmega6450p",
            .llvm_name = "atmega6450p",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega645a = CpuModel{
            .name = "atmega645a",
            .llvm_name = "atmega645a",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega645p = CpuModel{
            .name = "atmega645p",
            .llvm_name = "atmega645p",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega649 = CpuModel{
            .name = "atmega649",
            .llvm_name = "atmega649",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega6490 = CpuModel{
            .name = "atmega6490",
            .llvm_name = "atmega6490",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega6490a = CpuModel{
            .name = "atmega6490a",
            .llvm_name = "atmega6490a",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega6490p = CpuModel{
            .name = "atmega6490p",
            .llvm_name = "atmega6490p",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega649a = CpuModel{
            .name = "atmega649a",
            .llvm_name = "atmega649a",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega649p = CpuModel{
            .name = "atmega649p",
            .llvm_name = "atmega649p",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega64a = CpuModel{
            .name = "atmega64a",
            .llvm_name = "atmega64a",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega64c1 = CpuModel{
            .name = "atmega64c1",
            .llvm_name = "atmega64c1",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega64hve = CpuModel{
            .name = "atmega64hve",
            .llvm_name = "atmega64hve",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega64hve2 = CpuModel{
            .name = "atmega64hve2",
            .llvm_name = "atmega64hve2",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega64m1 = CpuModel{
            .name = "atmega64m1",
            .llvm_name = "atmega64m1",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega64rfr2 = CpuModel{
            .name = "atmega64rfr2",
            .llvm_name = "atmega64rfr2",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const atmega8 = CpuModel{
            .name = "atmega8",
            .llvm_name = "atmega8",
            .features = featureSet(&[_]Feature{
                .avr2,
                .lpmx,
                .movw,
                .mul,
                .spm,
            }),
        };
        pub const atmega808 = CpuModel{
            .name = "atmega808",
            .llvm_name = "atmega808",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const atmega809 = CpuModel{
            .name = "atmega809",
            .llvm_name = "atmega809",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const atmega8515 = CpuModel{
            .name = "atmega8515",
            .llvm_name = "atmega8515",
            .features = featureSet(&[_]Feature{
                .avr2,
                .lpmx,
                .movw,
                .mul,
                .spm,
            }),
        };
        pub const atmega8535 = CpuModel{
            .name = "atmega8535",
            .llvm_name = "atmega8535",
            .features = featureSet(&[_]Feature{
                .avr2,
                .lpmx,
                .movw,
                .mul,
                .spm,
            }),
        };
        pub const atmega88 = CpuModel{
            .name = "atmega88",
            .llvm_name = "atmega88",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const atmega88a = CpuModel{
            .name = "atmega88a",
            .llvm_name = "atmega88a",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const atmega88p = CpuModel{
            .name = "atmega88p",
            .llvm_name = "atmega88p",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const atmega88pa = CpuModel{
            .name = "atmega88pa",
            .llvm_name = "atmega88pa",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const atmega88pb = CpuModel{
            .name = "atmega88pb",
            .llvm_name = "atmega88pb",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const atmega8a = CpuModel{
            .name = "atmega8a",
            .llvm_name = "atmega8a",
            .features = featureSet(&[_]Feature{
                .avr2,
                .lpmx,
                .movw,
                .mul,
                .spm,
            }),
        };
        pub const atmega8hva = CpuModel{
            .name = "atmega8hva",
            .llvm_name = "atmega8hva",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const atmega8u2 = CpuModel{
            .name = "atmega8u2",
            .llvm_name = "atmega8u2",
            .features = featureSet(&[_]Feature{
                .avr35,
            }),
        };
        pub const attiny10 = CpuModel{
            .name = "attiny10",
            .llvm_name = "attiny10",
            .features = featureSet(&[_]Feature{
                .avrtiny,
            }),
        };
        pub const attiny102 = CpuModel{
            .name = "attiny102",
            .llvm_name = "attiny102",
            .features = featureSet(&[_]Feature{
                .avrtiny,
            }),
        };
        pub const attiny104 = CpuModel{
            .name = "attiny104",
            .llvm_name = "attiny104",
            .features = featureSet(&[_]Feature{
                .avrtiny,
            }),
        };
        pub const attiny11 = CpuModel{
            .name = "attiny11",
            .llvm_name = "attiny11",
            .features = featureSet(&[_]Feature{
                .avr1,
                .smallstack,
            }),
        };
        pub const attiny12 = CpuModel{
            .name = "attiny12",
            .llvm_name = "attiny12",
            .features = featureSet(&[_]Feature{
                .avr1,
                .smallstack,
            }),
        };
        pub const attiny13 = CpuModel{
            .name = "attiny13",
            .llvm_name = "attiny13",
            .features = featureSet(&[_]Feature{
                .avr25,
                .smallstack,
            }),
        };
        pub const attiny13a = CpuModel{
            .name = "attiny13a",
            .llvm_name = "attiny13a",
            .features = featureSet(&[_]Feature{
                .avr25,
                .smallstack,
            }),
        };
        pub const attiny15 = CpuModel{
            .name = "attiny15",
            .llvm_name = "attiny15",
            .features = featureSet(&[_]Feature{
                .avr1,
                .smallstack,
            }),
        };
        pub const attiny1604 = CpuModel{
            .name = "attiny1604",
            .llvm_name = "attiny1604",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny1606 = CpuModel{
            .name = "attiny1606",
            .llvm_name = "attiny1606",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny1607 = CpuModel{
            .name = "attiny1607",
            .llvm_name = "attiny1607",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny1614 = CpuModel{
            .name = "attiny1614",
            .llvm_name = "attiny1614",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny1616 = CpuModel{
            .name = "attiny1616",
            .llvm_name = "attiny1616",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny1617 = CpuModel{
            .name = "attiny1617",
            .llvm_name = "attiny1617",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny1624 = CpuModel{
            .name = "attiny1624",
            .llvm_name = "attiny1624",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny1626 = CpuModel{
            .name = "attiny1626",
            .llvm_name = "attiny1626",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny1627 = CpuModel{
            .name = "attiny1627",
            .llvm_name = "attiny1627",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny1634 = CpuModel{
            .name = "attiny1634",
            .llvm_name = "attiny1634",
            .features = featureSet(&[_]Feature{
                .avr35,
            }),
        };
        pub const attiny167 = CpuModel{
            .name = "attiny167",
            .llvm_name = "attiny167",
            .features = featureSet(&[_]Feature{
                .avr35,
            }),
        };
        pub const attiny20 = CpuModel{
            .name = "attiny20",
            .llvm_name = "attiny20",
            .features = featureSet(&[_]Feature{
                .avrtiny,
            }),
        };
        pub const attiny202 = CpuModel{
            .name = "attiny202",
            .llvm_name = "attiny202",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny204 = CpuModel{
            .name = "attiny204",
            .llvm_name = "attiny204",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny212 = CpuModel{
            .name = "attiny212",
            .llvm_name = "attiny212",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny214 = CpuModel{
            .name = "attiny214",
            .llvm_name = "attiny214",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny22 = CpuModel{
            .name = "attiny22",
            .llvm_name = "attiny22",
            .features = featureSet(&[_]Feature{
                .avr2,
                .smallstack,
            }),
        };
        pub const attiny2313 = CpuModel{
            .name = "attiny2313",
            .llvm_name = "attiny2313",
            .features = featureSet(&[_]Feature{
                .avr25,
                .smallstack,
            }),
        };
        pub const attiny2313a = CpuModel{
            .name = "attiny2313a",
            .llvm_name = "attiny2313a",
            .features = featureSet(&[_]Feature{
                .avr25,
                .smallstack,
            }),
        };
        pub const attiny24 = CpuModel{
            .name = "attiny24",
            .llvm_name = "attiny24",
            .features = featureSet(&[_]Feature{
                .avr25,
                .smallstack,
            }),
        };
        pub const attiny24a = CpuModel{
            .name = "attiny24a",
            .llvm_name = "attiny24a",
            .features = featureSet(&[_]Feature{
                .avr25,
                .smallstack,
            }),
        };
        pub const attiny25 = CpuModel{
            .name = "attiny25",
            .llvm_name = "attiny25",
            .features = featureSet(&[_]Feature{
                .avr25,
                .smallstack,
            }),
        };
        pub const attiny26 = CpuModel{
            .name = "attiny26",
            .llvm_name = "attiny26",
            .features = featureSet(&[_]Feature{
                .avr2,
                .lpmx,
                .smallstack,
            }),
        };
        pub const attiny261 = CpuModel{
            .name = "attiny261",
            .llvm_name = "attiny261",
            .features = featureSet(&[_]Feature{
                .avr25,
                .smallstack,
            }),
        };
        pub const attiny261a = CpuModel{
            .name = "attiny261a",
            .llvm_name = "attiny261a",
            .features = featureSet(&[_]Feature{
                .avr25,
                .smallstack,
            }),
        };
        pub const attiny28 = CpuModel{
            .name = "attiny28",
            .llvm_name = "attiny28",
            .features = featureSet(&[_]Feature{
                .avr1,
                .smallstack,
            }),
        };
        pub const attiny3216 = CpuModel{
            .name = "attiny3216",
            .llvm_name = "attiny3216",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny3217 = CpuModel{
            .name = "attiny3217",
            .llvm_name = "attiny3217",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny4 = CpuModel{
            .name = "attiny4",
            .llvm_name = "attiny4",
            .features = featureSet(&[_]Feature{
                .avrtiny,
            }),
        };
        pub const attiny40 = CpuModel{
            .name = "attiny40",
            .llvm_name = "attiny40",
            .features = featureSet(&[_]Feature{
                .avrtiny,
            }),
        };
        pub const attiny402 = CpuModel{
            .name = "attiny402",
            .llvm_name = "attiny402",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny404 = CpuModel{
            .name = "attiny404",
            .llvm_name = "attiny404",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny406 = CpuModel{
            .name = "attiny406",
            .llvm_name = "attiny406",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny412 = CpuModel{
            .name = "attiny412",
            .llvm_name = "attiny412",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny414 = CpuModel{
            .name = "attiny414",
            .llvm_name = "attiny414",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny416 = CpuModel{
            .name = "attiny416",
            .llvm_name = "attiny416",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny417 = CpuModel{
            .name = "attiny417",
            .llvm_name = "attiny417",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny4313 = CpuModel{
            .name = "attiny4313",
            .llvm_name = "attiny4313",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const attiny43u = CpuModel{
            .name = "attiny43u",
            .llvm_name = "attiny43u",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const attiny44 = CpuModel{
            .name = "attiny44",
            .llvm_name = "attiny44",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const attiny441 = CpuModel{
            .name = "attiny441",
            .llvm_name = "attiny441",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const attiny44a = CpuModel{
            .name = "attiny44a",
            .llvm_name = "attiny44a",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const attiny45 = CpuModel{
            .name = "attiny45",
            .llvm_name = "attiny45",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const attiny461 = CpuModel{
            .name = "attiny461",
            .llvm_name = "attiny461",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const attiny461a = CpuModel{
            .name = "attiny461a",
            .llvm_name = "attiny461a",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const attiny48 = CpuModel{
            .name = "attiny48",
            .llvm_name = "attiny48",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const attiny5 = CpuModel{
            .name = "attiny5",
            .llvm_name = "attiny5",
            .features = featureSet(&[_]Feature{
                .avrtiny,
            }),
        };
        pub const attiny804 = CpuModel{
            .name = "attiny804",
            .llvm_name = "attiny804",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny806 = CpuModel{
            .name = "attiny806",
            .llvm_name = "attiny806",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny807 = CpuModel{
            .name = "attiny807",
            .llvm_name = "attiny807",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny814 = CpuModel{
            .name = "attiny814",
            .llvm_name = "attiny814",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny816 = CpuModel{
            .name = "attiny816",
            .llvm_name = "attiny816",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny817 = CpuModel{
            .name = "attiny817",
            .llvm_name = "attiny817",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const attiny828 = CpuModel{
            .name = "attiny828",
            .llvm_name = "attiny828",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const attiny84 = CpuModel{
            .name = "attiny84",
            .llvm_name = "attiny84",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const attiny841 = CpuModel{
            .name = "attiny841",
            .llvm_name = "attiny841",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const attiny84a = CpuModel{
            .name = "attiny84a",
            .llvm_name = "attiny84a",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const attiny85 = CpuModel{
            .name = "attiny85",
            .llvm_name = "attiny85",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const attiny861 = CpuModel{
            .name = "attiny861",
            .llvm_name = "attiny861",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const attiny861a = CpuModel{
            .name = "attiny861a",
            .llvm_name = "attiny861a",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const attiny87 = CpuModel{
            .name = "attiny87",
            .llvm_name = "attiny87",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const attiny88 = CpuModel{
            .name = "attiny88",
            .llvm_name = "attiny88",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const attiny9 = CpuModel{
            .name = "attiny9",
            .llvm_name = "attiny9",
            .features = featureSet(&[_]Feature{
                .avrtiny,
            }),
        };
        pub const atxmega128a1 = CpuModel{
            .name = "atxmega128a1",
            .llvm_name = "atxmega128a1",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega128a1u = CpuModel{
            .name = "atxmega128a1u",
            .llvm_name = "atxmega128a1u",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega128a3 = CpuModel{
            .name = "atxmega128a3",
            .llvm_name = "atxmega128a3",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega128a3u = CpuModel{
            .name = "atxmega128a3u",
            .llvm_name = "atxmega128a3u",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega128a4u = CpuModel{
            .name = "atxmega128a4u",
            .llvm_name = "atxmega128a4u",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega128b1 = CpuModel{
            .name = "atxmega128b1",
            .llvm_name = "atxmega128b1",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega128b3 = CpuModel{
            .name = "atxmega128b3",
            .llvm_name = "atxmega128b3",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega128c3 = CpuModel{
            .name = "atxmega128c3",
            .llvm_name = "atxmega128c3",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega128d3 = CpuModel{
            .name = "atxmega128d3",
            .llvm_name = "atxmega128d3",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega128d4 = CpuModel{
            .name = "atxmega128d4",
            .llvm_name = "atxmega128d4",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega16a4 = CpuModel{
            .name = "atxmega16a4",
            .llvm_name = "atxmega16a4",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega16a4u = CpuModel{
            .name = "atxmega16a4u",
            .llvm_name = "atxmega16a4u",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega16c4 = CpuModel{
            .name = "atxmega16c4",
            .llvm_name = "atxmega16c4",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega16d4 = CpuModel{
            .name = "atxmega16d4",
            .llvm_name = "atxmega16d4",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega16e5 = CpuModel{
            .name = "atxmega16e5",
            .llvm_name = "atxmega16e5",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega192a3 = CpuModel{
            .name = "atxmega192a3",
            .llvm_name = "atxmega192a3",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega192a3u = CpuModel{
            .name = "atxmega192a3u",
            .llvm_name = "atxmega192a3u",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega192c3 = CpuModel{
            .name = "atxmega192c3",
            .llvm_name = "atxmega192c3",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega192d3 = CpuModel{
            .name = "atxmega192d3",
            .llvm_name = "atxmega192d3",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega256a3 = CpuModel{
            .name = "atxmega256a3",
            .llvm_name = "atxmega256a3",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega256a3b = CpuModel{
            .name = "atxmega256a3b",
            .llvm_name = "atxmega256a3b",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega256a3bu = CpuModel{
            .name = "atxmega256a3bu",
            .llvm_name = "atxmega256a3bu",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega256a3u = CpuModel{
            .name = "atxmega256a3u",
            .llvm_name = "atxmega256a3u",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega256c3 = CpuModel{
            .name = "atxmega256c3",
            .llvm_name = "atxmega256c3",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega256d3 = CpuModel{
            .name = "atxmega256d3",
            .llvm_name = "atxmega256d3",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega32a4 = CpuModel{
            .name = "atxmega32a4",
            .llvm_name = "atxmega32a4",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega32a4u = CpuModel{
            .name = "atxmega32a4u",
            .llvm_name = "atxmega32a4u",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega32c3 = CpuModel{
            .name = "atxmega32c3",
            .llvm_name = "atxmega32c3",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega32c4 = CpuModel{
            .name = "atxmega32c4",
            .llvm_name = "atxmega32c4",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega32d3 = CpuModel{
            .name = "atxmega32d3",
            .llvm_name = "atxmega32d3",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega32d4 = CpuModel{
            .name = "atxmega32d4",
            .llvm_name = "atxmega32d4",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega32e5 = CpuModel{
            .name = "atxmega32e5",
            .llvm_name = "atxmega32e5",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega384c3 = CpuModel{
            .name = "atxmega384c3",
            .llvm_name = "atxmega384c3",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega384d3 = CpuModel{
            .name = "atxmega384d3",
            .llvm_name = "atxmega384d3",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega64a1 = CpuModel{
            .name = "atxmega64a1",
            .llvm_name = "atxmega64a1",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega64a1u = CpuModel{
            .name = "atxmega64a1u",
            .llvm_name = "atxmega64a1u",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega64a3 = CpuModel{
            .name = "atxmega64a3",
            .llvm_name = "atxmega64a3",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega64a3u = CpuModel{
            .name = "atxmega64a3u",
            .llvm_name = "atxmega64a3u",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega64a4u = CpuModel{
            .name = "atxmega64a4u",
            .llvm_name = "atxmega64a4u",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega64b1 = CpuModel{
            .name = "atxmega64b1",
            .llvm_name = "atxmega64b1",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega64b3 = CpuModel{
            .name = "atxmega64b3",
            .llvm_name = "atxmega64b3",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega64c3 = CpuModel{
            .name = "atxmega64c3",
            .llvm_name = "atxmega64c3",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const atxmega64d3 = CpuModel{
            .name = "atxmega64d3",
            .llvm_name = "atxmega64d3",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega64d4 = CpuModel{
            .name = "atxmega64d4",
            .llvm_name = "atxmega64d4",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const atxmega8e5 = CpuModel{
            .name = "atxmega8e5",
            .llvm_name = "atxmega8e5",
            .features = featureSet(&[_]Feature{
                .xmegau,
            }),
        };
        pub const avr1 = CpuModel{
            .name = "avr1",
            .llvm_name = "avr1",
            .features = featureSet(&[_]Feature{
                .avr1,
            }),
        };
        pub const avr2 = CpuModel{
            .name = "avr2",
            .llvm_name = "avr2",
            .features = featureSet(&[_]Feature{
                .avr2,
            }),
        };
        pub const avr25 = CpuModel{
            .name = "avr25",
            .llvm_name = "avr25",
            .features = featureSet(&[_]Feature{
                .avr25,
            }),
        };
        pub const avr3 = CpuModel{
            .name = "avr3",
            .llvm_name = "avr3",
            .features = featureSet(&[_]Feature{
                .avr3,
            }),
        };
        pub const avr31 = CpuModel{
            .name = "avr31",
            .llvm_name = "avr31",
            .features = featureSet(&[_]Feature{
                .avr31,
            }),
        };
        pub const avr35 = CpuModel{
            .name = "avr35",
            .llvm_name = "avr35",
            .features = featureSet(&[_]Feature{
                .avr35,
            }),
        };
        pub const avr4 = CpuModel{
            .name = "avr4",
            .llvm_name = "avr4",
            .features = featureSet(&[_]Feature{
                .avr4,
            }),
        };
        pub const avr5 = CpuModel{
            .name = "avr5",
            .llvm_name = "avr5",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
        pub const avr51 = CpuModel{
            .name = "avr51",
            .llvm_name = "avr51",
            .features = featureSet(&[_]Feature{
                .avr51,
            }),
        };
        pub const avr6 = CpuModel{
            .name = "avr6",
            .llvm_name = "avr6",
            .features = featureSet(&[_]Feature{
                .avr6,
            }),
        };
        pub const avrtiny = CpuModel{
            .name = "avrtiny",
            .llvm_name = "avrtiny",
            .features = featureSet(&[_]Feature{
                .avrtiny,
            }),
        };
        pub const avrxmega1 = CpuModel{
            .name = "avrxmega1",
            .llvm_name = "avrxmega1",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const avrxmega2 = CpuModel{
            .name = "avrxmega2",
            .llvm_name = "avrxmega2",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const avrxmega3 = CpuModel{
            .name = "avrxmega3",
            .llvm_name = "avrxmega3",
            .features = featureSet(&[_]Feature{
                .xmega3,
            }),
        };
        pub const avrxmega4 = CpuModel{
            .name = "avrxmega4",
            .llvm_name = "avrxmega4",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const avrxmega5 = CpuModel{
            .name = "avrxmega5",
            .llvm_name = "avrxmega5",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const avrxmega6 = CpuModel{
            .name = "avrxmega6",
            .llvm_name = "avrxmega6",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const avrxmega7 = CpuModel{
            .name = "avrxmega7",
            .llvm_name = "avrxmega7",
            .features = featureSet(&[_]Feature{
                .xmega,
            }),
        };
        pub const m3000 = CpuModel{
            .name = "m3000",
            .llvm_name = "m3000",
            .features = featureSet(&[_]Feature{
                .avr5,
            }),
        };
    };